#!/usr/bin/python
#vim: set fileencoding=utf8
# parse-kickstart - read a kickstart file and emit equivalent dracut boot args.
#
# Copyright © 2012 Red Hat, Inc.
# BLAH BLAH GPL BLAH.
#
# Designed to run inside the dracut initramfs environment.
# Requires python 2.7 or later.
#
# Authors:
#   Will Woods <wwoods@redhat.com>

import sys, os
import logging
import shutil
import uuid
from pykickstart.parser import KickstartParser, preprocessKickstart
from pykickstart.version import returnClassForVersion
from pykickstart.errors import KickstartError
from pykickstart.constants import *
from pykickstart import commands
from collections import OrderedDict

# Default logging: none
log = logging.getLogger('parse-kickstart').addHandler(logging.NullHandler())

# Helper function for reading simple files in /sys
def readsysfile(f):
    '''Return the contents of f, or "" if missing.'''
    try:
        val = open(f).readline().strip()
    except IOError:
        val = ""
    return val

def read_cmdline(f):
    '''Returns an OrderedDict containing key-value pairs from a file with
    boot arguments (e.g. /proc/cmdline).'''
    args = OrderedDict()
    try:
        lines = open(f).readlines()
    except IOError:
        lines = []
    for line in lines:
        for arg in line.split():
            k,e,v = arg.partition("=")
            args[k] = v
    return args

proc_cmdline = read_cmdline("/proc/cmdline")

# Here are the kickstart commands we care about:

class Cdrom(commands.cdrom.FC3_Cdrom):
    def dracut_args(self, args, lineno, obj):
        return "inst.repo=cdrom"

class HardDrive(commands.harddrive.FC3_HardDrive):
    def dracut_args(self, args, lineno, obj):
        if self.biospart:
            return "inst.repo=bd:%s:%s" % (self.partition, self.dir)
        else:
            return "inst.repo=hd:%s:%s" % (self.partition, self.dir)

class NFS(commands.nfs.FC6_NFS):
    def dracut_args(self, args, lineno, obj):
        method="nfs:%s:%s" % (self.server, self.dir)
        if self.opts:
            method += ":%s" % self.opts

        return "inst.repo=%s" % method

class URL(commands.url.F18_Url):
    def dracut_args(self, args, lineno, obj):
        # FIXME: self.proxy, self.noverifyssl
        return "inst.repo=%s" % self.url

class Updates(commands.updates.F7_Updates):
    def dracut_args(self, args, lineno, obj):
        if self.url == "floppy":
            return "live.updates=/dev/fd0"
        elif self.url:
            return "live.updates=%s" % self.url

class MediaCheck(commands.mediacheck.FC4_MediaCheck):
    def dracut_args(self, args, lineno, obj):
        if self.mediacheck:
            return "rd.live.check"

class DriverDisk(commands.driverdisk.F14_DriverDisk):
    def dracut_args(self, args, lineno, obj):
        dd = self.driverdiskList[-1]
        if dd.biospart:
            location = "bd:%s" % dd.biospart
        else:
            location = dd.partition or dd.source
        if location:
            return "inst.driverdisk=%s" % location

class Network(commands.network.F20_Network):
    def dracut_args(self, args, lineno, net):
        '''
        NOTE: The first 'network' line get special treatment:
            * '--activate' is always enabled
            * '--device' is optional (defaults to the 'ksdevice=' boot arg)
            * the device gets brought online in initramfs
        '''
        netline = None

        # first 'network' line
        if len(self.network) == 1:
            net.activate = True
            if net.device == "link" or not net.device:
                # NOTE: this might still be empty (e.g. 'ks=file:...')
                # XXX FIXME: handle "link" properly?
                net.device = self.handler.ksdevice
            # tell dracut to bring this device up
            netline = ksnet_to_dracut(args, lineno, net, bootdev=True)

            # HACK: current dracut dies if you have BOOTIF= and ip= together.
            # Until that gets fixed upstream, we have to defer to dracut.
            # XXX FIXME: remove this when dracut can handle BOOTIF+ip!
            if 'BOOTIF' in proc_cmdline:
                # let dracut use BOOTIF to bring up the network
                netline = None

        else:
            # all subsequent 'network' lines require '--device'
            if not net.device or net.device == "link":
                log.error("'%s': missing --device", " ".join(args))
                return

        # write ifcfg so NM will set up the device correctly later
        ksnet_to_ifcfg(net)

        return netline

class DisplayMode(commands.displaymode.FC3_DisplayMode):
    def dracut_args(self, args, lineno, obj):
        if self.displayMode == DISPLAY_MODE_CMDLINE:
            return "inst.cmdline"
        elif self.displayMode == DISPLAY_MODE_TEXT:
            return "inst.text"
        elif self.displayMode == DISPLAY_MODE_GRAPHICAL:
            return "inst.graphical"

class Bootloader(commands.bootloader.F19_Bootloader):
    def dracut_args(self, args, lineno, obj):
        if self.extlinux:
            return "extlinux"

# TODO: keymap, lang... device? selinux?

dracutCmds = {
    'cdrom': Cdrom,
    'harddrive': HardDrive,
    'nfs': NFS,
    'url': URL,
    'updates': Updates,
    'mediacheck': MediaCheck,
    'driverdisk': DriverDisk,
    'network': Network,
    'cmdline': DisplayMode,
    'graphical': DisplayMode,
    'text': DisplayMode,
    'bootloader': Bootloader,
}
handlerclass = returnClassForVersion()
class DracutHandler(handlerclass):
    def __init__(self):
        handlerclass.__init__(self, commandUpdates=dracutCmds)
        self.output = []
        self.ksdevice = None
    def dispatcher(self, args, lineno):
        obj = handlerclass.dispatcher(self, args, lineno)
        # and execute any specified dracut_args
        cmd = args[0]
        command = self.commands[cmd]
        if hasattr(command, "dracut_args"):
            log.debug("kickstart line %u: handling %s", lineno, cmd)
            self.output.append(command.dracut_args(args, lineno, obj))
        return obj

def init_logger(level=None):
    if level is None and 'rd.debug' in proc_cmdline:
        level = logging.DEBUG
    logfmt = "%(name)s %(levelname)s: %(message)s"
    logging.basicConfig(format=logfmt, level=level)
    logger = logging.getLogger('parse-kickstart')
    return logger

def is_mac(addr):
    return addr and len(addr) == 17 and addr.count(":") == 5 # good enough

def find_devname(mac):
    for netif in os.listdir("/sys/class/net"):
        thismac = readsysfile("/sys/class/net/%s/address" % netif)
        if thismac.lower() == mac.lower():
            return netif

def ksnet_to_dracut(args, lineno, net, bootdev=False):
    '''Translate the kickstart network data into dracut network data.'''
    line = []
    ip=""
    autoconf=""

    if is_mac(net.device): # this is a MAC - find the interface name
        mac = net.device
        net.device = find_devname(mac)
        if net.device is None:  # iface not active - pick a name for it
            net.device = "ksdev0" # we only get called once, so this is OK
            line.append("ifname=%s:%s" % (net.device, mac.lower()))

    # NOTE: dracut currently only does ipv4 *or* ipv6, so only one ip=arg..
    if net.bootProto in (BOOTPROTO_DHCP, BOOTPROTO_BOOTP):
        autoconf="dhcp"
    elif net.bootProto == BOOTPROTO_IBFT:
        autoconf="ibft"
    elif net.bootProto == BOOTPROTO_QUERY:
        log.error("'%s': --bootproto=query is deprecated", " ".join(args))
    elif net.bootProto == BOOTPROTO_STATIC:
        req = ("gateway", "netmask", "nameserver", "ip")
        missing = ", ".join("--%s" % i for i in req if not hasattr(net, i))
        if missing:
            log.warn("line %u: network missing %s", lineno, missing)
        else:
            ip="{0.ip}::{0.gateway}:{0.netmask}:" \
               "{0.hostname}:{0.device}:none:{0.mtu}".format(net)
    elif net.ipv6 == "auto":
        autoconf="auto6"
    elif net.ipv6 == "dhcp":
        autoconf="dhcp6"
    elif net.ipv6:
        ip="[{0.ipv6}]::{0.ipv6gateway}:{0.netmask}:" \
           "{0.hostname}:{0.device}:none:{0.mtu}".format(net)

    if autoconf:
        if net.device or net.mtu:
            ip="%s:%s:%s" % (net.device, autoconf, net.mtu)
        else:
            ip=autoconf

    if ip:
        line.append("ip=%s" % ip)

    for ns in net.nameserver.split(","):
        if ns:
            line.append("nameserver=%s" % ns)

    if net.mtu:
        # XXX FIXME: dracut doesn't support mtu= (yet)
        if net.device:
            line.append("mtu=%s:%s" % (net.device, net.mtu))
        else:
            line.append("mtu=%s" % net.mtu)

    if bootdev:
        if net.device:
            line.append("bootdev=%s" % net.device)
        # touch /tmp/net.ifaces to make sure dracut brings up network
        open("/tmp/net.ifaces", "a")

    if net.essid or net.wepkey or net.wpakey:
        # TODO: make dracut support wireless? (do we care?)
        log.error("'%s': dracut doesn't support wireless networks",
                      " ".join(args))

    return " ".join(line)

def ksnet_to_ifcfg(net, filename=None):
    '''Write an ifcfg file for the given kickstart network config'''
    dev = net.device
    if is_mac(dev):
        dev = find_devname(dev)
    if not dev:
        return
    if (not os.path.isdir("/sys/class/net/%s" % dev)
        and not net.bondslaves and not net.teamslaves):
        log.info("can't find device %s" % dev)
        return
    ifcfg = dict()
    if filename is None:
        filename = "/tmp/ifcfg/ifcfg-%s" % dev
        if not os.path.isdir("/tmp/ifcfg"):
            os.makedirs("/tmp/ifcfg")
    ifcfg['DEVICE'] = dev
    ifcfg['HWADDR'] = readsysfile("/sys/class/net/%s/address" % dev)
    ifcfg['UUID'] = str(uuid.uuid4())
    # we set real ONBOOT value in anaconda, here
    # we use it to activate devcies by NM on start
    ifcfg['ONBOOT'] = "yes" if net.activate else "no"

    # dhcp etc.
    ifcfg['BOOTPROTO'] = net.bootProto
    if net.bootProto == 'static':
        ifcfg['IPADDR'] = net.ip
        ifcfg['NETMASK'] = net.netmask
        ifcfg['GATEWAY'] = net.gateway
    if net.bootProto == 'dhcp':
        if net.hostname:
            ifcfg['DHCP_HOSTNAME'] = net.hostname

    # ipv6 settings
    if net.noipv6:
        ifcfg['IPV6INIT'] = "no"
    else:
        ifcfg['IPV6INIT'] = "yes"

        if net.ipv6 == 'dhcp':
            ifcfg['DHCPV6C'] = "yes"
            ifcfg['IPV6_AUTOCONF'] = "no"
            if net.ipv6gateway:
                ifcfg['IPV6_DEFAULTGW'] = net.ipv6gateway
        elif net.ipv6 == 'auto':
            ifcfg['IPV6_AUTOCONF'] = "yes" # NOTE: redundant (this is the default)
        elif ':' in net.ipv6:
            ifcfg['IPV6ADDR'] = net.ipv6
            ifcfg['IPV6_AUTOCONF'] = "no"

    # misc stuff
    if net.mtu:
        ifcfg['MTU'] = net.mtu
    if net.nameserver:
        for i, ip in enumerate(net.nameserver.split(",")):
            ifcfg["DNS%d" % (i+1)] = ip
    if net.nodefroute:
        ifcfg['DEFROUTE'] = "no"

    # TODO: dhcpclass, ethtool, essid/wepkey/wpakay, etc.

    if net.bootProto == 'dhcp':
        srcpath = "/tmp/dhclient.%s.lease" % dev
        dstdir = "/tmp/ifcfg-leases"
        dstpath = "%s/dhclient-%s-%s.lease" % (dstdir, ifcfg['UUID'], dev)
        if os.path.exists(srcpath):
            if not os.path.isdir(dstdir):
                os.makedirs(dstdir)
            shutil.copyfile(srcpath, dstpath)

    if net.bondslaves:
        ifcfg.pop('HWADDR')
        ifcfg['TYPE'] = "Bond"
        ifcfg['BONDING_MASTER'] = "yes"
        ifcfg['NAME'] = "Bond connection %s" % dev
        if ';' in net.bondopts:
            sep = ";"
        else:
            sep = ","
        ifcfg['BONDING_OPTS'] = '"' + " ".join(net.bondopts.split(sep)) + '"'

        for i, slave in enumerate(net.bondslaves.split(","), 1):
            slave_ifcfg = {
                            'TYPE' : "Ethernet",
                            'NAME' : "%s slave %s" % (dev, i),
                            'UUID' : str(uuid.uuid4()),
                            'ONBOOT' : "yes",
                            'MASTER' : dev,
                            'HWADDR' : readsysfile("/sys/class/net/%s/address" % slave),
                          }
            # not using NM naming conventions, following dracut so that it does not
            # override kickstart config by generating its own ifcfg files for slaves
            #slave_filename = "/tmp/ifcfg/ifcfg-%s" % "_".join(slave_ifcfg['NAME'].split(" "))
            # FIXME - change in dracut?
            slave_filename = "/tmp/ifcfg/ifcfg-%s" % slave
            log.info("writing ifcfg %s for slave %s of bond %s" % (slave_filename, slave, dev))
            write_ifcfg(slave_filename, slave_ifcfg)

    if net.teamslaves:

        ifcfg.pop('HWADDR')
        ifcfg['TYPE'] = "Team"
        ifcfg['NAME'] = "Team connection %s" % dev
        ifcfg['TEAM_CONFIG'] = "'" + net.teamconfig + "'"

        for i, (slave, cfg) in enumerate(net.teamslaves):
            slave_ifcfg = {
                            'DEVICE': slave,
                            'DEVICETYPE' : "TeamPort",
                            'NAME' : "%s slave %s" % (dev, i),
                            'UUID' : str(uuid.uuid4()),
                            'ONBOOT' : "yes",
                            'TEAM_MASTER' : dev,
#                            'HWADDR' : readsysfile("/sys/class/net/%s/address" % slave),
                          }
            if cfg:
                slave_ifcfg['TEAM_PORT_CONFIG'] = "'" + cfg + "'"

            # not using NM naming conventions, following dracut so that it does not
            # override kickstart config by generating its own ifcfg files for slaves
            #slave_filename = "/tmp/ifcfg/ifcfg-%s" % "_".join(slave_ifcfg['NAME'].split(" "))
            # FIXME - change in dracut?
            slave_filename = "/tmp/ifcfg/ifcfg-%s" % slave
            log.info("writing ifcfg %s for slave %s of team %s" % (slave_filename, slave, dev))
            write_ifcfg(slave_filename, slave_ifcfg)

    if net.vlanid:
        interface_name = "%s.%s" % (dev, net.vlanid)
        ifcfg.pop('HWADDR')
        ifcfg['TYPE'] = "Vlan"
        ifcfg['VLAN'] = "yes"
        ifcfg['VLAN_ID'] = net.vlanid
        ifcfg['NAME'] = "VLAN connection %s" % interface_name
        ifcfg['DEVICE'] = interface_name
        ifcfg['PHYSDEV'] = dev
        filename = "/tmp/ifcfg/ifcfg-%s" % interface_name

    log.info("writing ifcfg %s for %s" % (filename, dev))
    if write_ifcfg(filename, ifcfg):
        return filename

def write_ifcfg(filename, ifcfg):
    try:
        with open(filename, "w") as f:
            f.write('# Generated by parse-kickstart\n')
            for k,v in ifcfg.items():
                f.write("%s=%s\n" % (k,v))
    except IOError as e:
        log.error("can't write %s: %s" % (filename, e))
        return False
    return True

def process_kickstart(ksfile):
    handler = DracutHandler()
    handler.ksdevice = os.environ.get('ksdevice')
    parser = KickstartParser(handler, missingIncludeIsFatal=False, errorsAreFatal=False)
    log.info("processing kickstart file %s", ksfile)
    processed_file = preprocessKickstart(ksfile)
    try:
        parser.readKickstart(processed_file)
    except KickstartError as e:
        log.error(str(e))
    with open("/tmp/ks.info", "a") as f:
        f.write('parsed_kickstart="%s"\n' % processed_file)
    log.info("finished parsing kickstart")
    return processed_file, handler.output

if __name__ == '__main__':
    log = init_logger()
    for path in sys.argv[1:]:
        outfile, output = process_kickstart(path)
        for line in filter(None, output):
            print line
