From fd0e435b0fe85622f167b84432552885a4856ac8 Mon Sep 17 00:00:00 2001
From: Phil Oester <kernel@linuxace.com>
Date: Mon, 14 Mar 2011 06:22:04 +0000
Subject: [PATCH] bonding: Incorrect TX queue offset
Git-commit: fd0e435b0fe85622f167b84432552885a4856ac8
Patch-mainline: v2.6.39-rc1~468^2~15
Reference: bnc#687116, CVE-2011-1581

When packets come in from a device with >= 16 receive queues
headed out a bonding interface, syslog gets filled with this:

    kernel: bond0 selects TX queue 16, but real number of TX queues is 16

because queue_mapping is offset by 1.  Adjust return value
to account for the offset.

This is a revision of my earlier patch (which did not use the
skb_rx_queue_* helpers - thanks to Ben for the suggestion).
Andy submitted a similar patch which emits a pr_warning on
invalid queue selection, but I believe the log spew is
not useful.  We can revisit that question in the future,
but in the interim I believe fixing the core problem is
worthwhile.

Signed-off-by: Phil Oester <kernel@linuxace.com>
Signed-off-by: Andy Gospodarek <andy@greyhouse.net>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Brandon Philips <bphilips@suse.de>

---
 drivers/net/bonding/bond_main.c |   11 +++++++++--
 1 files changed, 9 insertions(+), 2 deletions(-)

diff --git a/drivers/net/bonding/bond_main.c b/drivers/net/bonding/bond_main.c
index 3ad4f50..a93d941 100644
--- a/drivers/net/bonding/bond_main.c
+++ b/drivers/net/bonding/bond_main.c
@@ -4341,11 +4341,18 @@ static u16 bond_select_queue(struct net_device *dev, struct sk_buff *skb)
 {
 	/*
 	 * This helper function exists to help dev_pick_tx get the correct
-	 * destination queue.  Using a helper function skips the a call to
+	 * destination queue.  Using a helper function skips a call to
 	 * skb_tx_hash and will put the skbs in the queue we expect on their
 	 * way down to the bonding driver.
 	 */
-	return skb->queue_mapping;
+	u16 txq = skb_rx_queue_recorded(skb) ? skb_get_rx_queue(skb) : 0;
+
+	if (unlikely(txq >= dev->real_num_tx_queues)) {
+		do
+			txq -= dev->real_num_tx_queues;
+		while (txq >= dev->real_num_tx_queues);
+	}
+	return txq;
 }
 
 static netdev_tx_t bond_start_xmit(struct sk_buff *skb, struct net_device *dev)
-- 
1.7.3.4

