From: www.kernel.org
Subject: Update to 2.6.23
Patch-mainline: 2.6.23

Automatically created from "patches.kernel.org/patch-2.6.23" by xen-port-patches.py

Acked-by: jbeulich@novell.com

--- head-2011-03-17.orig/arch/x86/Kbuild	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/arch/x86/Kbuild	2011-01-31 17:49:31.000000000 +0100
@@ -2,7 +2,7 @@
 obj-$(CONFIG_KVM) += kvm/
 
 # Xen paravirtualization support
-obj-$(CONFIG_XEN) += xen/
+obj-$(CONFIG_PARAVIRT_XEN) += xen/
 
 # lguest paravirtualization support
 obj-$(CONFIG_LGUEST_GUEST) += lguest/
--- head-2011-03-17.orig/arch/x86/kernel/acpi/sleep_32-xen.c	2008-04-15 09:29:41.000000000 +0200
+++ head-2011-03-17/arch/x86/kernel/acpi/sleep_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -15,7 +15,7 @@
 #ifndef CONFIG_ACPI_PV_SLEEP
 /* address in low memory of the wakeup routine. */
 unsigned long acpi_wakeup_address = 0;
-unsigned long acpi_video_flags;
+unsigned long acpi_realmode_flags;
 extern char wakeup_start, wakeup_end;
 
 extern unsigned long FASTCALL(acpi_copy_wakeup_routine(unsigned long));
@@ -74,9 +74,11 @@ static int __init acpi_sleep_setup(char 
 {
 	while ((str != NULL) && (*str != '\0')) {
 		if (strncmp(str, "s3_bios", 7) == 0)
-			acpi_video_flags = 1;
+			acpi_realmode_flags |= 1;
 		if (strncmp(str, "s3_mode", 7) == 0)
-			acpi_video_flags |= 2;
+			acpi_realmode_flags |= 2;
+		if (strncmp(str, "s3_beep", 7) == 0)
+			acpi_realmode_flags |= 4;
 		str = strchr(str, ',');
 		if (str != NULL)
 			str += strspn(str, ", \t");
@@ -86,9 +88,11 @@ static int __init acpi_sleep_setup(char 
 
 __setup("acpi_sleep=", acpi_sleep_setup);
 
+/* Ouch, we want to delete this. We already have better version in userspace, in
+   s2ram from suspend.sf.net project */
 static __init int reset_videomode_after_s3(struct dmi_system_id *d)
 {
-	acpi_video_flags |= 2;
+	acpi_realmode_flags |= 2;
 	return 0;
 }
 
--- head-2011-03-17.orig/arch/x86/kernel/asm-offsets_32.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/asm-offsets_32.c	2011-01-31 17:49:31.000000000 +0100
@@ -20,7 +20,9 @@
 #include <asm/elf.h>
 #include <asm/suspend.h>
 
+#if defined(CONFIG_XEN) || defined(CONFIG_PARAVIRT_XEN)
 #include <xen/interface/xen.h>
+#endif
 
 #include <linux/lguest.h>
 #include "../../../drivers/lguest/lg.h"
@@ -55,7 +57,6 @@ void foo(void)
 	OFFSET(TI_exec_domain, thread_info, exec_domain);
 	OFFSET(TI_flags, thread_info, flags);
 	OFFSET(TI_status, thread_info, status);
-	OFFSET(TI_cpu, thread_info, cpu);
 	OFFSET(TI_preempt_count, thread_info, preempt_count);
 	OFFSET(TI_addr_limit, thread_info, addr_limit);
 	OFFSET(TI_restart_block, thread_info, restart_block);
@@ -121,7 +122,7 @@ void foo(void)
 	OFFSET(PV_CPU_read_cr0, pv_cpu_ops, read_cr0);
 #endif
 
-#ifdef CONFIG_XEN
+#ifdef CONFIG_PARAVIRT_XEN
 	BLANK();
 	OFFSET(XEN_vcpu_info_mask, vcpu_info, evtchn_upcall_mask);
 	OFFSET(XEN_vcpu_info_pending, vcpu_info, evtchn_upcall_pending);
--- head-2011-03-17.orig/arch/x86/kernel/cpu/common-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/cpu/common-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -362,6 +362,8 @@ static void __cpuinit generic_identify(s
 			if ( xlvl >= 0x80000004 )
 				get_model_name(c); /* Default name */
 		}
+
+		init_scattered_cpuid_features(c);
 	}
 
 	early_intel_workaround(c);
@@ -613,7 +615,6 @@ extern int nsc_init_cpu(void);
 extern int amd_init_cpu(void);
 extern int centaur_init_cpu(void);
 extern int transmeta_init_cpu(void);
-extern int rise_init_cpu(void);
 extern int nexgen_init_cpu(void);
 extern int umc_init_cpu(void);
 
@@ -625,7 +626,6 @@ void __init early_cpu_init(void)
 	amd_init_cpu();
 	centaur_init_cpu();
 	transmeta_init_cpu();
-	rise_init_cpu();
 	nexgen_init_cpu();
 	umc_init_cpu();
 	early_cpu_detect();
--- head-2011-03-17.orig/arch/x86/kernel/cpu/mtrr/main-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/cpu/mtrr/main-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -167,7 +167,7 @@ mtrr_del(int reg, unsigned long base, un
 EXPORT_SYMBOL(mtrr_add);
 EXPORT_SYMBOL(mtrr_del);
 
-__init void mtrr_bp_init(void)
+void __init mtrr_bp_init(void)
 {
 }
 
--- head-2011-03-17.orig/arch/x86/kernel/e820_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/e820_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -10,6 +10,7 @@
 #include <linux/efi.h>
 #include <linux/pfn.h>
 #include <linux/uaccess.h>
+#include <linux/suspend.h>
 
 #include <asm/pgtable.h>
 #include <asm/page.h>
@@ -343,6 +344,37 @@ static int __init request_standard_resou
 
 subsys_initcall(request_standard_resources);
 
+#if defined(CONFIG_PM) && defined(CONFIG_HIBERNATION)
+/**
+ * e820_mark_nosave_regions - Find the ranges of physical addresses that do not
+ * correspond to e820 RAM areas and mark the corresponding pages as nosave for
+ * hibernation.
+ *
+ * This function requires the e820 map to be sorted and without any
+ * overlapping entries and assumes the first e820 area to be RAM.
+ */
+void __init e820_mark_nosave_regions(void)
+{
+	int i;
+	unsigned long pfn;
+
+	pfn = PFN_DOWN(e820.map[0].addr + e820.map[0].size);
+	for (i = 1; i < e820.nr_map; i++) {
+		struct e820entry *ei = &e820.map[i];
+
+		if (pfn < PFN_UP(ei->addr))
+			register_nosave_region(pfn, PFN_UP(ei->addr));
+
+		pfn = PFN_DOWN(ei->addr + ei->size);
+		if (ei->type != E820_RAM)
+			register_nosave_region(PFN_UP(ei->addr), pfn);
+
+		if (pfn >= max_low_pfn)
+			break;
+	}
+}
+#endif
+
 void __init add_memory_region(unsigned long long start,
 			      unsigned long long size, int type)
 {
@@ -791,7 +823,7 @@ void __init print_memory_map(char *who)
 		case E820_NVS:
 				printk("(ACPI NVS)\n");
 				break;
-		default:	printk("type %lu\n", e820.map[i].type);
+		default:	printk("type %u\n", e820.map[i].type);
 				break;
 		}
 	}
--- head-2011-03-17.orig/arch/x86/kernel/entry_32.S	2011-02-01 14:10:27.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/entry_32.S	2011-02-01 14:10:55.000000000 +0100
@@ -1047,7 +1047,7 @@ ENTRY(kernel_thread_helper)
 	CFI_ENDPROC
 ENDPROC(kernel_thread_helper)
 
-#ifdef CONFIG_XEN
+#ifdef CONFIG_PARAVIRT_XEN
 /* Xen doesn't set %esp to be precisely what the normal sysenter
    entrypoint expects, so fix it up before using the normal path. */
 ENTRY(xen_sysenter_target)
@@ -1139,7 +1139,7 @@ ENDPROC(xen_failsafe_callback)
 BUILD_INTERRUPT3(xen_hvm_callback_vector, XEN_HVM_EVTCHN_CALLBACK,
 		xen_evtchn_do_upcall)
 
-#endif	/* CONFIG_XEN */
+#endif	/* CONFIG_PARAVIRT_XEN */
 
 #ifdef CONFIG_FUNCTION_TRACER
 #ifdef CONFIG_DYNAMIC_FTRACE
--- head-2011-03-17.orig/arch/x86/kernel/entry_32-xen.S	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/entry_32-xen.S	2011-01-31 17:49:31.000000000 +0100
@@ -452,9 +452,6 @@ restore_nocheck_notrace:
 1:	INTERRUPT_RETURN
 .section .fixup,"ax"
 iret_exc:
-#ifndef CONFIG_XEN
-	ENABLE_INTERRUPTS(CLBR_NONE)
-#endif
 	pushl $0			# no error code
 	pushl $do_iret_error
 	jmp error_code
--- head-2011-03-17.orig/arch/x86/kernel/head_32-xen.S	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/head_32-xen.S	2011-01-31 17:49:31.000000000 +0100
@@ -86,7 +86,10 @@ ENTRY(_stext)
 /*
  * BSS section
  */
-.section ".bss.page_aligned","w"
+.section ".bss.page_aligned","wa"
+	.align PAGE_SIZE_asm
+ENTRY(swapper_pg_pmd)
+	.fill 1024,4,0
 ENTRY(empty_zero_page)
 	.fill 4096,1,0
 
@@ -136,25 +139,25 @@ ENTRY(empty_zero_page)
 #endif /* CONFIG_XEN_COMPAT <= 0x030002 */
 
 
-	ELFNOTE(Xen, XEN_ELFNOTE_GUEST_OS,       .asciz, "linux")	
-	ELFNOTE(Xen, XEN_ELFNOTE_GUEST_VERSION,  .asciz, "2.6")
-	ELFNOTE(Xen, XEN_ELFNOTE_XEN_VERSION,    .asciz, "xen-3.0")
-	ELFNOTE(Xen, XEN_ELFNOTE_VIRT_BASE,      .long,  __PAGE_OFFSET)
+	ELFNOTE(Xen, XEN_ELFNOTE_GUEST_OS,       .asciz "linux")
+	ELFNOTE(Xen, XEN_ELFNOTE_GUEST_VERSION,  .asciz "2.6")
+	ELFNOTE(Xen, XEN_ELFNOTE_XEN_VERSION,    .asciz "xen-3.0")
+	ELFNOTE(Xen, XEN_ELFNOTE_VIRT_BASE,      .long __PAGE_OFFSET)
 #if CONFIG_XEN_COMPAT <= 0x030002
-	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   .long,  __PAGE_OFFSET)
+	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   .long __PAGE_OFFSET)
 #else
-	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   .long,  0)
+	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   .long 0)
 #endif
-	ELFNOTE(Xen, XEN_ELFNOTE_ENTRY,          .long,  startup_32)
-	ELFNOTE(Xen, XEN_ELFNOTE_HYPERCALL_PAGE, .long,  hypercall_page)
-	ELFNOTE(Xen, XEN_ELFNOTE_HV_START_LOW,   .long,  HYPERVISOR_VIRT_START)
-	ELFNOTE(Xen, XEN_ELFNOTE_FEATURES,       .asciz, "writable_page_tables|writable_descriptor_tables|auto_translated_physmap|pae_pgdir_above_4gb|supervisor_mode_kernel")
+	ELFNOTE(Xen, XEN_ELFNOTE_ENTRY,          .long startup_32)
+	ELFNOTE(Xen, XEN_ELFNOTE_HYPERCALL_PAGE, .long hypercall_page)
+	ELFNOTE(Xen, XEN_ELFNOTE_HV_START_LOW,   .long HYPERVISOR_VIRT_START)
+	ELFNOTE(Xen, XEN_ELFNOTE_FEATURES,       .asciz "writable_page_tables|writable_descriptor_tables|auto_translated_physmap|pae_pgdir_above_4gb|supervisor_mode_kernel")
 #ifdef CONFIG_X86_PAE
-	ELFNOTE(Xen, XEN_ELFNOTE_PAE_MODE,       .asciz, "yes")
-	ELFNOTE(Xen, XEN_ELFNOTE_L1_MFN_VALID,   .quad,  _PAGE_PRESENT,_PAGE_PRESENT)
+	ELFNOTE(Xen, XEN_ELFNOTE_PAE_MODE,       .asciz "yes")
+	ELFNOTE(Xen, XEN_ELFNOTE_L1_MFN_VALID,   .quad _PAGE_PRESENT, _PAGE_PRESENT)
 #else
-	ELFNOTE(Xen, XEN_ELFNOTE_PAE_MODE,       .asciz, "no")
-	ELFNOTE(Xen, XEN_ELFNOTE_L1_MFN_VALID,   .long,  _PAGE_PRESENT,_PAGE_PRESENT)
+	ELFNOTE(Xen, XEN_ELFNOTE_PAE_MODE,       .asciz "no")
+	ELFNOTE(Xen, XEN_ELFNOTE_L1_MFN_VALID,   .long _PAGE_PRESENT, _PAGE_PRESENT)
 #endif
-	ELFNOTE(Xen, XEN_ELFNOTE_LOADER,         .asciz, "generic")
-	ELFNOTE(Xen, XEN_ELFNOTE_SUSPEND_CANCEL, .long,  1)
+	ELFNOTE(Xen, XEN_ELFNOTE_LOADER,         .asciz "generic")
+	ELFNOTE(Xen, XEN_ELFNOTE_SUSPEND_CANCEL, .long 1)
--- head-2011-03-17.orig/arch/x86/kernel/io_apic_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/io_apic_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -402,14 +402,6 @@ static void set_ioapic_affinity_irq(unsi
 # include <linux/slab.h>		/* kmalloc() */
 # include <linux/timer.h>	/* time_after() */
  
-#ifdef CONFIG_BALANCED_IRQ_DEBUG
-#  define TDprintk(x...) do { printk("<%ld:%s:%d>: ", jiffies, __FILE__, __LINE__); printk(x); } while (0)
-#  define Dprintk(x...) do { TDprintk(x); } while (0)
-# else
-#  define TDprintk(x...) 
-#  define Dprintk(x...) 
-# endif
-
 #define IRQBALANCE_CHECK_ARCH -999
 #define MAX_BALANCED_IRQ_INTERVAL	(5*HZ)
 #define MIN_BALANCED_IRQ_INTERVAL	(HZ/2)
@@ -492,7 +484,7 @@ static inline void balance_irq(int cpu, 
 static inline void rotate_irqs_among_cpus(unsigned long useful_load_threshold)
 {
 	int i, j;
-	Dprintk("Rotating IRQs among CPUs.\n");
+
 	for_each_online_cpu(i) {
 		for (j = 0; j < NR_IRQS; j++) {
 			if (!irq_desc[j].action)
@@ -609,19 +601,11 @@ tryanothercpu:
 	max_loaded = tmp_loaded;	/* processor */
 	imbalance = (max_cpu_irq - min_cpu_irq) / 2;
 	
-	Dprintk("max_loaded cpu = %d\n", max_loaded);
-	Dprintk("min_loaded cpu = %d\n", min_loaded);
-	Dprintk("max_cpu_irq load = %ld\n", max_cpu_irq);
-	Dprintk("min_cpu_irq load = %ld\n", min_cpu_irq);
-	Dprintk("load imbalance = %lu\n", imbalance);
-
 	/* if imbalance is less than approx 10% of max load, then
 	 * observe diminishing returns action. - quit
 	 */
-	if (imbalance < (max_cpu_irq >> 3)) {
-		Dprintk("Imbalance too trivial\n");
+	if (imbalance < (max_cpu_irq >> 3))
 		goto not_worth_the_effort;
-	}
 
 tryanotherirq:
 	/* if we select an IRQ to move that can't go where we want, then
@@ -678,9 +662,6 @@ tryanotherirq:
 	cpus_and(tmp, target_cpu_mask, allowed_mask);
 
 	if (!cpus_empty(tmp)) {
-
-		Dprintk("irq = %d moved to cpu = %d\n",
-				selected_irq, min_loaded);
 		/* mark for change destination */
 		set_pending_irq(selected_irq, cpumask_of_cpu(min_loaded));
 
@@ -700,7 +681,6 @@ not_worth_the_effort:
 	 */
 	balanced_irq_interval = min((long)MAX_BALANCED_IRQ_INTERVAL,
 		balanced_irq_interval + BALANCED_IRQ_MORE_DELTA);	
-	Dprintk("IRQ worth rotating not found\n");
 	return;
 }
 
@@ -716,6 +696,7 @@ static int balanced_irq(void *unused)
 		set_pending_irq(i, cpumask_of_cpu(0));
 	}
 
+	set_freezable();
 	for ( ; ; ) {
 		time_remaining = schedule_timeout_interruptible(time_remaining);
 		try_to_freeze();
@@ -825,14 +806,6 @@ static int pirq_entries [MAX_PIRQS];
 static int pirqs_enabled;
 int skip_ioapic_setup;
 
-static int __init ioapic_setup(char *str)
-{
-	skip_ioapic_setup = 1;
-	return 1;
-}
-
-__setup("noapic", ioapic_setup);
-
 static int __init ioapic_pirq_setup(char *str)
 {
 	int i, max;
@@ -1323,12 +1296,15 @@ static struct irq_chip ioapic_chip;
 static void ioapic_register_intr(int irq, int vector, unsigned long trigger)
 {
 	if ((trigger == IOAPIC_AUTO && IO_APIC_irq_trigger(irq)) ||
-			trigger == IOAPIC_LEVEL)
+	    trigger == IOAPIC_LEVEL) {
+		irq_desc[irq].status |= IRQ_LEVEL;
 		set_irq_chip_and_handler_name(irq, &ioapic_chip,
 					 handle_fasteoi_irq, "fasteoi");
-	else
+	} else {
+		irq_desc[irq].status &= ~IRQ_LEVEL;
 		set_irq_chip_and_handler_name(irq, &ioapic_chip,
 					 handle_edge_irq, "edge");
+	}
 	set_intr_gate(vector, interrupt[irq]);
 }
 #else
@@ -1957,7 +1933,7 @@ __setup("no_timer_check", notimercheck);
  *	- if this function detects that timer IRQs are defunct, then we fall
  *	  back to ISA timer IRQs
  */
-int __init timer_irq_works(void)
+static int __init timer_irq_works(void)
 {
 	unsigned long t1 = jiffies;
 
--- head-2011-03-17.orig/arch/x86/kernel/microcode-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/microcode-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -33,6 +33,7 @@
 #include <linux/miscdevice.h>
 #include <linux/spinlock.h>
 #include <linux/mm.h>
+#include <linux/fs.h>
 #include <linux/mutex.h>
 #include <linux/cpu.h>
 #include <linux/firmware.h>
--- head-2011-03-17.orig/arch/x86/kernel/pci-dma-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/pci-dma-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -24,7 +24,7 @@
 #include <asm/bug.h>
 
 #ifdef __x86_64__
-#include <asm/proto.h>
+#include <asm/iommu.h>
 
 int iommu_merge __read_mostly = 0;
 EXPORT_SYMBOL(iommu_merge);
--- head-2011-03-17.orig/arch/x86/kernel/process_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/process_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -241,6 +241,7 @@ early_param("idle", idle_setup);
 void show_regs(struct pt_regs * regs)
 {
 	unsigned long cr0 = 0L, cr2 = 0L, cr3 = 0L, cr4 = 0L;
+	unsigned long d0, d1, d2, d3, d6, d7;
 
 	printk("\n");
 	printk("Pid: %d, comm: %20s\n", current->pid, current->comm);
@@ -265,6 +266,17 @@ void show_regs(struct pt_regs * regs)
 	cr3 = read_cr3();
 	cr4 = read_cr4_safe();
 	printk("CR0: %08lx CR2: %08lx CR3: %08lx CR4: %08lx\n", cr0, cr2, cr3, cr4);
+
+	get_debugreg(d0, 0);
+	get_debugreg(d1, 1);
+	get_debugreg(d2, 2);
+	get_debugreg(d3, 3);
+	printk("DR0: %08lx DR1: %08lx DR2: %08lx DR3: %08lx\n",
+			d0, d1, d2, d3);
+	get_debugreg(d6, 6);
+	get_debugreg(d7, 7);
+	printk("DR6: %08lx DR7: %08lx\n", d6, d7);
+
 	show_trace(NULL, regs, &regs->esp);
 }
 
@@ -473,7 +485,30 @@ int dump_task_regs(struct task_struct *t
 	return 1;
 }
 
-static noinline void __switch_to_xtra(struct task_struct *next_p)
+#ifdef CONFIG_SECCOMP
+void hard_disable_TSC(void)
+{
+	write_cr4(read_cr4() | X86_CR4_TSD);
+}
+void disable_TSC(void)
+{
+	preempt_disable();
+	if (!test_and_set_thread_flag(TIF_NOTSC))
+		/*
+		 * Must flip the CPU state synchronously with
+		 * TIF_NOTSC in the current running context.
+		 */
+		hard_disable_TSC();
+	preempt_enable();
+}
+void hard_enable_TSC(void)
+{
+	write_cr4(read_cr4() & ~X86_CR4_TSD);
+}
+#endif /* CONFIG_SECCOMP */
+
+static noinline void
+__switch_to_xtra(struct task_struct *prev_p, struct task_struct *next_p)
 {
 	struct thread_struct *next;
 
@@ -488,33 +523,17 @@ static noinline void __switch_to_xtra(st
 		set_debugreg(next->debugreg[6], 6);
 		set_debugreg(next->debugreg[7], 7);
 	}
-}
 
-/*
- * This function selects if the context switch from prev to next
- * has to tweak the TSC disable bit in the cr4.
- */
-static inline void disable_tsc(struct task_struct *prev_p,
-			       struct task_struct *next_p)
-{
-	struct thread_info *prev, *next;
-
-	/*
-	 * gcc should eliminate the ->thread_info dereference if
-	 * has_secure_computing returns 0 at compile time (SECCOMP=n).
-	 */
-	prev = task_thread_info(prev_p);
-	next = task_thread_info(next_p);
-
-	if (has_secure_computing(prev) || has_secure_computing(next)) {
-		/* slow path here */
-		if (has_secure_computing(prev) &&
-		    !has_secure_computing(next)) {
-			write_cr4(read_cr4() & ~X86_CR4_TSD);
-		} else if (!has_secure_computing(prev) &&
-			   has_secure_computing(next))
-			write_cr4(read_cr4() | X86_CR4_TSD);
+#ifdef CONFIG_SECCOMP
+	if (test_tsk_thread_flag(prev_p, TIF_NOTSC) ^
+	    test_tsk_thread_flag(next_p, TIF_NOTSC)) {
+		/* prev and next are different */
+		if (test_tsk_thread_flag(next_p, TIF_NOTSC))
+			hard_disable_TSC();
+		else
+			hard_enable_TSC();
 	}
+#endif
 }
 
 /*
@@ -649,10 +668,9 @@ struct task_struct fastcall * __switch_t
 	/*
 	 * Now maybe handle debug registers
 	 */
-	if (unlikely(task_thread_info(next_p)->flags & _TIF_WORK_CTXSW))
-		__switch_to_xtra(next_p);
-
-	disable_tsc(prev_p, next_p);
+	if (unlikely(task_thread_info(prev_p)->flags & _TIF_WORK_CTXSW_PREV ||
+		     task_thread_info(next_p)->flags & _TIF_WORK_CTXSW_NEXT))
+		__switch_to_xtra(prev_p, next_p);
 
 	/*
 	 * Leave lazy mode, flushing any hypercalls made here.
--- head-2011-03-17.orig/arch/x86/kernel/setup_32-xen.c	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/setup_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -114,19 +114,10 @@ static unsigned int highmem_pages = -1;
 /*
  * Setup options
  */
-struct drive_info_struct { char dummy[32]; } drive_info;
-#if defined(CONFIG_BLK_DEV_IDE) || defined(CONFIG_BLK_DEV_HD) || \
-    defined(CONFIG_BLK_DEV_IDE_MODULE) || defined(CONFIG_BLK_DEV_HD_MODULE)
-EXPORT_SYMBOL(drive_info);
-#endif
 struct screen_info screen_info;
 EXPORT_SYMBOL(screen_info);
 struct apm_info apm_info;
 EXPORT_SYMBOL(apm_info);
-struct sys_desc_table_struct {
-	unsigned short length;
-	unsigned char table[0];
-};
 struct edid_info edid_info;
 EXPORT_SYMBOL_GPL(edid_info);
 #ifndef CONFIG_XEN
@@ -149,7 +140,7 @@ unsigned long saved_videomode;
 
 static char __initdata command_line[COMMAND_LINE_SIZE];
 
-unsigned char __initdata boot_params[PARAM_SIZE];
+struct boot_params __initdata boot_params;
 
 /*
  * Point at the empty zero page to start with. We map the real shared_info
@@ -316,18 +307,18 @@ unsigned long __init find_max_low_pfn(vo
 		printk(KERN_WARNING "Warning only %ldMB will be used.\n",
 					MAXMEM>>20);
 		if (max_pfn > MAX_NONPAE_PFN)
-			printk(KERN_WARNING "Use a PAE enabled kernel.\n");
+			printk(KERN_WARNING "Use a HIGHMEM64G enabled kernel.\n");
 		else
 			printk(KERN_WARNING "Use a HIGHMEM enabled kernel.\n");
 		max_pfn = MAXMEM_PFN;
 #else /* !CONFIG_HIGHMEM */
-#ifndef CONFIG_X86_PAE
+#ifndef CONFIG_HIGHMEM64G
 		if (max_pfn > MAX_NONPAE_PFN) {
 			max_pfn = MAX_NONPAE_PFN;
 			printk(KERN_WARNING "Warning only 4GB will be used.\n");
-			printk(KERN_WARNING "Use a PAE enabled kernel.\n");
+			printk(KERN_WARNING "Use a HIGHMEM64G enabled kernel.\n");
 		}
-#endif /* !CONFIG_X86_PAE */
+#endif /* !CONFIG_HIGHMEM64G */
 #endif /* !CONFIG_HIGHMEM */
 	} else {
 		if (highmem_pages == -1)
@@ -516,7 +507,7 @@ void __init setup_bootmem_allocator(void
  *
  * This should all compile down to nothing when NUMA is off.
  */
-void __init remapped_pgdat_init(void)
+static void __init remapped_pgdat_init(void)
 {
 	int nid;
 
@@ -591,7 +582,6 @@ void __init setup_arch(char **cmdline_p)
 	   properly.  Setting ROOT_DEV to default to /dev/ram0 breaks initrd.
 	*/
 	ROOT_DEV = MKDEV(UNNAMED_MAJOR,0);
- 	drive_info = DRIVE_INFO;
  	screen_info = SCREEN_INFO;
 	copy_edid();
 	apm_info.bios = APM_BIOS_INFO;
@@ -769,6 +759,8 @@ void __init setup_arch(char **cmdline_p)
 	 * NOTE: at this point the bootmem allocator is fully available.
 	 */
 
+	paravirt_post_allocator_init();
+
 	if (is_initial_xendomain())
 		dmi_scan_machine();
 
@@ -816,6 +808,7 @@ void __init setup_arch(char **cmdline_p)
 #endif
 
 	e820_register_memory();
+	e820_mark_nosave_regions();
 
 	if (is_initial_xendomain()) {
 #ifdef CONFIG_VT
--- head-2011-03-17.orig/arch/x86/kernel/smp_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/smp_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -22,6 +22,7 @@
 
 #include <asm/mtrr.h>
 #include <asm/tlbflush.h>
+#include <asm/mmu_context.h>
 #if 0
 #include <mach_apic.h>
 #endif
@@ -217,13 +218,13 @@ static unsigned long flush_va;
 static DEFINE_SPINLOCK(tlbstate_lock);
 
 /*
- * We cannot call mmdrop() because we are in interrupt context, 
+ * We cannot call mmdrop() because we are in interrupt context,
  * instead update mm->cpu_vm_mask.
  *
  * We need to reload %cr3 since the page tables may be going
  * away from under us..
  */
-static inline void leave_mm (unsigned long cpu)
+void leave_mm(unsigned long cpu)
 {
 	if (per_cpu(cpu_tlbstate, cpu).state == TLBSTATE_OK)
 		BUG();
--- head-2011-03-17.orig/arch/x86/kernel/time-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/time-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -75,11 +75,12 @@
 #include <xen/evtchn.h>
 #include <xen/interface/vcpu.h>
 
-#ifdef CONFIG_X86_32
 #include <asm/i8253.h>
 DEFINE_SPINLOCK(i8253_lock);
 EXPORT_SYMBOL(i8253_lock);
-#else
+
+#ifdef CONFIG_X86_64
+#include <asm/vsyscall.h>
 volatile unsigned long __jiffies __section_jiffies = INITIAL_JIFFIES;
 #endif
 
@@ -760,56 +761,10 @@ unsigned long read_persistent_clock(void
 	return retval;
 }
 
-static void sync_cmos_clock(unsigned long dummy);
-
-static DEFINE_TIMER(sync_cmos_timer, sync_cmos_clock, 0, 0);
-int no_sync_cmos_clock;
-
-static void sync_cmos_clock(unsigned long dummy)
-{
-	struct timeval now, next;
-	int fail = 1;
-
-	/*
-	 * If we have an externally synchronized Linux clock, then update
-	 * CMOS clock accordingly every ~11 minutes. Set_rtc_mmss() has to be
-	 * called as close as possible to 500 ms before the new second starts.
-	 * This code is run on a timer.  If the clock is set, that timer
-	 * may not expire at the correct time.  Thus, we adjust...
-	 */
-	if (!ntp_synced())
-		/*
-		 * Not synced, exit, do not restart a timer (if one is
-		 * running, let it run out).
-		 */
-		return;
-
-	do_gettimeofday(&now);
-	if (now.tv_usec >= USEC_AFTER - ((unsigned) TICK_SIZE) / 2 &&
-	    now.tv_usec <= USEC_BEFORE + ((unsigned) TICK_SIZE) / 2)
-		fail = set_rtc_mmss(now.tv_sec);
-
-	next.tv_usec = USEC_AFTER - now.tv_usec;
-	if (next.tv_usec <= 0)
-		next.tv_usec += USEC_PER_SEC;
-
-	if (!fail)
-		next.tv_sec = 659;
-	else
-		next.tv_sec = 0;
-
-	if (next.tv_usec >= USEC_PER_SEC) {
-		next.tv_sec++;
-		next.tv_usec -= USEC_PER_SEC;
-	}
-	mod_timer(&sync_cmos_timer, jiffies + timeval_to_jiffies(&next));
-}
-
-void notify_arch_cmos_timer(void)
+int update_persistent_clock(struct timespec now)
 {
-	if (!no_sync_cmos_clock)
-		mod_timer(&sync_cmos_timer, jiffies + 1);
 	mod_timer(&sync_xen_wallclock_timer, jiffies + 1);
+	return set_rtc_mmss(now.tv_sec);
 }
 
 extern void (*late_time_init)(void);
--- head-2011-03-17.orig/arch/x86/kernel/traps_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/traps_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -41,6 +41,10 @@
 #include <linux/mca.h>
 #endif
 
+#if defined(CONFIG_EDAC)
+#include <linux/edac.h>
+#endif
+
 #include <asm/processor.h>
 #include <asm/system.h>
 #include <asm/io.h>
@@ -102,36 +106,45 @@ asmlinkage void machine_check(void);
 int kstack_depth_to_print = 24;
 static unsigned int code_bytes = 64;
 
-static inline int valid_stack_ptr(struct thread_info *tinfo, void *p)
+static inline int valid_stack_ptr(struct thread_info *tinfo, void *p, unsigned size)
 {
 	return	p > (void *)tinfo &&
-		p < (void *)tinfo + THREAD_SIZE - 3;
+		p <= (void *)tinfo + THREAD_SIZE - size;
 }
 
+/* The form of the top of the frame on the stack */
+struct stack_frame {
+	struct stack_frame *next_frame;
+	unsigned long return_address;
+};
+
 static inline unsigned long print_context_stack(struct thread_info *tinfo,
 				unsigned long *stack, unsigned long ebp,
 				struct stacktrace_ops *ops, void *data)
 {
-	unsigned long addr;
-
 #ifdef	CONFIG_FRAME_POINTER
-	while (valid_stack_ptr(tinfo, (void *)ebp)) {
-		unsigned long new_ebp;
-		addr = *(unsigned long *)(ebp + 4);
+	struct stack_frame *frame = (struct stack_frame *)ebp;
+	while (valid_stack_ptr(tinfo, frame, sizeof(*frame))) {
+		struct stack_frame *next;
+		unsigned long addr;
+
+		addr = frame->return_address;
 		ops->address(data, addr);
 		/*
 		 * break out of recursive entries (such as
 		 * end_of_stack_stop_unwind_function). Also,
 		 * we can never allow a frame pointer to
 		 * move downwards!
-	 	 */
-	 	new_ebp = *(unsigned long *)ebp;
-		if (new_ebp <= ebp)
+		 */
+		next = frame->next_frame;
+		if (next <= frame)
 			break;
-		ebp = new_ebp;
+		frame = next;
 	}
 #else
-	while (valid_stack_ptr(tinfo, stack)) {
+	while (valid_stack_ptr(tinfo, stack, sizeof(*stack))) {
+		unsigned long addr;
+
 		addr = *stack++;
 		if (__kernel_text_address(addr))
 			ops->address(data, addr);
@@ -154,7 +167,7 @@ void dump_trace(struct task_struct *task
 	if (!stack) {
 		unsigned long dummy;
 		stack = &dummy;
-		if (task && task != current)
+		if (task != current)
 			stack = (unsigned long *)task->thread.esp;
 	}
 
@@ -213,6 +226,7 @@ static void print_trace_address(void *da
 {
 	printk("%s [<%08lx>] ", (char *)data, addr);
 	print_symbol("%s\n", addr);
+	touch_nmi_watchdog();
 }
 
 static struct stacktrace_ops print_trace_ops = {
@@ -396,7 +410,7 @@ void die(const char * str, struct pt_reg
 		unsigned long esp;
 		unsigned short ss;
 
-		report_bug(regs->eip);
+		report_bug(regs->eip, regs);
 
 		printk(KERN_EMERG "%s: %04lx [#%d]\n", str, err & 0xffff, ++die_counter);
 #ifdef CONFIG_PREEMPT
@@ -439,6 +453,7 @@ void die(const char * str, struct pt_reg
 
 	bust_spinlocks(0);
 	die.lock_owner = -1;
+	add_taint(TAINT_DIE);
 	spin_unlock_irqrestore(&die.lock, flags);
 
 	if (!regs)
@@ -523,10 +538,12 @@ fastcall void do_##name(struct pt_regs *
 	do_trap(trapnr, signr, str, 0, regs, error_code, NULL); \
 }
 
-#define DO_ERROR_INFO(trapnr, signr, str, name, sicode, siaddr) \
+#define DO_ERROR_INFO(trapnr, signr, str, name, sicode, siaddr, irq) \
 fastcall void do_##name(struct pt_regs * regs, long error_code) \
 { \
 	siginfo_t info; \
+	if (irq) \
+		local_irq_enable(); \
 	info.si_signo = signr; \
 	info.si_errno = 0; \
 	info.si_code = sicode; \
@@ -566,13 +583,13 @@ DO_VM86_ERROR( 3, SIGTRAP, "int3", int3)
 #endif
 DO_VM86_ERROR( 4, SIGSEGV, "overflow", overflow)
 DO_VM86_ERROR( 5, SIGSEGV, "bounds", bounds)
-DO_ERROR_INFO( 6, SIGILL,  "invalid opcode", invalid_op, ILL_ILLOPN, regs->eip)
+DO_ERROR_INFO( 6, SIGILL,  "invalid opcode", invalid_op, ILL_ILLOPN, regs->eip, 0)
 DO_ERROR( 9, SIGFPE,  "coprocessor segment overrun", coprocessor_segment_overrun)
 DO_ERROR(10, SIGSEGV, "invalid TSS", invalid_TSS)
 DO_ERROR(11, SIGBUS,  "segment not present", segment_not_present)
 DO_ERROR(12, SIGBUS,  "stack segment", stack_segment)
-DO_ERROR_INFO(17, SIGBUS, "alignment check", alignment_check, BUS_ADRALN, 0)
-DO_ERROR_INFO(32, SIGSEGV, "iret exception", iret_error, ILL_BADSTK, 0)
+DO_ERROR_INFO(17, SIGBUS, "alignment check", alignment_check, BUS_ADRALN, 0, 0)
+DO_ERROR_INFO(32, SIGSEGV, "iret exception", iret_error, ILL_BADSTK, 0, 1)
 
 fastcall void __kprobes do_general_protection(struct pt_regs * regs,
 					      long error_code)
@@ -585,6 +602,13 @@ fastcall void __kprobes do_general_prote
 
 	current->thread.error_code = error_code;
 	current->thread.trap_no = 13;
+	if (show_unhandled_signals && unhandled_signal(current, SIGSEGV) &&
+	    printk_ratelimit())
+		printk(KERN_INFO
+		    "%s[%d] general protection eip:%lx esp:%lx error:%lx\n",
+		    current->comm, current->pid,
+		    regs->eip, regs->esp, error_code);
+
 	force_sig(SIGSEGV, current);
 	return;
 
@@ -610,6 +634,14 @@ mem_parity_error(unsigned char reason, s
 	printk(KERN_EMERG "Uhhuh. NMI received for unknown reason %02x on "
 		"CPU %d.\n", reason, smp_processor_id());
 	printk(KERN_EMERG "You have some hardware problem, likely on the PCI bus.\n");
+
+#if defined(CONFIG_EDAC)
+	if(edac_handler_set()) {
+		edac_atomic_assert_error();
+		return;
+	}
+#endif
+
 	if (panic_on_unrecovered_nmi)
                 panic("NMI: Not continuing");
 
@@ -720,6 +752,8 @@ static __kprobes void default_do_nmi(str
 	reassert_nmi();
 }
 
+static int ignore_nmis;
+
 fastcall __kprobes void do_nmi(struct pt_regs * regs, long error_code)
 {
 	int cpu;
@@ -730,11 +764,24 @@ fastcall __kprobes void do_nmi(struct pt
 
 	++nmi_count(cpu);
 
-	default_do_nmi(regs);
+	if (!ignore_nmis)
+		default_do_nmi(regs);
 
 	nmi_exit();
 }
 
+void stop_nmi(void)
+{
+	acpi_nmi_disable();
+	ignore_nmis++;
+}
+
+void restart_nmi(void)
+{
+	ignore_nmis--;
+	acpi_nmi_enable();
+}
+
 #ifdef CONFIG_KPROBES
 fastcall void __kprobes do_int3(struct pt_regs *regs, long error_code)
 {
@@ -1023,6 +1070,7 @@ asmlinkage void math_state_restore(void)
 	thread->status |= TS_USEDFPU;	/* So we fnsave on switch_to() */
 	tsk->fpu_counter++;
 }
+EXPORT_SYMBOL_GPL(math_state_restore);
 
 #ifndef CONFIG_MATH_EMULATION
 
--- head-2011-03-17.orig/arch/x86/mach-xen/setup.c	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/arch/x86/mach-xen/setup.c	2011-01-31 17:49:31.000000000 +0100
@@ -12,6 +12,7 @@
 #include <asm/e820.h>
 #include <asm/setup.h>
 #include <asm/fixmap.h>
+#include <asm/pgtable.h>
 
 #include <xen/interface/callback.h>
 #include <xen/interface/memory.h>
@@ -101,7 +102,7 @@ void __init pre_setup_arch_hook(void)
 
 	init_mm.pgd = swapper_pg_dir = (pgd_t *)xen_start_info->pt_base;
 
-	setup_xen_features();
+	xen_setup_features();
 
 	if (HYPERVISOR_xen_version(XENVER_platform_parameters, &pp) == 0) {
 		hypervisor_virt_start = pp.virt_start;
@@ -157,4 +158,18 @@ void __init machine_specific_arch_setup(
 		HYPERVISOR_nmi_op(XENNMI_register_callback, &cb);
 	}
 #endif
+
+	/* Do an early initialization of the fixmap area */
+	{
+		extern pte_t swapper_pg_pmd[PTRS_PER_PTE];
+		unsigned long addr = __fix_to_virt(FIX_EARLYCON_MEM_BASE);
+		pgd_t *pgd = (pgd_t *)xen_start_info->pt_base;
+		pud_t *pud = pud_offset(pgd + pgd_index(addr), addr);
+		pmd_t *pmd = pmd_offset(pud, addr);
+
+		swapper_pg_dir = pgd;
+		init_mm.pgd    = pgd;
+		make_lowmem_page_readonly(swapper_pg_pmd, XENFEAT_writable_page_tables);
+		set_pmd(pmd, __pmd(__pa_symbol(swapper_pg_pmd) | _PAGE_TABLE));
+	}
 }
--- head-2011-03-17.orig/arch/x86/mm/fault_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/mm/fault_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -346,7 +346,10 @@ static inline pmd_t *vmalloc_sync_one(pg
 	pmd_k = pmd_offset(pud_k, address);
 	if (!pmd_present(*pmd_k))
 		return NULL;
-	if (!pmd_present(*pmd))
+	if (!pmd_present(*pmd)) {
+		bool lazy = x86_read_percpu(xen_lazy_mmu);
+
+		x86_write_percpu(xen_lazy_mmu, false);
 #if CONFIG_XEN_COMPAT > 0x030002
 		set_pmd(pmd, *pmd_k);
 #else
@@ -356,7 +359,8 @@ static inline pmd_t *vmalloc_sync_one(pg
 		 */
 		set_pmd(pmd, __pmd(pmd_val(*pmd_k)));
 #endif
-	else
+		x86_write_percpu(xen_lazy_mmu, lazy);
+	} else
 		BUG_ON(pmd_page(*pmd) != pmd_page(*pmd_k));
 	return pmd_k;
 }
@@ -388,6 +392,8 @@ static inline int vmalloc_fault(unsigned
 	return 0;
 }
 
+int show_unhandled_signals = 1;
+
 /*
  * This routine handles page faults.  It determines the address,
  * and the problem, and then passes it off to one of the appropriate
@@ -408,6 +414,7 @@ fastcall void __kprobes do_page_fault(st
 	struct vm_area_struct * vma;
 	unsigned long address;
 	int write, si_code;
+	int fault;
 
 	/* get the address */
         address = read_cr2();
@@ -541,20 +548,18 @@ good_area:
 	 * make sure we exit gracefully rather than endlessly redo
 	 * the fault.
 	 */
-	switch (handle_mm_fault(mm, vma, address, write)) {
-		case VM_FAULT_MINOR:
-			tsk->min_flt++;
-			break;
-		case VM_FAULT_MAJOR:
-			tsk->maj_flt++;
-			break;
-		case VM_FAULT_SIGBUS:
-			goto do_sigbus;
-		case VM_FAULT_OOM:
+	fault = handle_mm_fault(mm, vma, address, write);
+	if (unlikely(fault & VM_FAULT_ERROR)) {
+		if (fault & VM_FAULT_OOM)
 			goto out_of_memory;
-		default:
-			BUG();
+		else if (fault & VM_FAULT_SIGBUS)
+			goto do_sigbus;
+		BUG();
 	}
+	if (fault & VM_FAULT_MAJOR)
+		tsk->maj_flt++;
+	else
+		tsk->min_flt++;
 
 	/*
 	 * Did it hit the DOS screen memory VA from vm86 mode?
@@ -589,6 +594,14 @@ bad_area_nosemaphore:
 		if (is_prefetch(regs, address, error_code))
 			return;
 
+		if (show_unhandled_signals && unhandled_signal(tsk, SIGSEGV) &&
+		    printk_ratelimit()) {
+			printk("%s%s[%d]: segfault at %08lx eip %08lx "
+			    "esp %08lx error %lx\n",
+			    tsk->pid > 1 ? KERN_INFO : KERN_EMERG,
+			    tsk->comm, tsk->pid, address, regs->eip,
+			    regs->esp, error_code);
+		}
 		tsk->thread.cr2 = address;
 		/* Kernel addresses are always protection faults */
 		tsk->thread.error_code = error_code | (address >= TASK_SIZE);
--- head-2011-03-17.orig/arch/x86/mm/highmem_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/mm/highmem_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -34,17 +34,16 @@ void *kmap_atomic_prot(struct page *page
 	/* even !CONFIG_PREEMPT needs this, for in_atomic in do_page_fault */
 	pagefault_disable();
 
-	idx = type + KM_TYPE_NR*smp_processor_id();
-	BUG_ON(!pte_none(*(kmap_pte-idx)));
-
 	if (!PageHighMem(page))
 		return page_address(page);
 
+	idx = type + KM_TYPE_NR*smp_processor_id();
 	vaddr = __fix_to_virt(FIX_KMAP_BEGIN + idx);
+	BUG_ON(!pte_none(*(kmap_pte-idx)));
 	set_pte_at(&init_mm, vaddr, kmap_pte-idx, mk_pte(page, prot));
 	/*arch_flush_lazy_mmu_mode();*/
 
-	return (void*) vaddr;
+	return (void *)vaddr;
 }
 
 void *kmap_atomic(struct page *page, enum km_type type)
--- head-2011-03-17.orig/arch/x86/mm/init_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/mm/init_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -96,7 +96,7 @@ static pte_t * __init one_page_table_ini
 #endif
 		pte_t *page_table = (pte_t *) alloc_bootmem_low_pages(PAGE_SIZE);
 
-		paravirt_alloc_pt(__pa(page_table) >> PAGE_SHIFT);
+		paravirt_alloc_pt(&init_mm, __pa(page_table) >> PAGE_SHIFT);
 		make_lowmem_page_readonly(page_table,
 					  XENFEAT_writable_page_tables);
 		set_pmd(pmd, __pmd(__pa(page_table) | _PAGE_TABLE));
@@ -453,7 +453,7 @@ static void __init pagetable_init (void)
 	xen_pagetable_setup_done(pgd_base);
 }
 
-#if defined(CONFIG_SOFTWARE_SUSPEND) || defined(CONFIG_ACPI_SLEEP)
+#if defined(CONFIG_HIBERNATION) || defined(CONFIG_ACPI)
 /*
  * Swap suspend & friends need this for resume because things like the intel-agp
  * driver might have split up a kernel 4MB mapping.
@@ -492,9 +492,13 @@ void zap_low_mappings (void)
 	flush_tlb_all();
 }
 
+int nx_enabled = 0;
+
+#ifdef CONFIG_X86_PAE
+
 static int disable_nx __initdata = 0;
 u64 __supported_pte_mask __read_mostly = ~_PAGE_NX;
-EXPORT_SYMBOL(__supported_pte_mask);
+EXPORT_SYMBOL_GPL(__supported_pte_mask);
 
 /*
  * noexec = on|off
@@ -521,9 +525,6 @@ static int __init noexec_setup(char *str
 }
 early_param("noexec", noexec_setup);
 
-int nx_enabled = 0;
-#ifdef CONFIG_X86_PAE
-
 static void __init set_nx(void)
 {
 	unsigned int v[4], l, h;
@@ -770,7 +771,7 @@ void __init mem_init(void)
 	zap_low_mappings();
 #endif
 
-	set_bit(PG_pinned, &virt_to_page(init_mm.pgd)->flags);
+	SetPagePinned(virt_to_page(init_mm.pgd));
 }
 
 #ifdef CONFIG_MEMORY_HOTPLUG
@@ -802,8 +803,7 @@ void __init pgtable_cache_init(void)
 					PTRS_PER_PMD*sizeof(pmd_t),
 					PTRS_PER_PMD*sizeof(pmd_t),
 					SLAB_PANIC,
-					pmd_ctor,
-					NULL);
+					pmd_ctor);
 		if (!SHARED_KERNEL_PMD) {
 			/* If we're in PAE mode and have a non-shared
 			   kernel pmd, then the pgd size must be a
--- head-2011-03-17.orig/arch/x86/mm/ioremap-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/mm/ioremap-xen.c	2011-02-07 15:38:30.000000000 +0100
@@ -344,9 +344,8 @@ void iounmap(volatile void __iomem *addr
 
 	/* Reset the direct mapping. Can block */
 	if ((p->flags >> 20) && is_local_lowmem(p->phys_addr)) {
-		/* p->size includes the guard page, but cpa doesn't like that */
 		change_page_attr(virt_to_page(bus_to_virt(p->phys_addr)),
-				 (p->size - PAGE_SIZE) >> PAGE_SHIFT,
+				 get_vm_area_size(p) >> PAGE_SHIFT,
 				 PAGE_KERNEL);
 		global_flush_tlb();
 	} 
--- head-2011-03-17.orig/arch/x86/mm/pgtable_32-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/mm/pgtable_32-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -198,7 +198,7 @@ void pte_free(struct page *pte)
 				va, pfn_pte(pfn, PAGE_KERNEL), 0))
 				BUG();
 	} else
-		clear_bit(PG_pinned, &pte->flags);
+		ClearPagePinned(pte);
 
 	ClearPageForeign(pte);
 	init_page_count(pte);
@@ -249,7 +249,7 @@ static inline void pgd_list_del(pgd_t *p
 
 #if (PTRS_PER_PMD == 1)
 /* Non-PAE pgd constructor */
-void pgd_ctor(void *pgd)
+static void pgd_ctor(void *pgd)
 {
 	unsigned long flags;
 
@@ -272,7 +272,7 @@ void pgd_ctor(void *pgd)
 }
 #else  /* PTRS_PER_PMD > 1 */
 /* PAE pgd constructor */
-void pgd_ctor(void *pgd)
+static void pgd_ctor(void *pgd)
 {
 	/* PAE, kernel PMD may be shared */
 
@@ -286,7 +286,7 @@ void pgd_ctor(void *pgd)
 }
 #endif	/* PTRS_PER_PMD */
 
-void pgd_dtor(void *pgd)
+static void pgd_dtor(void *pgd)
 {
 	unsigned long flags; /* can be called from interrupt context */
 
@@ -644,9 +644,9 @@ static inline unsigned int pgd_walk_set_
 
 	if (PageHighMem(page)) {
 		if (pgprot_val(flags) & _PAGE_RW)
-			clear_bit(PG_pinned, &page->flags);
+			ClearPagePinned(page);
 		else
-			set_bit(PG_pinned, &page->flags);
+			SetPagePinned(page);
 	} else {
 		MULTI_update_va_mapping(per_cpu(pb_mcl, cpu) + seq,
 				(unsigned long)__va(pfn << PAGE_SHIFT),
@@ -716,19 +716,19 @@ static void __pgd_pin(pgd_t *pgd)
 	pgd_walk(pgd, PAGE_KERNEL_RO);
 	kmap_flush_unused();
 	xen_pgd_pin(__pa(pgd));
-	set_bit(PG_pinned, &virt_to_page(pgd)->flags);
+	SetPagePinned(virt_to_page(pgd));
 }
 
 static void __pgd_unpin(pgd_t *pgd)
 {
 	xen_pgd_unpin(__pa(pgd));
 	pgd_walk(pgd, PAGE_KERNEL);
-	clear_bit(PG_pinned, &virt_to_page(pgd)->flags);
+	ClearPagePinned(virt_to_page(pgd));
 }
 
 static void pgd_test_and_unpin(pgd_t *pgd)
 {
-	if (test_bit(PG_pinned, &virt_to_page(pgd)->flags))
+	if (PagePinned(virt_to_page(pgd)))
 		__pgd_unpin(pgd);
 }
 
@@ -766,7 +766,7 @@ void mm_pin_all(void)
 	 */
 	spin_lock_irqsave(&pgd_lock, flags);
 	for (page = pgd_list; page; page = (struct page *)page->index) {
-		if (!test_bit(PG_pinned, &page->flags))
+		if (!PagePinned(page))
 			__pgd_pin((pgd_t *)page_address(page));
 	}
 	spin_unlock_irqrestore(&pgd_lock, flags);
@@ -774,7 +774,7 @@ void mm_pin_all(void)
 
 void arch_dup_mmap(struct mm_struct *oldmm, struct mm_struct *mm)
 {
-	if (!test_bit(PG_pinned, &virt_to_page(mm->pgd)->flags))
+	if (!PagePinned(virt_to_page(mm->pgd)))
 		mm_pin(mm);
 }
 
@@ -800,7 +800,7 @@ void arch_exit_mmap(struct mm_struct *mm
 
 	task_unlock(tsk);
 
-	if (test_bit(PG_pinned, &virt_to_page(mm->pgd)->flags) &&
+	if (PagePinned(virt_to_page(mm->pgd)) &&
 	    (atomic_read(&mm->mm_count) == 1) &&
 	    !mm->context.has_foreign_mappings)
 		mm_unpin(mm);
--- head-2011-03-17.orig/arch/x86/pci/irq-xen.c	2011-01-31 17:32:16.000000000 +0100
+++ head-2011-03-17/arch/x86/pci/irq-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -142,8 +142,9 @@ static void __init pirq_peer_trick(void)
 	for(i = 1; i < 256; i++) {
 		if (!busmap[i] || pci_find_bus(0, i))
 			continue;
-		if (pci_scan_bus(i, &pci_root_ops, NULL))
-			printk(KERN_INFO "PCI: Discovered primary peer bus %02x [IRQ]\n", i);
+		if (pci_scan_bus_with_sysdata(i))
+			printk(KERN_INFO "PCI: Discovered primary peer "
+			       "bus %02x [IRQ]\n", i);
 	}
 	pcibios_last_bus = -1;
 }
@@ -553,6 +554,7 @@ static __init int intel_router_probe(str
 		case PCI_DEVICE_ID_INTEL_ICH9_3:
 		case PCI_DEVICE_ID_INTEL_ICH9_4:
 		case PCI_DEVICE_ID_INTEL_ICH9_5:
+		case PCI_DEVICE_ID_INTEL_TOLAPAI_0:
 			r->name = "PIIX/ICH";
 			r->get = pirq_piix_get;
 			r->set = pirq_piix_set;
--- head-2011-03-17.orig/arch/x86/xen/Kconfig	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/arch/x86/xen/Kconfig	2011-01-31 17:49:31.000000000 +0100
@@ -2,7 +2,7 @@
 # This Kconfig describes xen options
 #
 
-config XEN
+config PARAVIRT_XEN
 	bool "Xen guest support"
 	select PARAVIRT
 	select PARAVIRT_CLOCK
--- head-2011-03-17.orig/arch/x86/xen/xen-head.S	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/arch/x86/xen/xen-head.S	2011-01-31 17:49:31.000000000 +0100
@@ -1,7 +1,7 @@
 /* Xen-specific pieces of head.S, intended to be included in the right
 	place in head.S */
 
-#ifdef CONFIG_XEN
+#ifdef CONFIG_PARAVIRT_XEN
 
 #include <linux/elfnote.h>
 #include <linux/init.h>
@@ -52,4 +52,4 @@ ENTRY(hypercall_page)
 	ELFNOTE(Xen, XEN_ELFNOTE_HV_START_LOW,   _ASM_PTR __HYPERVISOR_VIRT_START)
 	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   _ASM_PTR 0)
 
-#endif /*CONFIG_XEN */
+#endif /* CONFIG_PARAVIRT_XEN */
--- head-2011-03-17.orig/arch/x86/ia32/ia32entry-xen.S	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/ia32/ia32entry-xen.S	2011-01-31 17:49:31.000000000 +0100
@@ -105,7 +105,7 @@ ENTRY(ia32_sysenter_target)
 	movl	$VSYSCALL32_SYSEXIT,8(%rsp)
 	movq	%rax,(%rsp)
 	cld
-	SAVE_ARGS 0,0,0
+	SAVE_ARGS 0,0,1
  	/* no need to do an access_ok check here because rbp has been
  	   32bit zero extended */ 
 1:	movl	(%rbp),%r9d
@@ -244,7 +244,7 @@ ia32_badarg:
  */ 				
 
 ENTRY(ia32_syscall)
-	CFI_STARTPROC	simple
+	CFI_STARTPROC32	simple
 	CFI_SIGNAL_FRAME
 	CFI_DEF_CFA	rsp,SS+8-RIP+16
 	/*CFI_REL_OFFSET	ss,SS-RIP+16*/
@@ -280,6 +280,7 @@ ia32_sysret:
 
 ia32_tracesys:			 
 	SAVE_REST
+	CLEAR_RREGS
 	movq $-ENOSYS,RAX(%rsp)	/* really needed? */
 	movq %rsp,%rdi        /* &pt_regs -> arg1 */
 	call syscall_trace_enter
@@ -476,7 +477,7 @@ ia32_sys_call_table:
 	.quad sys_init_module
 	.quad sys_delete_module
 	.quad quiet_ni_syscall		/* 130  get_kernel_syms */
-	.quad sys_quotactl
+	.quad sys32_quotactl
 	.quad sys_getpgid
 	.quad sys_fchdir
 	.quad quiet_ni_syscall	/* bdflush */
@@ -669,4 +670,5 @@ ia32_sys_call_table:
 	.quad compat_sys_signalfd
 	.quad compat_sys_timerfd
 	.quad sys_eventfd
+	.quad sys32_fallocate
 ia32_syscall_end:
--- head-2011-03-17.orig/arch/x86/kernel/acpi/sleep_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/acpi/sleep_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -51,12 +51,10 @@
                               Low-Level Sleep Support
    -------------------------------------------------------------------------- */
 
-#ifdef CONFIG_ACPI_SLEEP
-
 #ifndef CONFIG_ACPI_PV_SLEEP
 /* address in low memory of the wakeup routine. */
 unsigned long acpi_wakeup_address = 0;
-unsigned long acpi_video_flags;
+unsigned long acpi_realmode_flags;
 extern char wakeup_start, wakeup_end;
 
 extern unsigned long acpi_copy_wakeup_routine(unsigned long);
@@ -109,9 +107,11 @@ static int __init acpi_sleep_setup(char 
 {
 	while ((str != NULL) && (*str != '\0')) {
 		if (strncmp(str, "s3_bios", 7) == 0)
-			acpi_video_flags = 1;
+			acpi_realmode_flags |= 1;
 		if (strncmp(str, "s3_mode", 7) == 0)
-			acpi_video_flags |= 2;
+			acpi_realmode_flags |= 2;
+		if (strncmp(str, "s3_beep", 7) == 0)
+			acpi_realmode_flags |= 4;
 		str = strchr(str, ',');
 		if (str != NULL)
 			str += strspn(str, ", \t");
@@ -123,8 +123,6 @@ static int __init acpi_sleep_setup(char 
 __setup("acpi_sleep=", acpi_sleep_setup);
 #endif				/* CONFIG_ACPI_PV_SLEEP */
 
-#endif				/*CONFIG_ACPI_SLEEP */
-
 void acpi_pci_link_exit(void)
 {
 }
--- head-2011-03-17.orig/arch/x86/kernel/e820_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/e820_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -224,37 +224,6 @@ unsigned long __init e820_end_of_ram(voi
 }
 
 /*
- * Find the hole size in the range.
- */
-unsigned long __init e820_hole_size(unsigned long start, unsigned long end)
-{
-	unsigned long ram = 0;
-	int i;
-
-	for (i = 0; i < e820.nr_map; i++) {
-		struct e820entry *ei = &e820.map[i];
-		unsigned long last, addr;
-
-		if (ei->type != E820_RAM ||
-		    ei->addr+ei->size <= start ||
-		    ei->addr >= end)
-			continue;
-
-		addr = round_up(ei->addr, PAGE_SIZE);
-		if (addr < start)
-			addr = start;
-
-		last = round_down(ei->addr + ei->size, PAGE_SIZE);
-		if (last >= end)
-			last = end;
-
-		if (last > addr)
-			ram += last - addr;
-	}
-	return ((end - start) - ram);
-}
-
-/*
  * Mark e820 reserved areas as busy for the resource manager.
  */
 void __init e820_reserve_resources(struct e820entry *e820, int nr_map)
@@ -327,54 +296,66 @@ void __init e820_mark_nosave_regions(voi
 }
 #endif
 
+/*
+ * Finds an active region in the address range from start_pfn to end_pfn and
+ * returns its range in ei_startpfn and ei_endpfn for the e820 entry.
+ */
+static int __init e820_find_active_region(const struct e820entry *ei,
+					  unsigned long start_pfn,
+					  unsigned long end_pfn,
+					  unsigned long *ei_startpfn,
+					  unsigned long *ei_endpfn)
+{
+#ifdef CONFIG_XEN
+	if (end_pfn > xen_start_info->nr_pages)
+		end_pfn = xen_start_info->nr_pages;
+#endif
+
+	*ei_startpfn = round_up(ei->addr, PAGE_SIZE) >> PAGE_SHIFT;
+	*ei_endpfn = round_down(ei->addr + ei->size, PAGE_SIZE) >> PAGE_SHIFT;
+
+	/* Skip map entries smaller than a page */
+	if (*ei_startpfn >= *ei_endpfn)
+		return 0;
+
+	/* Check if end_pfn_map should be updated */
+	if (ei->type != E820_RAM && *ei_endpfn > end_pfn_map)
+		end_pfn_map = *ei_endpfn;
+
+	/* Skip if map is outside the node */
+	if (ei->type != E820_RAM || *ei_endpfn <= start_pfn ||
+				    *ei_startpfn >= end_pfn)
+		return 0;
+
+	/* Check for overlaps */
+	if (*ei_startpfn < start_pfn)
+		*ei_startpfn = start_pfn;
+	if (*ei_endpfn > end_pfn)
+		*ei_endpfn = end_pfn;
+
+	/* Obey end_user_pfn to save on memmap */
+	if (*ei_startpfn >= end_user_pfn)
+		return 0;
+	if (*ei_endpfn > end_user_pfn)
+		*ei_endpfn = end_user_pfn;
+
+	return 1;
+}
+
 /* Walk the e820 map and register active regions within a node */
 void __init
 e820_register_active_regions(int nid, unsigned long start_pfn,
 							unsigned long end_pfn)
 {
+	unsigned long ei_startpfn;
+	unsigned long ei_endpfn;
 	int i;
-	unsigned long ei_startpfn, ei_endpfn;
-	for (i = 0; i < e820.nr_map; i++) {
-		struct e820entry *ei = &e820.map[i];
-		ei_startpfn = round_up(ei->addr, PAGE_SIZE) >> PAGE_SHIFT;
-		ei_endpfn = round_down(ei->addr + ei->size, PAGE_SIZE)
-								>> PAGE_SHIFT;
-
-		/* Skip map entries smaller than a page */
-		if (ei_startpfn >= ei_endpfn)
-			continue;
-
-		/* Check if end_pfn_map should be updated */
-		if (ei->type != E820_RAM && ei_endpfn > end_pfn_map)
-			end_pfn_map = ei_endpfn;
-
-		/* Skip if map is outside the node */
-		if (ei->type != E820_RAM ||
-				ei_endpfn <= start_pfn ||
-				ei_startpfn >= end_pfn)
-			continue;
-
-		/* Check for overlaps */
-		if (ei_startpfn < start_pfn)
-			ei_startpfn = start_pfn;
-		if (ei_endpfn > end_pfn)
-			ei_endpfn = end_pfn;
-
-		/* Obey end_user_pfn to save on memmap */
-		if (ei_startpfn >= end_user_pfn)
-			continue;
-		if (ei_endpfn > end_user_pfn)
-			ei_endpfn = end_user_pfn;
-
-#ifdef CONFIG_XEN
-		if (ei_startpfn >= xen_start_info->nr_pages)
-			continue;
-		if (ei_endpfn > xen_start_info->nr_pages)
-			ei_endpfn = xen_start_info->nr_pages;
-#endif
 
-		add_active_range(nid, ei_startpfn, ei_endpfn);
-	}
+	for (i = 0; i < e820.nr_map; i++)
+		if (e820_find_active_region(&e820.map[i],
+					    start_pfn, end_pfn,
+					    &ei_startpfn, &ei_endpfn))
+			add_active_range(nid, ei_startpfn, ei_endpfn);
 #ifdef CONFIG_XEN
 	BUG_ON(nid);
 	add_active_range(nid, end_pfn, end_pfn);
@@ -399,12 +380,35 @@ void __init add_memory_region(unsigned l
 	e820.nr_map++;
 }
 
+/*
+ * Find the hole size (in bytes) in the memory range.
+ * @start: starting address of the memory range to scan
+ * @end: ending address of the memory range to scan
+ */
+unsigned long __init e820_hole_size(unsigned long start, unsigned long end)
+{
+	unsigned long start_pfn = start >> PAGE_SHIFT;
+	unsigned long end_pfn = end >> PAGE_SHIFT;
+	unsigned long ei_startpfn;
+	unsigned long ei_endpfn;
+	unsigned long ram = 0;
+	int i;
+
+	for (i = 0; i < e820.nr_map; i++) {
+		if (e820_find_active_region(&e820.map[i],
+					    start_pfn, end_pfn,
+					    &ei_startpfn, &ei_endpfn))
+			ram += ei_endpfn - ei_startpfn;
+	}
+	return end - start - (ram << PAGE_SHIFT);
+}
+
 void __init e820_print_map(char *who)
 {
 	int i;
 
 	for (i = 0; i < e820.nr_map; i++) {
-		printk(" %s: %016Lx - %016Lx ", who,
+		printk(KERN_INFO " %s: %016Lx - %016Lx ", who,
 			(unsigned long long) e820.map[i].addr,
 			(unsigned long long) (e820.map[i].addr + e820.map[i].size));
 		switch (e820.map[i].type) {
--- head-2011-03-17.orig/arch/x86/kernel/early_printk-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/early_printk-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -174,6 +174,7 @@ static __init void early_serial_init(cha
  * mappings. Someone should fix this for domain 0. For now, use fake serial.
  */
 #define early_vga_console early_serial_console
+#define xenboot_console early_serial_console
 
 #endif
 
@@ -261,20 +262,22 @@ static int __init setup_early_printk(cha
 	} else if (!strncmp(buf, "ttyS", 4)) {
 		early_serial_init(buf);
 		early_console = &early_serial_console;
-	} else if (!strncmp(buf, "vga", 3)
+	} else if (!strncmp(buf, "vga", 3)) {
 #ifndef CONFIG_XEN
 	           && SCREEN_INFO.orig_video_isVGA == 1) {
 		max_xpos = SCREEN_INFO.orig_video_cols;
 		max_ypos = SCREEN_INFO.orig_video_lines;
 		current_ypos = SCREEN_INFO.orig_y;
-#else
-	           || !strncmp(buf, "xen", 3)) {
 #endif
 		early_console = &early_vga_console;
  	} else if (!strncmp(buf, "simnow", 6)) {
  		simnow_init(buf + 6);
  		early_console = &simnow_console;
  		keep_early = 1;
+#ifdef CONFIG_XEN
+	} else if (!strncmp(buf, "xen", 3)) {
+		early_console = &xenboot_console;
+#endif
 	}
 
 	if (keep_early)
--- head-2011-03-17.orig/arch/x86/kernel/entry_64-xen.S	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/entry_64-xen.S	2011-01-31 17:49:31.000000000 +0100
@@ -310,7 +310,7 @@ sysret_signal:
 	TRACE_IRQS_ON
 /*	sti */
         XEN_UNBLOCK_EVENTS(%rsi)        
-	testl $(_TIF_SIGPENDING|_TIF_NOTIFY_RESUME|_TIF_SINGLESTEP),%edx
+	testl $(_TIF_SIGPENDING|_TIF_SINGLESTEP|_TIF_MCE_NOTIFY),%edx
 	jz    1f
 
 	/* Really a signal */
@@ -409,7 +409,7 @@ int_very_careful:
 	jmp int_restore_rest
 	
 int_signal:
-	testl $(_TIF_NOTIFY_RESUME|_TIF_SIGPENDING|_TIF_SINGLESTEP),%edx
+	testl $(_TIF_SIGPENDING|_TIF_SINGLESTEP|_TIF_MCE_NOTIFY),%edx
 	jz 1f
 	movq %rsp,%rdi		# &ptregs -> arg1
 	xorl %esi,%esi		# oldset -> arg2
@@ -552,7 +552,7 @@ retint_careful:
 	jmp retint_check
 	
 retint_signal:
-	testl $(_TIF_SIGPENDING|_TIF_NOTIFY_RESUME|_TIF_SINGLESTEP),%edx
+	testl $(_TIF_SIGPENDING|_TIF_SINGLESTEP|_TIF_MCE_NOTIFY),%edx
 	jz    retint_restore_args
 	TRACE_IRQS_ON
         XEN_UNBLOCK_EVENTS(%rsi)
--- head-2011-03-17.orig/arch/x86/kernel/head_64-xen.S	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/head_64-xen.S	2011-01-31 17:49:31.000000000 +0100
@@ -23,7 +23,7 @@
 #include <asm/dwarf2.h>
 #include <xen/interface/elfnote.h>
 
-	.section .bootstrap.text, "ax", @progbits
+	.section .text.head, "ax", @progbits
 	.code64
 	.globl startup_64
 startup_64:
@@ -39,7 +39,7 @@ startup_64:
 
 #define NEXT_PAGE(name) \
 	.balign	PAGE_SIZE; \
-	phys_##name = . - .bootstrap.text; \
+	phys_##name = . - .text.head; \
 ENTRY(name)
 
 NEXT_PAGE(init_level4_pgt)
@@ -63,6 +63,12 @@ NEXT_PAGE(level3_kernel_pgt)
 NEXT_PAGE(level3_user_pgt)
         .fill	512,8,0
 
+NEXT_PAGE(level2_fixmap_pgt)
+	.fill	512,8,0
+
+NEXT_PAGE(level1_fixmap_pgt)
+	.fill	512,8,0
+
 NEXT_PAGE(hypercall_page)
 	CFI_STARTPROC
 	.rept 0x1000 / 0x20
@@ -169,18 +175,18 @@ ENTRY(empty_zero_page)
 	.byte	0
 #endif /* CONFIG_XEN_COMPAT <= 0x030002 */
 	
-	ELFNOTE(Xen, XEN_ELFNOTE_GUEST_OS,       .asciz, "linux")
-	ELFNOTE(Xen, XEN_ELFNOTE_GUEST_VERSION,  .asciz, "2.6")
-	ELFNOTE(Xen, XEN_ELFNOTE_XEN_VERSION,    .asciz, "xen-3.0")
-	ELFNOTE(Xen, XEN_ELFNOTE_VIRT_BASE,      .quad,  __START_KERNEL_map)
+	ELFNOTE(Xen, XEN_ELFNOTE_GUEST_OS,       .asciz "linux")
+	ELFNOTE(Xen, XEN_ELFNOTE_GUEST_VERSION,  .asciz "2.6")
+	ELFNOTE(Xen, XEN_ELFNOTE_XEN_VERSION,    .asciz "xen-3.0")
+	ELFNOTE(Xen, XEN_ELFNOTE_VIRT_BASE,      .quad __START_KERNEL_map)
 #if CONFIG_XEN_COMPAT <= 0x030002
-	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   .quad,  __START_KERNEL_map)
+	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   .quad __START_KERNEL_map)
 #else
-	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   .quad,  0)
+	ELFNOTE(Xen, XEN_ELFNOTE_PADDR_OFFSET,   .quad 0)
 #endif
-	ELFNOTE(Xen, XEN_ELFNOTE_ENTRY,          .quad,  startup_64)
-	ELFNOTE(Xen, XEN_ELFNOTE_HYPERCALL_PAGE, .quad,  hypercall_page)
-	ELFNOTE(Xen, XEN_ELFNOTE_L1_MFN_VALID,   .quad,  _PAGE_PRESENT,_PAGE_PRESENT)
-	ELFNOTE(Xen, XEN_ELFNOTE_FEATURES,       .asciz, "writable_page_tables|writable_descriptor_tables|auto_translated_physmap|supervisor_mode_kernel")
-	ELFNOTE(Xen, XEN_ELFNOTE_LOADER,         .asciz, "generic")
-	ELFNOTE(Xen, XEN_ELFNOTE_SUSPEND_CANCEL, .long,  1)
+	ELFNOTE(Xen, XEN_ELFNOTE_ENTRY,          .quad startup_64)
+	ELFNOTE(Xen, XEN_ELFNOTE_HYPERCALL_PAGE, .quad hypercall_page)
+	ELFNOTE(Xen, XEN_ELFNOTE_L1_MFN_VALID,   .quad _PAGE_PRESENT, _PAGE_PRESENT)
+	ELFNOTE(Xen, XEN_ELFNOTE_FEATURES,       .asciz "writable_page_tables|writable_descriptor_tables|auto_translated_physmap|supervisor_mode_kernel")
+	ELFNOTE(Xen, XEN_ELFNOTE_LOADER,         .asciz "generic")
+	ELFNOTE(Xen, XEN_ELFNOTE_SUSPEND_CANCEL, .long 1)
--- head-2011-03-17.orig/arch/x86/kernel/head64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/head64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -90,7 +90,7 @@ void __init x86_64_start_kernel(char * r
 	unsigned long machine_to_phys_nr_ents;
 	int i;
 
-	setup_xen_features();
+	xen_setup_features();
 
 	xen_start_info = (struct start_info *)real_mode_data;
 	if (!xen_feature(XENFEAT_auto_translated_physmap))
--- head-2011-03-17.orig/arch/x86/kernel/io_apic_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/io_apic_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -165,7 +165,9 @@ static inline void io_apic_write(unsigne
 #endif
 }
 
-#ifndef CONFIG_XEN
+#ifdef CONFIG_XEN
+#define io_apic_modify io_apic_write
+#else
 /*
  * Re-write a value: to be used for read-modify-write
  * cycles where the read already set up the index register.
@@ -175,8 +177,32 @@ static inline void io_apic_modify(unsign
 	struct io_apic __iomem *io_apic = io_apic_base(apic);
 	writel(value, &io_apic->data);
 }
-#else
-#define io_apic_modify io_apic_write
+
+static int io_apic_level_ack_pending(unsigned int irq)
+{
+	struct irq_pin_list *entry;
+	unsigned long flags;
+	int pending = 0;
+
+	spin_lock_irqsave(&ioapic_lock, flags);
+	entry = irq_2_pin + irq;
+	for (;;) {
+		unsigned int reg;
+		int pin;
+
+		pin = entry->pin;
+		if (pin == -1)
+			break;
+		reg = io_apic_read(entry->apic, 0x10 + pin*2);
+		/* Is the remote IRR bit set? */
+		pending |= (reg >> 14) & 1;
+		if (!entry->next)
+			break;
+		entry = irq_2_pin + entry->next;
+	}
+	spin_unlock_irqrestore(&ioapic_lock, flags);
+	return pending;
+}
 #endif
 
 /*
@@ -406,14 +432,12 @@ static void clear_IO_APIC (void)
 int skip_ioapic_setup;
 int ioapic_force;
 
-/* dummy parsing: see setup.c */
-
-static int __init disable_ioapic_setup(char *str)
+static int __init parse_noapic(char *str)
 {
-	skip_ioapic_setup = 1;
+	disable_ioapic_setup();
 	return 0;
 }
-early_param("noapic", disable_ioapic_setup);
+early_param("noapic", parse_noapic);
 
 /* Actually the next is obsolete, but keep it for paranoid reasons -AK */
 static int __init disable_timer_pin_setup(char *arg)
@@ -765,12 +789,15 @@ static struct irq_chip ioapic_chip;
 
 static void ioapic_register_intr(int irq, unsigned long trigger)
 {
-	if (trigger)
+	if (trigger) {
+		irq_desc[irq].status |= IRQ_LEVEL;
 		set_irq_chip_and_handler_name(irq, &ioapic_chip,
 					      handle_fasteoi_irq, "fasteoi");
-	else
+	} else {
+		irq_desc[irq].status &= ~IRQ_LEVEL;
 		set_irq_chip_and_handler_name(irq, &ioapic_chip,
 					      handle_edge_irq, "edge");
+	}
 }
 #else
 #define ioapic_register_intr(irq, trigger) evtchn_register_pirq(irq)
@@ -1419,9 +1446,37 @@ static void ack_apic_level(unsigned int 
 	ack_APIC_irq();
 
 	/* Now we can move and renable the irq */
-	move_masked_irq(irq);
-	if (unlikely(do_unmask_irq))
+	if (unlikely(do_unmask_irq)) {
+		/* Only migrate the irq if the ack has been received.
+		 *
+		 * On rare occasions the broadcast level triggered ack gets
+		 * delayed going to ioapics, and if we reprogram the
+		 * vector while Remote IRR is still set the irq will never
+		 * fire again.
+		 *
+		 * To prevent this scenario we read the Remote IRR bit
+		 * of the ioapic.  This has two effects.
+		 * - On any sane system the read of the ioapic will
+		 *   flush writes (and acks) going to the ioapic from
+		 *   this cpu.
+		 * - We get to see if the ACK has actually been delivered.
+		 *
+		 * Based on failed experiments of reprogramming the
+		 * ioapic entry from outside of irq context starting
+		 * with masking the ioapic entry and then polling until
+		 * Remote IRR was clear before reprogramming the
+		 * ioapic I don't trust the Remote IRR bit to be
+		 * completey accurate.
+		 *
+		 * However there appears to be no other way to plug
+		 * this race, so if the Remote IRR bit is not
+		 * accurate and is causing problems then it is a hardware bug
+		 * and you can go talk to the chipset vendor about it.
+		 */
+		if (!io_apic_level_ack_pending(irq))
+			move_masked_irq(irq);
 		unmask_IO_APIC_irq(irq);
+	}
 }
 
 static struct irq_chip ioapic_chip __read_mostly = {
--- head-2011-03-17.orig/arch/x86/kernel/ldt_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/ldt_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -114,6 +114,8 @@ int init_new_context(struct task_struct 
 	memset(&mm->context, 0, sizeof(mm->context));
 	init_MUTEX(&mm->context.sem);
 	old_mm = current->mm;
+	if (old_mm)
+		mm->context.vdso = old_mm->context.vdso;
 	if (old_mm && old_mm->context.size > 0) {
 		down(&old_mm->context.sem);
 		retval = copy_ldt(&mm->context, &old_mm->context);
@@ -146,7 +148,7 @@ void destroy_context(struct mm_struct *m
 			kfree(mm->context.ldt);
 		mm->context.size = 0;
 	}
-	if (!mm->context.pinned) {
+	if (!PagePinned(virt_to_page(mm->pgd))) {
 		spin_lock(&mm_unpinned_lock);
 		list_del(&mm->context.unpinned);
 		spin_unlock(&mm_unpinned_lock);
--- head-2011-03-17.orig/arch/x86/kernel/mpparse_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/mpparse_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -32,7 +32,6 @@
 
 /* Have we found an MP table */
 int smp_found_config;
-unsigned int __initdata maxcpus = NR_CPUS;
 
 /*
  * Various Linux-internal data structures created from the
@@ -657,6 +656,20 @@ static int mp_find_ioapic(int gsi)
 	return -1;
 }
 
+static u8 uniq_ioapic_id(u8 id)
+{
+	int i;
+	DECLARE_BITMAP(used, 256);
+	bitmap_zero(used, 256);
+	for (i = 0; i < nr_ioapics; i++) {
+		struct mpc_config_ioapic *ia = &mp_ioapics[i];
+		__set_bit(ia->mpc_apicid, used);
+	}
+	if (!test_bit(id, used))
+		return id;
+	return find_first_zero_bit(used, 256);
+}
+
 void __init mp_register_ioapic(u8 id, u32 address, u32 gsi_base)
 {
 	int idx = 0;
@@ -664,7 +677,7 @@ void __init mp_register_ioapic(u8 id, u3
 	if (bad_ioapic(address))
 		return;
 
-	idx = nr_ioapics++;
+	idx = nr_ioapics;
 
 	mp_ioapics[idx].mpc_type = MP_IOAPIC;
 	mp_ioapics[idx].mpc_flags = MPC_APIC_USABLE;
@@ -673,7 +686,7 @@ void __init mp_register_ioapic(u8 id, u3
 #ifndef CONFIG_XEN
 	set_fixmap_nocache(FIX_IO_APIC_BASE_0 + idx, address);
 #endif
-	mp_ioapics[idx].mpc_apicid = id;
+	mp_ioapics[idx].mpc_apicid = uniq_ioapic_id(id);
 	mp_ioapics[idx].mpc_apicver = 0;
 	
 	/* 
@@ -690,6 +703,8 @@ void __init mp_register_ioapic(u8 id, u3
 		mp_ioapics[idx].mpc_apicaddr,
 		mp_ioapic_routing[idx].gsi_start,
 		mp_ioapic_routing[idx].gsi_end);
+
+	nr_ioapics++;
 }
 
 void __init
--- head-2011-03-17.orig/arch/x86/kernel/process_64-xen.c	2011-02-02 08:31:39.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/process_64-xen.c	2011-02-02 08:31:50.000000000 +0100
@@ -26,6 +26,7 @@
 #include <linux/sched.h>
 #include <linux/kernel.h>
 #include <linux/mm.h>
+#include <linux/fs.h>
 #include <linux/elfcore.h>
 #include <linux/smp.h>
 #include <linux/slab.h>
@@ -248,6 +249,7 @@ early_param("idle", idle_setup);
 void __show_regs(struct pt_regs * regs)
 {
 	unsigned long fs, gs, shadowgs;
+	unsigned long d0, d1, d2, d3, d6, d7;
 	unsigned int fsindex,gsindex;
 	unsigned int ds,cs,es; 
 
@@ -287,6 +289,14 @@ void __show_regs(struct pt_regs * regs)
 	       fs,fsindex,gs,gsindex,shadowgs); 
 	printk("CS:  %04x DS: %04x ES: %04x\n", cs, ds, es); 
 
+	get_debugreg(d0, 0);
+	get_debugreg(d1, 1);
+	get_debugreg(d2, 2);
+	printk("DR0: %016lx DR1: %016lx DR2: %016lx\n", d0, d1, d2);
+	get_debugreg(d3, 3);
+	get_debugreg(d6, 6);
+	get_debugreg(d7, 7);
+	printk("DR3: %016lx DR6: %016lx DR7: %016lx\n", d3, d6, d7);
 }
 
 void show_regs(struct pt_regs *regs)
--- head-2011-03-17.orig/arch/x86/kernel/setup_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/setup_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -828,6 +828,8 @@ static void __cpuinit init_amd(struct cp
 	level = cpuid_eax(1);
 	if (c->x86 == 15 && ((level >= 0x0f48 && level < 0x0f50) || level >= 0x0f58))
 		set_bit(X86_FEATURE_REP_GOOD, &c->x86_capability);
+	if (c->x86 == 0x10)
+		set_bit(X86_FEATURE_REP_GOOD, &c->x86_capability);
 
 	/* Enable workaround for FXSAVE leak */
 	if (c->x86 >= 6)
@@ -853,8 +855,14 @@ static void __cpuinit init_amd(struct cp
 	if (c->extended_cpuid_level >= 0x80000008)
 		amd_detect_cmp(c);
 
-	/* Fix cpuid4 emulation for more */
-	num_cache_leaves = 3;
+	if (c->extended_cpuid_level >= 0x80000006 &&
+		(cpuid_edx(0x80000006) & 0xf000))
+		num_cache_leaves = 4;
+	else
+		num_cache_leaves = 3;
+
+	if (c->x86 == 0xf || c->x86 == 0x10 || c->x86 == 0x11)
+		set_bit(X86_FEATURE_K8, &c->x86_capability);
 
 	/* RDTSC can be speculated around */
 	clear_bit(X86_FEATURE_SYNC_RDTSC, &c->x86_capability);
@@ -1099,6 +1107,8 @@ void __cpuinit identify_cpu(struct cpuin
 			c->x86_capability[2] = cpuid_edx(0x80860001);
 	}
 
+	init_scattered_cpuid_features(c);
+
 #ifndef CONFIG_XEN
 	c->apicid = phys_pkg_id(0);
 #endif
@@ -1186,7 +1196,7 @@ static int show_cpuinfo(struct seq_file 
 	        "fpu", "vme", "de", "pse", "tsc", "msr", "pae", "mce",
 	        "cx8", "apic", NULL, "sep", "mtrr", "pge", "mca", "cmov",
 	        "pat", "pse36", "pn", "clflush", NULL, "dts", "acpi", "mmx",
-	        "fxsr", "sse", "sse2", "ss", "ht", "tm", "ia64", NULL,
+	        "fxsr", "sse", "sse2", "ss", "ht", "tm", "ia64", "pbe",
 
 		/* AMD-defined */
 		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
@@ -1202,10 +1212,11 @@ static int show_cpuinfo(struct seq_file 
 		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
 
 		/* Other (Linux-defined) */
-		"cxmmx", NULL, "cyrix_arr", "centaur_mcr", NULL,
-		"constant_tsc", NULL, NULL,
-		"up", NULL, NULL, NULL, NULL, NULL, NULL, NULL,
-		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
+		"cxmmx", "k6_mtrr", "cyrix_arr", "centaur_mcr",
+		NULL, NULL, NULL, NULL,
+		"constant_tsc", "up", NULL, "arch_perfmon",
+		"pebs", "bts", NULL, "sync_rdtsc",
+		"rep_good", NULL, NULL, NULL, NULL, NULL, NULL, NULL,
 		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
 
 		/* Intel-defined (#2) */
@@ -1216,7 +1227,7 @@ static int show_cpuinfo(struct seq_file 
 
 		/* VIA/Cyrix/Centaur-defined */
 		NULL, NULL, "rng", "rng_en", NULL, NULL, "ace", "ace_en",
-		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
+		"ace2", "ace2_en", "phe", "phe_en", "pmm", "pmm_en", NULL, NULL,
 		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
 		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
 
@@ -1227,6 +1238,12 @@ static int show_cpuinfo(struct seq_file 
 		"osvw", "ibs", NULL, NULL, NULL, NULL,
 		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
 		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
+
+		/* Auxiliary (Linux-defined) */
+		"ida", NULL, NULL, NULL, NULL, NULL, NULL, NULL,
+		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
+		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
+		NULL, NULL, NULL, NULL, NULL, NULL, NULL, NULL,
 	};
 	static char *x86_power_flags[] = { 
 		"ts",	/* temperature sensor */
--- head-2011-03-17.orig/arch/x86/kernel/setup64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/setup64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -125,11 +125,14 @@ void __init setup_per_cpu_areas(void)
 } 
 
 #ifdef CONFIG_XEN
-static void switch_pt(void)
+static void __init_refok switch_pt(int cpu)
 {
+	if (cpu == 0)
+		xen_init_pt();
 	xen_pt_switch(__pa_symbol(init_level4_pgt));
 	xen_new_user_pt(__pa_symbol(__user_pgd(init_level4_pgt)));
 }
+#define switch_pt() switch_pt(cpu)
 
 static void __cpuinit cpu_gdt_init(const struct desc_ptr *gdt_descr)
 {
@@ -185,9 +188,6 @@ void pda_init(int cpu)
 	pda->mmu_state = 0;
 
 	if (cpu == 0) {
-#ifdef CONFIG_XEN
-		xen_init_pt();
-#endif
 		/* others are initialized in smpboot.c */
 		pda->pcurrent = &init_task;
 		pda->irqstackptr = boot_cpu_stack; 
--- head-2011-03-17.orig/arch/x86/kernel/smp_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/smp_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -362,7 +362,7 @@ __smp_call_function_single(int cpu, void
 }
 
 /*
- * smp_call_function_single - Run a function on another CPU
+ * smp_call_function_single - Run a function on a specific CPU
  * @func: The function to run. This must be fast and non-blocking.
  * @info: An arbitrary pointer to pass to the function.
  * @nonatomic: Currently unused.
@@ -379,17 +379,21 @@ int smp_call_function_single (int cpu, v
 {
 	/* prevent preemption and reschedule on another processor */
 	int me = get_cpu();
+
+	/* Can deadlock when called with interrupts disabled */
+	WARN_ON(irqs_disabled());
+
 	if (cpu == me) {
+		local_irq_disable();
+		func(info);
+		local_irq_enable();
 		put_cpu();
 		return 0;
 	}
 
-	/* Can deadlock when called with interrupts disabled */
-	WARN_ON(irqs_disabled());
-
-	spin_lock_bh(&call_lock);
+	spin_lock(&call_lock);
 	__smp_call_function_single(cpu, func, info, nonatomic, wait);
-	spin_unlock_bh(&call_lock);
+	spin_unlock(&call_lock);
 	put_cpu();
 	return 0;
 }
--- head-2011-03-17.orig/arch/x86/kernel/traps_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/traps_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -34,6 +34,10 @@
 #include <linux/bug.h>
 #include <linux/kdebug.h>
 
+#if defined(CONFIG_EDAC)
+#include <linux/edac.h>
+#endif
+
 #include <asm/system.h>
 #include <asm/io.h>
 #include <asm/atomic.h>
@@ -332,6 +336,7 @@ static int print_trace_stack(void *data,
 
 static void print_trace_address(void *data, unsigned long addr)
 {
+	touch_nmi_watchdog();
 	printk_address(addr);
 }
 
@@ -520,6 +525,7 @@ void __kprobes __die(const char * str, s
 	printk("\n");
 	notify_die(DIE_OOPS, str, regs, err, current->thread.trap_no, SIGSEGV);
 	show_registers(regs);
+	add_taint(TAINT_DIE);
 	/* Executive summary in case the oops scrolled away */
 	printk(KERN_ALERT "RIP ");
 	printk_address(regs->rip); 
@@ -533,7 +539,7 @@ void die(const char * str, struct pt_reg
 	unsigned long flags = oops_begin();
 
 	if (!user_mode(regs))
-		report_bug(regs->rip);
+		report_bug(regs->rip, regs);
 
 	__die(str, regs, err);
 	oops_end(flags);
@@ -582,7 +588,8 @@ static void __kprobes do_trap(int trapnr
 		tsk->thread.error_code = error_code;
 		tsk->thread.trap_no = trapnr;
 
-		if (exception_trace && unhandled_signal(tsk, signr))
+		if (show_unhandled_signals && unhandled_signal(tsk, signr) &&
+		    printk_ratelimit())
 			printk(KERN_INFO
 			       "%s[%d] trap %s rip:%lx rsp:%lx error:%lx\n",
 			       tsk->comm, tsk->pid, str,
@@ -686,7 +693,8 @@ asmlinkage void __kprobes do_general_pro
 		tsk->thread.error_code = error_code;
 		tsk->thread.trap_no = 13;
 
-		if (exception_trace && unhandled_signal(tsk, SIGSEGV))
+		if (show_unhandled_signals && unhandled_signal(tsk, SIGSEGV) &&
+		    printk_ratelimit())
 			printk(KERN_INFO
 		       "%s[%d] general protection rip:%lx rsp:%lx error:%lx\n",
 			       tsk->comm, tsk->pid,
@@ -721,6 +729,13 @@ mem_parity_error(unsigned char reason, s
 		reason);
 	printk(KERN_EMERG "You have some hardware problem, likely on the PCI bus.\n");
 
+#if defined(CONFIG_EDAC)
+	if(edac_handler_set()) {
+		edac_atomic_assert_error();
+		return;
+	}
+#endif
+
 	if (panic_on_unrecovered_nmi)
 		panic("NMI: Not continuing");
 
--- head-2011-03-17.orig/arch/x86/kernel/vsyscall_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/kernel/vsyscall_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -42,6 +42,7 @@
 #include <asm/segment.h>
 #include <asm/desc.h>
 #include <asm/topology.h>
+#include <asm/vgtod.h>
 
 #define __vsyscall(nr) __attribute__ ((unused,__section__(".vsyscall_" #nr)))
 #define __syscall_clobber "r11","rcx","memory"
@@ -57,26 +58,9 @@
  * - writen by timer interrupt or systcl (/proc/sys/kernel/vsyscall64)
  * Try to keep this structure as small as possible to avoid cache line ping pongs
  */
-struct vsyscall_gtod_data_t {
-	seqlock_t	lock;
-
-	/* open coded 'struct timespec' */
-	time_t		wall_time_sec;
-	u32		wall_time_nsec;
-
-	int		sysctl_enabled;
-	struct timezone sys_tz;
-	struct { /* extract of a clocksource struct */
-		cycle_t (*vread)(void);
-		cycle_t	cycle_last;
-		cycle_t	mask;
-		u32	mult;
-		u32	shift;
-	} clock;
-};
 int __vgetcpu_mode __section_vgetcpu_mode;
 
-struct vsyscall_gtod_data_t __vsyscall_gtod_data __section_vsyscall_gtod_data =
+struct vsyscall_gtod_data __vsyscall_gtod_data __section_vsyscall_gtod_data =
 {
 	.lock = SEQLOCK_UNLOCKED,
 	.sysctl_enabled = 1,
@@ -96,6 +80,8 @@ void update_vsyscall(struct timespec *wa
 	vsyscall_gtod_data.wall_time_sec = wall_time->tv_sec;
 	vsyscall_gtod_data.wall_time_nsec = wall_time->tv_nsec;
 	vsyscall_gtod_data.sys_tz = sys_tz;
+	vsyscall_gtod_data.wall_time_nsec = wall_time->tv_nsec;
+	vsyscall_gtod_data.wall_to_monotonic = wall_to_monotonic;
 	write_sequnlock_irqrestore(&vsyscall_gtod_data.lock, flags);
 }
 
--- head-2011-03-17.orig/arch/x86/mm/fault_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/mm/fault_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -159,7 +159,9 @@ void dump_pagetable(unsigned long addres
 	pmd_t *pmd;
 	pte_t *pte;
 
-	pgd = __va(read_cr3() & PHYSICAL_PAGE_MASK);
+	pgd = (pgd_t *)read_cr3();
+
+	pgd = __va((unsigned long)pgd & PHYSICAL_PAGE_MASK);
 	pgd += pgd_index(address);
 	if (bad_address(pgd)) goto bad;
 	printk("PGD %lx ", pgd_val(*pgd));
@@ -219,16 +221,6 @@ static int is_errata93(struct pt_regs *r
 	return 0;
 } 
 
-int unhandled_signal(struct task_struct *tsk, int sig)
-{
-	if (is_init(tsk))
-		return 1;
-	if (tsk->ptrace & PT_PTRACED)
-		return 0;
-	return (tsk->sighand->action[sig-1].sa.sa_handler == SIG_IGN) ||
-		(tsk->sighand->action[sig-1].sa.sa_handler == SIG_DFL);
-}
-
 static noinline void pgtable_bad(unsigned long address, struct pt_regs *regs,
 				 unsigned long error_code)
 {
@@ -302,8 +294,8 @@ static int vmalloc_fault(unsigned long a
 	return 0;
 }
 
-int page_fault_trace = 0;
-int exception_trace = 1;
+static int page_fault_trace;
+int show_unhandled_signals = 1;
 
 
 #define MEM_VERBOSE 1
@@ -372,7 +364,7 @@ asmlinkage void __kprobes do_page_fault(
 	struct vm_area_struct * vma;
 	unsigned long address;
 	const struct exception_table_entry *fixup;
-	int write;
+	int write, fault;
 	unsigned long flags;
 	siginfo_t info;
 
@@ -384,7 +376,7 @@ asmlinkage void __kprobes do_page_fault(
 	prefetchw(&mm->mmap_sem);
 
 	/* get the address */
-	address = current_vcpu_info()->arch.cr2;
+	address = read_cr2();
 
 	info.si_code = SEGV_MAPERR;
 
@@ -445,6 +437,13 @@ asmlinkage void __kprobes do_page_fault(
 	if (unlikely(in_atomic() || !mm))
 		goto bad_area_nosemaphore;
 
+	/*
+	 * User-mode registers count as a user access even for any
+	 * potential system fault or CPU buglet.
+	 */
+	if (user_mode_vm(regs))
+		error_code |= PF_USER;
+
  again:
 	/* When running in the kernel we expect faults to occur only to
 	 * addresses in user space.  All other faults represent errors in the
@@ -511,19 +510,18 @@ good_area:
 	 * make sure we exit gracefully rather than endlessly redo
 	 * the fault.
 	 */
-	switch (handle_mm_fault(mm, vma, address, write)) {
-	case VM_FAULT_MINOR:
-		tsk->min_flt++;
-		break;
-	case VM_FAULT_MAJOR:
-		tsk->maj_flt++;
-		break;
-	case VM_FAULT_SIGBUS:
-		goto do_sigbus;
-	default:
-		goto out_of_memory;
+	fault = handle_mm_fault(mm, vma, address, write);
+	if (unlikely(fault & VM_FAULT_ERROR)) {
+		if (fault & VM_FAULT_OOM)
+			goto out_of_memory;
+		else if (fault & VM_FAULT_SIGBUS)
+			goto do_sigbus;
+		BUG();
 	}
-
+	if (fault & VM_FAULT_MAJOR)
+		tsk->maj_flt++;
+	else
+		tsk->min_flt++;
 	up_read(&mm->mmap_sem);
 	return;
 
@@ -556,7 +554,8 @@ bad_area_nosemaphore:
 		    (address >> 32))
 			return;
 
-		if (exception_trace && unhandled_signal(tsk, SIGSEGV)) {
+		if (show_unhandled_signals && unhandled_signal(tsk, SIGSEGV) &&
+		    printk_ratelimit()) {
 			printk(
 		       "%s%s[%d]: segfault at %016lx rip %016lx rsp %016lx error %lx\n",
 					tsk->pid > 1 ? KERN_INFO : KERN_EMERG,
@@ -630,7 +629,7 @@ out_of_memory:
 	}
 	printk("VM: killing process %s\n", tsk->comm);
 	if (error_code & 4)
-		do_exit(SIGKILL);
+		do_group_exit(SIGKILL);
 	goto no_context;
 
 do_sigbus:
--- head-2011-03-17.orig/arch/x86/mm/init_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/mm/init_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -66,6 +66,9 @@ int after_bootmem;
 DEFINE_PER_CPU(struct mmu_gather, mmu_gathers);
 extern unsigned long start_pfn;
 
+extern pmd_t level2_fixmap_pgt[PTRS_PER_PMD];
+extern pte_t level1_fixmap_pgt[PTRS_PER_PTE];
+
 /*
  * Use this until direct mapping is established, i.e. before __va() is 
  * available in init_memory_mapping().
@@ -362,6 +365,10 @@ __set_fixmap (enum fixed_addresses idx, 
 		set_pte_phys(address, phys, prot, 0);
 		set_pte_phys(address, phys, prot, 1);
 		break;
+	case FIX_EARLYCON_MEM_BASE:
+		xen_l1_entry_update(level1_fixmap_pgt + pte_index(address),
+				    pfn_pte_ma(phys >> PAGE_SHIFT, prot));
+		break;
 	default:
 		set_pte_phys_ma(address, phys, prot);
 		break;
@@ -595,6 +602,19 @@ void __init xen_init_pt(void)
 	__user_pgd(init_level4_pgt)[pgd_index(VSYSCALL_START)] =
 		__pgd(__pa_symbol(level3_user_pgt) | _PAGE_TABLE);
 
+	/* Do an early initialization of the fixmap area. */
+	addr = __fix_to_virt(FIX_EARLYCON_MEM_BASE);
+	if (pud_present(level3_kernel_pgt[pud_index(addr)])) {
+		unsigned long adr = page[pud_index(addr)];
+
+		addr_to_page(adr, page);
+		copy_page(level2_fixmap_pgt, page);
+	}
+	level3_kernel_pgt[pud_index(addr)] =
+		__pud(__pa_symbol(level2_fixmap_pgt) | _PAGE_TABLE);
+	level2_fixmap_pgt[pmd_index(addr)] =
+		__pmd(__pa_symbol(level1_fixmap_pgt) | _PAGE_TABLE);
+
 	early_make_page_readonly(init_level4_pgt,
 				 XENFEAT_writable_page_tables);
 	early_make_page_readonly(__user_pgd(init_level4_pgt),
@@ -603,6 +623,10 @@ void __init xen_init_pt(void)
 				 XENFEAT_writable_page_tables);
 	early_make_page_readonly(level3_user_pgt,
 				 XENFEAT_writable_page_tables);
+	early_make_page_readonly(level2_fixmap_pgt,
+				 XENFEAT_writable_page_tables);
+	early_make_page_readonly(level1_fixmap_pgt,
+				 XENFEAT_writable_page_tables);
 
 	if (!xen_feature(XENFEAT_writable_page_tables)) {
 		xen_pgd_pin(__pa_symbol(init_level4_pgt));
@@ -832,7 +856,7 @@ void __init paging_init(void)
 	sparse_init();
 	free_area_init_nodes(max_zone_pfns);
 
-	init_mm.context.pinned = 1;
+	SetPagePinned(virt_to_page(init_mm.pgd));
 }
 #endif
 
@@ -1155,41 +1179,6 @@ int kern_addr_valid(unsigned long addr) 
 	return pfn_valid(pte_pfn(*pte));
 }
 
-#ifdef CONFIG_SYSCTL
-#include <linux/sysctl.h>
-
-extern int exception_trace, page_fault_trace;
-
-static ctl_table debug_table2[] = {
-	{
-		.ctl_name	= 99,
-		.procname	= "exception-trace",
-		.data		= &exception_trace,
-		.maxlen		= sizeof(int),
-		.mode		= 0644,
-		.proc_handler	= proc_dointvec
-	},
-	{}
-}; 
-
-static ctl_table debug_root_table2[] = { 
-	{
-		.ctl_name = CTL_DEBUG,
-		.procname = "debug",
-		.mode = 0555,
-		.child = debug_table2
-	},
-	{}
-}; 
-
-static __init int x8664_sysctl_init(void)
-{ 
-	register_sysctl_table(debug_root_table2);
-	return 0;
-}
-__initcall(x8664_sysctl_init);
-#endif
-
 /* A pseudo VMA to allow ptrace access for the vsyscall page.  This only
    covers the 64bit vsyscall page now. 32bit has a real VMA now and does
    not need special handling anymore. */
@@ -1228,9 +1217,18 @@ int in_gate_area_no_task(unsigned long a
 }
 
 #ifndef CONFIG_XEN
-void *alloc_bootmem_high_node(pg_data_t *pgdat, unsigned long size)
+void * __init alloc_bootmem_high_node(pg_data_t *pgdat, unsigned long size)
 {
 	return __alloc_bootmem_core(pgdat->bdata, size,
 			SMP_CACHE_BYTES, (4UL*1024*1024*1024), 0);
 }
 #endif
+
+const char *arch_vma_name(struct vm_area_struct *vma)
+{
+	if (vma->vm_mm && vma->vm_start == (long)vma->vm_mm->context.vdso)
+		return "[vdso]";
+	if (vma == &gate_vma)
+		return "[vsyscall]";
+	return NULL;
+}
--- head-2011-03-17.orig/arch/x86/mm/pageattr_64-xen.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/mm/pageattr_64-xen.c	2011-01-31 17:49:31.000000000 +0100
@@ -171,7 +171,7 @@ void mm_pin(struct mm_struct *mm)
 	mm_walk(mm, PAGE_KERNEL_RO);
 	xen_pgd_pin(__pa(mm->pgd)); /* kernel */
 	xen_pgd_pin(__pa(__user_pgd(mm->pgd))); /* user */
-	mm->context.pinned = 1;
+	SetPagePinned(virt_to_page(mm->pgd));
 	spin_lock(&mm_unpinned_lock);
 	list_del(&mm->context.unpinned);
 	spin_unlock(&mm_unpinned_lock);
@@ -189,7 +189,7 @@ void mm_unpin(struct mm_struct *mm)
 	xen_pgd_unpin(__pa(mm->pgd));
 	xen_pgd_unpin(__pa(__user_pgd(mm->pgd)));
 	mm_walk(mm, PAGE_KERNEL);
-	mm->context.pinned = 0;
+	ClearPagePinned(virt_to_page(mm->pgd));
 	spin_lock(&mm_unpinned_lock);
 	list_add(&mm->context.unpinned, &mm_unpinned);
 	spin_unlock(&mm_unpinned_lock);
@@ -217,7 +217,7 @@ void mm_pin_all(void)
 
 void arch_dup_mmap(struct mm_struct *oldmm, struct mm_struct *mm)
 {
-	if (!mm->context.pinned)
+	if (!PagePinned(virt_to_page(mm->pgd)))
 		mm_pin(mm);
 }
 
@@ -243,8 +243,9 @@ void arch_exit_mmap(struct mm_struct *mm
 
 	task_unlock(tsk);
 
-	if ( mm->context.pinned && (atomic_read(&mm->mm_count) == 1) &&
-	     !mm->context.has_foreign_mappings )
+	if (PagePinned(virt_to_page(mm->pgd))
+	    && (atomic_read(&mm->mm_count) == 1)
+	    && !mm->context.has_foreign_mappings)
 		mm_unpin(mm);
 }
 
@@ -343,14 +344,13 @@ static void flush_kernel_map(void *arg)
 	struct page *pg;
 
 	/* When clflush is available always use it because it is
-	   much cheaper than WBINVD. Disable clflush for now because
-	   the high level code is not ready yet */
+	   much cheaper than WBINVD. */
+	/* clflush is still broken. Disable for now. */
 	if (1 || !cpu_has_clflush)
 		asm volatile("wbinvd" ::: "memory");
 	else list_for_each_entry(pg, l, lru) {
 		void *adr = page_address(pg);
-		if (cpu_has_clflush)
-			cache_flush_page(adr);
+		cache_flush_page(adr);
 	}
 	__flush_tlb_all();
 }
@@ -364,7 +364,8 @@ static LIST_HEAD(deferred_pages); /* pro
 
 static inline void save_page(struct page *fpage)
 {
-	list_add(&fpage->lru, &deferred_pages);
+	if (!test_and_set_bit(PG_arch_1, &fpage->flags))
+		list_add(&fpage->lru, &deferred_pages);
 }
 
 /* 
@@ -398,9 +399,12 @@ __change_page_attr(unsigned long address
 	pte_t *kpte; 
 	struct page *kpte_page;
 	pgprot_t ref_prot2;
+
 	kpte = lookup_address(address);
 	if (!kpte) return 0;
 	kpte_page = virt_to_page(((unsigned long)kpte) & PAGE_MASK);
+	BUG_ON(PageLRU(kpte_page));
+	BUG_ON(PageCompound(kpte_page));
 	if (pgprot_val(prot) != pgprot_val(ref_prot)) { 
 		if (!pte_huge(*kpte)) {
 			set_pte(kpte, pfn_pte(pfn, prot));
@@ -439,10 +443,9 @@ __change_page_attr(unsigned long address
 		return 0;
 #endif
 
-	if (page_private(kpte_page) == 0) {
-		save_page(kpte_page);
+	save_page(kpte_page);
+	if (page_private(kpte_page) == 0)
 		revert_page(address, ref_prot);
-	}
 	return 0;
 } 
 
@@ -514,6 +517,10 @@ void global_flush_tlb(void)
 	flush_map(&l);
 
 	list_for_each_entry_safe(pg, next, &l, lru) {
+		list_del(&pg->lru);
+		clear_bit(PG_arch_1, &pg->flags);
+		if (page_private(pg) != 0)
+			continue;
 		ClearPagePrivate(pg);
 		__free_page(pg);
 	} 
--- head-2011-03-17.orig/arch/x86/oprofile/xenoprof.c	2008-01-28 12:24:19.000000000 +0100
+++ head-2011-03-17/arch/x86/oprofile/xenoprof.c	2011-01-31 17:49:31.000000000 +0100
@@ -18,9 +18,9 @@
 #include <linux/init.h>
 #include <linux/oprofile.h>
 #include <linux/sched.h>
+#include <linux/vmalloc.h>
 #include <asm/pgtable.h>
 
-#include <xen/driver_util.h>
 #include <xen/interface/xen.h>
 #include <xen/interface/xenoprof.h>
 #include <xen/xenoprof.h>
--- head-2011-03-17.orig/arch/x86/vdso/vdso32/note.S	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/arch/x86/vdso/vdso32/note.S	2011-01-31 17:49:31.000000000 +0100
@@ -13,7 +13,7 @@ ELFNOTE_START(Linux, 0, "a")
 	.long LINUX_VERSION_CODE
 ELFNOTE_END
 
-#ifdef CONFIG_XEN
+#if defined(CONFIG_X86_XEN) || defined(CONFIG_PARAVIRT_XEN)
 /*
  * Add a special note telling glibc's dynamic linker a fake hardware
  * flavor that it will use to choose the search path for libraries in the
@@ -37,8 +37,12 @@ ELFNOTE_END
 
 ELFNOTE_START(GNU, 2, "a")
 	.long 1			/* ncaps */
+#ifdef CONFIG_PARAVIRT_XEN
 VDSO32_NOTE_MASK:		/* Symbol used by arch/x86/xen/setup.c */
 	.long 0			/* mask */
+#else
+	.long 1 << VDSO_NOTE_NONEGSEG_BIT /* mask */
+#endif
 	.byte VDSO_NOTE_NONEGSEG_BIT; .asciz "nosegneg"	/* bit, name */
 ELFNOTE_END
 #endif
--- head-2011-03-17.orig/drivers/Makefile	2011-01-31 14:53:38.000000000 +0100
+++ head-2011-03-17/drivers/Makefile	2011-01-31 17:49:31.000000000 +0100
@@ -19,7 +19,7 @@ obj-$(CONFIG_PNP)		+= pnp/
 obj-$(CONFIG_ARM_AMBA)		+= amba/
 
 obj-$(CONFIG_VIRTIO)		+= virtio/
-obj-$(CONFIG_XEN)		+= xen/
+obj-$(CONFIG_PARAVIRT_XEN)	+= xen/
 
 # regulators early, since some subsystems rely on them to initialize
 obj-$(CONFIG_REGULATOR)		+= regulator/
--- head-2011-03-17.orig/drivers/block/Kconfig	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/drivers/block/Kconfig	2011-01-31 17:49:31.000000000 +0100
@@ -466,9 +466,9 @@ config XILINX_SYSACE
 	help
 	  Include support for the Xilinx SystemACE CompactFlash interface
 
-config XEN_BLKDEV_FRONTEND
+config PARAVIRT_XEN_BLKDEV_FRONTEND
 	tristate "Xen virtual block device support"
-	depends on XEN
+	depends on PARAVIRT_XEN
 	default y
 	select XEN_XENBUS_FRONTEND
 	help
--- head-2011-03-17.orig/drivers/block/Makefile	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/drivers/block/Makefile	2011-01-31 17:49:31.000000000 +0100
@@ -35,7 +35,7 @@ obj-$(CONFIG_BLK_DEV_SX8)	+= sx8.o
 obj-$(CONFIG_BLK_DEV_UB)	+= ub.o
 obj-$(CONFIG_BLK_DEV_HD)	+= hd.o
 
-obj-$(CONFIG_XEN_BLKDEV_FRONTEND)	+= xen-blkfront.o
+obj-$(CONFIG_PARAVIRT_XEN_BLKDEV_FRONTEND) += xen-blkfront.o
 obj-$(CONFIG_BLK_DEV_DRBD)     += drbd/
 obj-$(CONFIG_BLK_DEV_RBD)     += rbd.o
 
--- head-2011-03-17.orig/drivers/block/xen-blkfront.c	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/drivers/block/xen-blkfront.c	2011-01-31 17:49:31.000000000 +0100
@@ -1282,7 +1282,6 @@ static const struct xenbus_device_id blk
 
 static struct xenbus_driver blkfront = {
 	.name = "vbd",
-	.owner = THIS_MODULE,
 	.ids = blkfront_ids,
 	.probe = blkfront_probe,
 	.remove = blkfront_remove,
--- head-2011-03-17.orig/drivers/char/Kconfig	2011-01-31 14:42:03.000000000 +0100
+++ head-2011-03-17/drivers/char/Kconfig	2011-01-31 17:49:31.000000000 +0100
@@ -669,7 +669,7 @@ config HVC_IUCV
 
 config HVC_XEN
 	bool "Xen Hypervisor Console support"
-	depends on XEN
+	depends on PARAVIRT_XEN
 	select HVC_DRIVER
 	select HVC_IRQ
 	default y
--- head-2011-03-17.orig/drivers/net/Kconfig	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/drivers/net/Kconfig	2011-01-31 17:49:31.000000000 +0100
@@ -2960,9 +2960,9 @@ config TILE_NET
 	  To compile this driver as a module, choose M here: the module
 	  will be called tile_net.
 
-config XEN_NETDEV_FRONTEND
+config PARAVIRT_XEN_NETDEV_FRONTEND
 	tristate "Xen network device frontend driver"
-	depends on XEN
+	depends on PARAVIRT_XEN
 	select XEN_XENBUS_FRONTEND
 	default y
 	help
--- head-2011-03-17.orig/drivers/net/Makefile	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/drivers/net/Makefile	2011-01-31 17:49:31.000000000 +0100
@@ -170,7 +170,7 @@ obj-$(CONFIG_PPTP) += pppox.o pptp.o
 obj-$(CONFIG_SLIP) += slip.o
 obj-$(CONFIG_SLHC) += slhc.o
 
-obj-$(CONFIG_XEN_NETDEV_FRONTEND) += xen-netfront.o
+obj-$(CONFIG_PARAVIRT_XEN_NETDEV_FRONTEND) += xen-netfront.o
 
 obj-$(CONFIG_DUMMY) += dummy.o
 obj-$(CONFIG_IFB) += ifb.o
--- head-2011-03-17.orig/drivers/net/xen-netfront.c	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/drivers/net/xen-netfront.c	2011-02-17 10:10:21.000000000 +0100
@@ -1878,7 +1878,6 @@ static int __devexit xennet_remove(struc
 
 static struct xenbus_driver netfront_driver = {
 	.name = "vif",
-	.owner = THIS_MODULE,
 	.ids = netfront_ids,
 	.probe = netfront_probe,
 	.remove = __devexit_p(xennet_remove),
--- head-2011-03-17.orig/drivers/xen/Kconfig	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/Kconfig	2011-01-31 17:49:31.000000000 +0100
@@ -23,6 +23,9 @@ config XEN_PRIVILEGED_GUEST
 config XEN_UNPRIVILEGED_GUEST
 	def_bool !XEN_PRIVILEGED_GUEST
 	select PM
+	select PM_SLEEP
+	select PM_SLEEP_SMP if SMP
+	select SUSPEND
 
 config XEN_PRIVCMD
 	def_bool y
--- head-2011-03-17.orig/drivers/xen/Makefile	2011-02-24 13:56:24.000000000 +0100
+++ head-2011-03-17/drivers/xen/Makefile	2011-01-31 17:49:31.000000000 +0100
@@ -1,10 +1,14 @@
-obj-y	+= core/
-obj-y	+= console/
-obj-y	+= evtchn/
-obj-y	+= xenbus/
-obj-y	+= char/
+obj-$(CONFIG_PARAVIRT_XEN)	+= grant-table.o
 
-obj-y	+= util.o
+obj-$(CONFIG_XEN)		+= core/
+obj-$(CONFIG_XEN)		+= console/
+obj-$(CONFIG_XEN)		+= evtchn/
+obj-y				+= xenbus/
+obj-$(CONFIG_XEN)		+= char/
+
+xen-backend-$(CONFIG_XEN_BACKEND)	:= util.o
+
+obj-$(CONFIG_XEN)			+= $(xen-backend-y) $(xen-backend-m)
 obj-$(CONFIG_XEN_BALLOON)		+= balloon/
 obj-$(CONFIG_XEN_BLKDEV_BACKEND)	+= blkback/
 obj-$(CONFIG_XEN_BLKDEV_TAP)		+= blktap/
--- head-2011-03-17.orig/drivers/xen/balloon/balloon.c	2011-01-31 17:32:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/balloon/balloon.c	2011-01-31 17:49:31.000000000 +0100
@@ -324,13 +324,9 @@ static int increase_reservation(unsigned
 
 #ifndef MODULE
 	setup_per_zone_pages_min();
-# if defined(CONFIG_MEMORY_HOTPLUG) || defined(CONFIG_ACPI_HOTPLUG_MEMORY) \
-     || defined(CONFIG_ACPI_HOTPLUG_MEMORY_MODULE)
-	 /* build_all_zonelists() is __meminit */
 	if (need_zonelists_rebuild)
 		build_all_zonelists();
 	else
-# endif
 		vm_total_pages = nr_free_pagecache_pages();
 #endif
 
--- head-2011-03-17.orig/drivers/xen/blkback/blkback.c	2011-01-31 17:32:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/blkback/blkback.c	2011-01-31 17:49:31.000000000 +0100
@@ -156,7 +156,7 @@ static void unplug_queue(blkif_t *blkif)
 
 static void plug_queue(blkif_t *blkif, struct block_device *bdev)
 {
-	request_queue_t *q = bdev_get_queue(bdev);
+	struct request_queue *q = bdev_get_queue(bdev);
 
 	if (q == blkif->plug)
 		return;
--- head-2011-03-17.orig/drivers/xen/blkback/common.h	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/blkback/common.h	2011-01-31 17:49:31.000000000 +0100
@@ -41,7 +41,6 @@
 #include <asm/hypervisor.h>
 #include <xen/blkif.h>
 #include <xen/gnttab.h>
-#include <xen/driver_util.h>
 #include <xen/xenbus.h>
 #include "blkback-pagemap.h"
 
@@ -82,7 +81,7 @@ typedef struct blkif_st {
 	wait_queue_head_t   wq;
 	struct task_struct  *xenblkd;
 	unsigned int        waiting_reqs;
-	request_queue_t     *plug;
+	struct request_queue *plug;
 
 	/* statistics */
 	unsigned long       st_print;
--- head-2011-03-17.orig/drivers/xen/blkback/interface.c	2011-01-31 17:32:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/blkback/interface.c	2011-01-31 17:49:31.000000000 +0100
@@ -178,5 +178,5 @@ void blkif_free(blkif_t *blkif)
 void __init blkif_interface_init(void)
 {
 	blkif_cachep = kmem_cache_create("blkif_cache", sizeof(blkif_t), 
-					 0, 0, NULL, NULL);
+					 0, 0, NULL);
 }
--- head-2011-03-17.orig/drivers/xen/blkback/xenbus.c	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/drivers/xen/blkback/xenbus.c	2011-01-31 17:49:31.000000000 +0100
@@ -27,8 +27,6 @@
 	pr_debug("blkback/xenbus (%s:%d) " fmt ".\n",	\
 		 __FUNCTION__, __LINE__, ##args)
 
-static DEFINE_RWLOCK(sysfs_read_lock);
-
 static void connect(struct backend_info *);
 static int connect_ring(struct backend_info *);
 static void backend_changed(struct xenbus_watch *, const char **,
@@ -110,10 +108,8 @@ static void update_blkif_status(blkif_t 
 		if (!get_device(_dev))					\
 			return ret;					\
 		dev = to_xenbus_device(_dev);				\
-		read_lock(&sysfs_read_lock);				\
 		if ((be = dev->dev.driver_data) != NULL)		\
 			ret = sprintf(buf, format, ##args);		\
-		read_unlock(&sysfs_read_lock);				\
 		put_device(_dev);					\
 		return ret;						\
 	}								\
@@ -181,7 +177,6 @@ static int blkback_remove(struct xenbus_
 
 	DPRINTK("");
 
-	write_lock(&sysfs_read_lock);
 	if (be->major || be->minor)
 		xenvbd_sysfs_delif(dev);
 
@@ -200,7 +195,6 @@ static int blkback_remove(struct xenbus_
 
 	kfree(be);
 	dev->dev.driver_data = NULL;
-	write_unlock(&sysfs_read_lock);
 	return 0;
 }
 
--- head-2011-03-17.orig/drivers/xen/blkfront/blkfront.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/drivers/xen/blkfront/blkfront.c	2011-01-31 17:49:31.000000000 +0100
@@ -574,14 +574,20 @@ int blkif_ioctl(struct inode *inode, str
 		return -EINVAL;
 	}
 	default:
-		if (info->mi && info->gd) {
+		if (info->mi && info->gd && info->rq) {
 			switch (info->mi->major) {
 			case SCSI_DISK0_MAJOR:
 			case SCSI_DISK1_MAJOR ... SCSI_DISK7_MAJOR:
 		        case SCSI_DISK8_MAJOR ... SCSI_DISK15_MAJOR:
 		        case SCSI_CDROM_MAJOR:
+#if LINUX_VERSION_CODE < KERNEL_VERSION(2,6,23)
 				return scsi_cmd_ioctl(filep, info->gd, command,
 						      (void __user *)argument);
+#else
+				return scsi_cmd_ioctl(filep, info->rq,
+						      info->gd, command,
+						      (void __user *)argument);
+#endif
 			}
 		}
 
@@ -698,7 +704,7 @@ static int blkif_queue_request(struct re
  * do_blkif_request
  *  read a block; request is in a request queue
  */
-void do_blkif_request(request_queue_t *rq)
+void do_blkif_request(struct request_queue *rq)
 {
 	struct blkfront_info *info = NULL;
 	struct request *req;
--- head-2011-03-17.orig/drivers/xen/blkfront/block.h	2010-02-24 13:13:46.000000000 +0100
+++ head-2011-03-17/drivers/xen/blkfront/block.h	2011-01-31 17:49:31.000000000 +0100
@@ -107,7 +107,7 @@ struct blkfront_info
 	struct scatterlist sg[BLKIF_MAX_SEGMENTS_PER_REQUEST];
 	unsigned int irq;
 	struct xlbd_major_info *mi;
-	request_queue_t *rq;
+	struct request_queue *rq;
 	struct work_struct work;
 	struct gnttab_free_callback callback;
 	struct blk_shadow shadow[BLK_RING_SIZE];
@@ -131,7 +131,7 @@ extern int blkif_ioctl(struct inode *ino
 extern int blkif_getgeo(struct block_device *, struct hd_geometry *);
 extern int blkif_check(dev_t dev);
 extern int blkif_revalidate(dev_t dev);
-extern void do_blkif_request (request_queue_t *rq);
+extern void do_blkif_request (struct request_queue *rq);
 
 /* Virtual block-device subsystem. */
 /* Note that xlvbd_add doesn't call add_disk for you: you're expected
--- head-2011-03-17.orig/drivers/xen/blkfront/vbd.c	2010-01-18 15:23:12.000000000 +0100
+++ head-2011-03-17/drivers/xen/blkfront/vbd.c	2011-01-31 17:49:31.000000000 +0100
@@ -298,7 +298,7 @@ xlbd_release_minors(struct xlbd_major_in
 static int
 xlvbd_init_blk_queue(struct gendisk *gd, u16 sector_size)
 {
-	request_queue_t *rq;
+	struct request_queue *rq;
 
 	rq = blk_init_queue(do_blkif_request, &blkif_io_lock);
 	if (rq == NULL)
--- head-2011-03-17.orig/drivers/xen/blktap/common.h	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/blktap/common.h	2011-01-31 17:49:31.000000000 +0100
@@ -40,7 +40,6 @@
 #include <asm/hypervisor.h>
 #include <xen/blkif.h>
 #include <xen/gnttab.h>
-#include <xen/driver_util.h>
 
 #define DPRINTK(_f, _a...) pr_debug("(file=%s, line=%d) " _f, \
                                     __FILE__ , __LINE__ , ## _a )
@@ -68,7 +67,7 @@ typedef struct blkif_st {
 	wait_queue_head_t   wq;
 	struct task_struct  *xenblkd;
 	unsigned int        waiting_reqs;
-	request_queue_t     *plug;
+	struct request_queue *plug;
 
 	/* statistics */
 	unsigned long       st_print;
--- head-2011-03-17.orig/drivers/xen/blktap/interface.c	2011-01-31 17:32:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/blktap/interface.c	2011-01-31 17:49:31.000000000 +0100
@@ -178,5 +178,5 @@ void tap_blkif_kmem_cache_free(blkif_t *
 void __init tap_blkif_interface_init(void)
 {
 	blkif_cachep = kmem_cache_create("blktapif_cache", sizeof(blkif_t), 
-					 0, 0, NULL, NULL);
+					 0, 0, NULL);
 }
--- head-2011-03-17.orig/drivers/xen/blktap/xenbus.c	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/drivers/xen/blktap/xenbus.c	2011-01-31 17:49:31.000000000 +0100
@@ -50,8 +50,6 @@ struct backend_info
 	int group_added;
 };
 
-static DEFINE_RWLOCK(sysfs_read_lock);
-
 static void connect(struct backend_info *);
 static int connect_ring(struct backend_info *);
 static int blktap_remove(struct xenbus_device *dev);
@@ -130,10 +128,8 @@ static int blktap_name(blkif_t *blkif, c
 		if (!get_device(_dev))					\
 			return ret;					\
 		dev = to_xenbus_device(_dev);				\
-		read_lock(&sysfs_read_lock);				\
 		if ((be = dev->dev.driver_data) != NULL)		\
 			ret = sprintf(buf, format, ##args);		\
-		read_unlock(&sysfs_read_lock);				\
 		put_device(_dev);					\
 		return ret;						\
 	}								\
@@ -180,7 +176,6 @@ static int blktap_remove(struct xenbus_d
 {
 	struct backend_info *be = dev->dev.driver_data;
 
-	write_lock(&sysfs_read_lock);
 	if (be->group_added)
 		xentap_sysfs_delif(be->dev);
 	if (be->backend_watch.node) {
@@ -198,7 +193,6 @@ static int blktap_remove(struct xenbus_d
 	}
 	kfree(be);
 	dev->dev.driver_data = NULL;
-	write_unlock(&sysfs_read_lock);
 	return 0;
 }
 
--- head-2011-03-17.orig/drivers/xen/blktap2/blktap.h	2010-02-24 13:13:46.000000000 +0100
+++ head-2011-03-17/drivers/xen/blktap2/blktap.h	2011-01-31 17:49:31.000000000 +0100
@@ -203,6 +203,7 @@ blktap_validate_params(struct blktap *ta
 }
 
 int blktap_control_destroy_device(struct blktap *);
+int blktap_control_finish_destroy(struct blktap *);
 
 int blktap_ring_init(int *);
 int blktap_ring_free(void);
--- head-2011-03-17.orig/drivers/xen/blktap2/control.c	2011-02-24 15:15:38.000000000 +0100
+++ head-2011-03-17/drivers/xen/blktap2/control.c	2011-01-31 17:49:31.000000000 +0100
@@ -194,14 +194,20 @@ blktap_control_destroy_device(struct blk
 
 	clear_bit(BLKTAP_SHUTDOWN_REQUESTED, &tap->dev_inuse);
 
-	if (tap->dev_inuse == (1UL << BLKTAP_CONTROL)) {
+	if (blktap_control_finish_destroy(tap))
 		err = 0;
-		clear_bit(BLKTAP_CONTROL, &tap->dev_inuse);
-	}
 
 	return err;
 }
 
+int
+blktap_control_finish_destroy(struct blktap *tap)
+{
+	if (tap->dev_inuse == (1UL << BLKTAP_CONTROL))
+		clear_bit(BLKTAP_CONTROL, &tap->dev_inuse);
+	return !tap->dev_inuse;
+}
+
 static int __init
 blktap_control_init(void)
 {
--- head-2011-03-17.orig/drivers/xen/blktap2/device.c	2010-11-25 09:36:37.000000000 +0100
+++ head-2011-03-17/drivers/xen/blktap2/device.c	2011-01-31 17:49:31.000000000 +0100
@@ -833,7 +833,7 @@ static void
 blktap_device_run_queue(struct blktap *tap)
 {
 	int queued, err;
-	request_queue_t *rq;
+	struct request_queue *rq;
 	struct request *req;
 	struct blktap_ring *ring;
 	struct blktap_device *dev;
@@ -910,7 +910,7 @@ blktap_device_run_queue(struct blktap *t
  * dev->lock held on entry
  */
 static void
-blktap_device_do_request(request_queue_t *rq)
+blktap_device_do_request(struct request_queue *rq)
 {
 	struct request *req;
 	struct blktap *tap;
@@ -1186,6 +1186,5 @@ void
 blktap_device_free(void)
 {
 	if (blktap_device_major)
-		if (unregister_blkdev(blktap_device_major, "tapdev"))
-			BTERR("blktap device unregister failed\n");
+		unregister_blkdev(blktap_device_major, "tapdev");
 }
--- head-2011-03-17.orig/drivers/xen/blktap2/sysfs.c	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/blktap2/sysfs.c	2011-01-31 17:49:31.000000000 +0100
@@ -334,6 +334,24 @@ blktap_sysfs_create(struct blktap *tap)
 	return err;
 }
 
+static void
+_blktap_sysfs_destroy(struct device *_dev)
+{
+	struct class_device *dev = _dev->???;
+	struct blktap *tap = dev->class_data;
+
+	class_device_remove_file(dev, &class_device_attr_name);
+	class_device_remove_file(dev, &class_device_attr_remove);
+	class_device_remove_file(dev, &class_device_attr_pause);
+	class_device_remove_file(dev, &class_device_attr_resume);
+	class_device_remove_file(dev, &class_device_attr_debug);
+	class_device_unregister(dev);
+
+	clear_bit(BLKTAP_SYSFS, &tap->dev_inuse);
+
+	blktap_control_finish_destroy(tap);
+}
+
 int
 blktap_sysfs_destroy(struct blktap *tap)
 {
@@ -350,17 +368,7 @@ blktap_sysfs_destroy(struct blktap *tap)
 				     !atomic_read(&tap->ring.sysfs_refcnt)))
 		return -EAGAIN;
 
-	/* XXX: is it safe to remove the class from a sysfs attribute? */
-	class_device_remove_file(dev, &class_device_attr_name);
-	class_device_remove_file(dev, &class_device_attr_remove);
-	class_device_remove_file(dev, &class_device_attr_pause);
-	class_device_remove_file(dev, &class_device_attr_resume);
-	class_device_remove_file(dev, &class_device_attr_debug);
-	class_device_destroy(class, ring->devno);
-
-	clear_bit(BLKTAP_SYSFS, &tap->dev_inuse);
-
-	return 0;
+	return device_schedule_callback(dev->???, _blktap_sysfs_destroy);
 }
 
 static ssize_t
--- head-2011-03-17.orig/drivers/xen/core/gnttab.c	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/core/gnttab.c	2011-01-31 17:49:31.000000000 +0100
@@ -42,7 +42,6 @@
 #include <asm/synch_bitops.h>
 #include <asm/io.h>
 #include <xen/interface/memory.h>
-#include <xen/driver_util.h>
 #include <asm/gnttab_dma.h>
 
 #ifdef HAVE_XEN_PLATFORM_COMPAT_H
--- head-2011-03-17.orig/drivers/xen/core/reboot.c	2011-01-31 17:32:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/core/reboot.c	2011-01-31 17:49:31.000000000 +0100
@@ -3,6 +3,7 @@
 #include <linux/unistd.h>
 #include <linux/module.h>
 #include <linux/reboot.h>
+#include <linux/sched.h>
 #include <linux/sysrq.h>
 #include <asm/hypervisor.h>
 #include <xen/xenbus.h>
--- head-2011-03-17.orig/drivers/xen/netback/common.h	2011-02-17 10:09:57.000000000 +0100
+++ head-2011-03-17/drivers/xen/netback/common.h	2011-01-31 17:49:31.000000000 +0100
@@ -44,7 +44,6 @@
 #include <asm/pgalloc.h>
 #include <xen/interface/grant_table.h>
 #include <xen/gnttab.h>
-#include <xen/driver_util.h>
 #include <xen/xenbus.h>
 
 #define DPRINTK(_f, _a...)			\
--- head-2011-03-17.orig/drivers/xen/scsiback/common.h	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/scsiback/common.h	2011-01-31 17:49:31.000000000 +0100
@@ -55,7 +55,6 @@
 #include <xen/evtchn.h>
 #include <asm/hypervisor.h>
 #include <xen/gnttab.h>
-#include <xen/driver_util.h>
 #include <xen/xenbus.h>
 #include <xen/interface/io/ring.h>
 #include <xen/interface/grant_table.h>
--- head-2011-03-17.orig/drivers/xen/scsiback/interface.c	2011-01-31 17:32:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/scsiback/interface.c	2011-01-31 17:49:31.000000000 +0100
@@ -166,7 +166,7 @@ void scsiback_free(struct vscsibk_info *
 int __init scsiback_interface_init(void)
 {
 	scsiback_cachep = kmem_cache_create("vscsiif_cache",
-		sizeof(struct vscsibk_info), 0, 0, NULL, NULL);
+		sizeof(struct vscsibk_info), 0, 0, NULL);
 	if (!scsiback_cachep) {
 		printk(KERN_ERR "scsiback: can't init scsi cache\n");
 		return -ENOMEM;
--- head-2011-03-17.orig/drivers/xen/scsifront/scsifront.c	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/scsifront/scsifront.c	2011-02-08 10:03:55.000000000 +0100
@@ -147,7 +147,7 @@ static void scsifront_cdb_cmd_done(struc
 	add_id_to_freelist(info, id);
 
 	sc->result = ring_res->rslt;
-	sc->resid  = ring_res->residual_len;
+	scsi_set_resid(sc, ring_res->residual_len);
 
 	if (ring_res->sense_len > VSCSIIF_SENSE_BUFFERSIZE)
 		sense_len = VSCSIIF_SENSE_BUFFERSIZE;
@@ -351,8 +351,7 @@ big_to_sg:
 static int scsifront_queuecommand(struct scsi_cmnd *sc,
 				  void (*done)(struct scsi_cmnd *))
 {
-	struct vscsifrnt_info *info =
-		(struct vscsifrnt_info *) sc->device->host->hostdata;
+	struct vscsifrnt_info *info = shost_priv(sc->device->host);
 	vscsiif_request_t *ring_req;
 	int ref_cnt;
 	uint16_t rqid;
@@ -428,8 +427,7 @@ static int scsifront_eh_abort_handler(st
 static int scsifront_dev_reset_handler(struct scsi_cmnd *sc)
 {
 	struct Scsi_Host *host = sc->device->host;
-	struct vscsifrnt_info *info =
-		(struct vscsifrnt_info *) sc->device->host->hostdata;
+	struct vscsifrnt_info *info = shost_priv(host);
 
 	vscsiif_request_t *ring_req;
 	uint16_t rqid;
--- head-2011-03-17.orig/drivers/xen/sfc_netback/accel_solarflare.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/drivers/xen/sfc_netback/accel_solarflare.c	2011-01-31 17:49:31.000000000 +0100
@@ -37,7 +37,6 @@
 #include "ci/efhw/public.h"
 
 #include <xen/evtchn.h>
-#include <xen/driver_util.h>
 #include <linux/list.h>
 #include <linux/mutex.h>
 
--- head-2011-03-17.orig/drivers/xen/sfc_netutil/accel_util.c	2010-09-23 15:39:04.000000000 +0200
+++ head-2011-03-17/drivers/xen/sfc_netutil/accel_util.c	2011-01-31 17:49:31.000000000 +0100
@@ -28,7 +28,6 @@
 #include <asm/pgtable.h>
 #include <asm/hypercall.h>
 #include <xen/xenbus.h>
-#include <xen/driver_util.h>
 #include <xen/gnttab.h>
 
 #include "accel_util.h"
--- head-2011-03-17.orig/drivers/xen/tpmback/common.h	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/drivers/xen/tpmback/common.h	2011-01-31 17:49:31.000000000 +0100
@@ -10,7 +10,6 @@
 #include <linux/interrupt.h>
 #include <linux/slab.h>
 #include <xen/evtchn.h>
-#include <xen/driver_util.h>
 #include <xen/interface/grant_table.h>
 #include <xen/interface/io/tpmif.h>
 #include <asm/io.h>
--- head-2011-03-17.orig/drivers/xen/tpmback/interface.c	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/drivers/xen/tpmback/interface.c	2011-01-31 17:49:31.000000000 +0100
@@ -13,6 +13,7 @@
 
 #include "common.h"
 #include <linux/delay.h>
+#include <linux/err.h>
 #include <xen/balloon.h>
 #include <xen/gnttab.h>
 
@@ -160,7 +161,7 @@ void tpmif_disconnect_complete(tpmif_t *
 int __init tpmif_interface_init(void)
 {
 	tpmif_cachep = kmem_cache_create("tpmif_cache", sizeof (tpmif_t),
-					 0, 0, NULL, NULL);
+					 0, 0, NULL);
 	return tpmif_cachep ? 0 : -ENOMEM;
 }
 
--- head-2011-03-17.orig/drivers/xen/usbback/usbback.h	2011-01-31 17:29:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/usbback/usbback.h	2011-01-31 17:49:31.000000000 +0100
@@ -57,7 +57,6 @@
 #include <linux/kref.h>
 #include <xen/evtchn.h>
 #include <xen/gnttab.h>
-#include <xen/driver_util.h>
 #include <xen/interface/xen.h>
 #include <xen/xenbus.h>
 #include <xen/interface/io/usbif.h>
--- head-2011-03-17.orig/drivers/xen/usbfront/xenbus.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/drivers/xen/usbfront/xenbus.c	2011-01-31 17:49:31.000000000 +0100
@@ -393,7 +393,7 @@ static int __init usbfront_init(void)
 		return -ENODEV;
 
 	xenhcd_urbp_cachep = kmem_cache_create("xenhcd_urb_priv",
-			sizeof(struct urb_priv), 0, 0, NULL, NULL);
+			sizeof(struct urb_priv), 0, 0, NULL);
 	if (!xenhcd_urbp_cachep) {
 		printk(KERN_ERR "usbfront failed to create kmem cache\n");
 		return -ENOMEM;
--- head-2011-03-17.orig/drivers/xen/util.c	2007-07-10 09:42:30.000000000 +0200
+++ head-2011-03-17/drivers/xen/util.c	2011-01-31 17:49:31.000000000 +0100
@@ -1,8 +1,5 @@
-#include <linux/mm.h>
+#include <linux/err.h>
 #include <linux/module.h>
-#include <linux/slab.h>
-#include <linux/vmalloc.h>
-#include <asm/uaccess.h>
 #include <xen/driver_util.h>
 
 struct class *get_xen_class(void)
@@ -21,45 +18,3 @@ struct class *get_xen_class(void)
 	return xen_class;
 }
 EXPORT_SYMBOL_GPL(get_xen_class);
-
-#ifdef CONFIG_X86
-static int f(pte_t *pte, struct page *pmd_page, unsigned long addr, void *data)
-{
-	/* apply_to_page_range() does all the hard work. */
-	return 0;
-}
-
-struct vm_struct *alloc_vm_area(unsigned long size)
-{
-	struct vm_struct *area;
-
-	area = get_vm_area(size, VM_IOREMAP);
-	if (area == NULL)
-		return NULL;
-
-	/*
-	 * This ensures that page tables are constructed for this region
-	 * of kernel virtual address space and mapped into init_mm.
-	 */
-	if (apply_to_page_range(&init_mm, (unsigned long)area->addr,
-				area->size, f, NULL)) {
-		free_vm_area(area);
-		return NULL;
-	}
-
-	/* Map page directories into every address space. */
-	vmalloc_sync_all();
-
-	return area;
-}
-EXPORT_SYMBOL_GPL(alloc_vm_area);
-
-void free_vm_area(struct vm_struct *area)
-{
-	struct vm_struct *ret;
-	ret = remove_vm_area(area->addr);
-	BUG_ON(ret != area);
-	kfree(area);
-}
-EXPORT_SYMBOL_GPL(free_vm_area);
-#endif /* CONFIG_X86 */
--- head-2011-03-17.orig/drivers/xen/xenbus/xenbus_backend_client.c	2010-09-23 15:39:04.000000000 +0200
+++ head-2011-03-17/drivers/xen/xenbus/xenbus_backend_client.c	2011-01-31 17:49:31.000000000 +0100
@@ -32,9 +32,9 @@
 
 #include <linux/err.h>
 #include <linux/delay.h>
+#include <linux/vmalloc.h>
 #include <xen/gnttab.h>
 #include <xen/xenbus.h>
-#include <xen/driver_util.h>
 
 /* Based on Rusty Russell's skeleton driver's map_page */
 struct vm_struct *xenbus_map_ring_valloc(struct xenbus_device *dev, int gnt_ref)
--- head-2011-03-17.orig/drivers/xen/xenbus/xenbus_client.c	2011-01-31 15:14:12.000000000 +0100
+++ head-2011-03-17/drivers/xen/xenbus/xenbus_client.c	2011-01-31 17:49:31.000000000 +0100
@@ -30,19 +30,25 @@
  * IN THE SOFTWARE.
  */
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 #include <linux/slab.h>
 #include <xen/evtchn.h>
 #include <xen/gnttab.h>
+#else
+#include <linux/types.h>
+#include <linux/vmalloc.h>
+#include <asm/xen/hypervisor.h>
+#include <xen/interface/xen.h>
+#include <xen/interface/event_channel.h>
+#include <xen/events.h>
+#include <xen/grant_table.h>
+#endif
 #include <xen/xenbus.h>
-#include <xen/driver_util.h>
 
 #ifdef HAVE_XEN_PLATFORM_COMPAT_H
 #include <xen/platform-compat.h>
 #endif
 
-#define DPRINTK(fmt, args...) \
-    pr_debug("xenbus_client (%s:%d) " fmt ".\n", __FUNCTION__, __LINE__, ##args)
-
 const char *xenbus_strstate(enum xenbus_state state)
 {
 	static const char *const name[] = {
@@ -60,6 +66,20 @@ const char *xenbus_strstate(enum xenbus_
 }
 EXPORT_SYMBOL_GPL(xenbus_strstate);
 
+/**
+ * xenbus_watch_path - register a watch
+ * @dev: xenbus device
+ * @path: path to watch
+ * @watch: watch to register
+ * @callback: callback to register
+ *
+ * Register a @watch on the given path, using the given xenbus_watch structure
+ * for storage, and the given @callback function as the callback.  Return 0 on
+ * success, or -errno on error.  On success, the given @path will be saved as
+ * @watch->node, and remains the caller's to free.  On error, @watch->node will
+ * be NULL, the device will switch to %XenbusStateClosing, and the error will
+ * be saved in the store.
+ */
 int xenbus_watch_path(struct xenbus_device *dev, const char *path,
 		      struct xenbus_watch *watch,
 		      void (*callback)(struct xenbus_watch *,
@@ -83,6 +103,7 @@ int xenbus_watch_path(struct xenbus_devi
 EXPORT_SYMBOL_GPL(xenbus_watch_path);
 
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 int xenbus_watch_path2(struct xenbus_device *dev, const char *path,
 		       const char *path2, struct xenbus_watch *watch,
 		       void (*callback)(struct xenbus_watch *,
@@ -101,8 +122,60 @@ int xenbus_watch_path2(struct xenbus_dev
 	return err;
 }
 EXPORT_SYMBOL_GPL(xenbus_watch_path2);
+#else
+/**
+ * xenbus_watch_pathfmt - register a watch on a sprintf-formatted path
+ * @dev: xenbus device
+ * @watch: watch to register
+ * @callback: callback to register
+ * @pathfmt: format of path to watch
+ *
+ * Register a watch on the given @path, using the given xenbus_watch
+ * structure for storage, and the given @callback function as the callback.
+ * Return 0 on success, or -errno on error.  On success, the watched path
+ * (@path/@path2) will be saved as @watch->node, and becomes the caller's to
+ * kfree().  On error, watch->node will be NULL, so the caller has nothing to
+ * free, the device will switch to %XenbusStateClosing, and the error will be
+ * saved in the store.
+ */
+int xenbus_watch_pathfmt(struct xenbus_device *dev,
+			 struct xenbus_watch *watch,
+			 void (*callback)(struct xenbus_watch *,
+					const char **, unsigned int),
+			 const char *pathfmt, ...)
+{
+	int err;
+	va_list ap;
+	char *path;
+
+	va_start(ap, pathfmt);
+	path = kvasprintf(GFP_KERNEL, pathfmt, ap);
+	va_end(ap);
+
+	if (!path) {
+		xenbus_dev_fatal(dev, -ENOMEM, "allocating path for watch");
+		return -ENOMEM;
+	}
+	err = xenbus_watch_path(dev, path, watch, callback);
+
+	if (err)
+		kfree(path);
+	return err;
+}
+EXPORT_SYMBOL_GPL(xenbus_watch_pathfmt);
+#endif
 
 
+/**
+ * xenbus_switch_state
+ * @dev: xenbus device
+ * @xbt: transaction handle
+ * @state: new state
+ *
+ * Advertise in the store a change of the given driver to the given new_state.
+ * Return 0 on success, or -errno on error.  On error, the device will switch
+ * to XenbusStateClosing, and the error will be saved in the store.
+ */
 int xenbus_switch_state(struct xenbus_device *dev, enum xenbus_state state)
 {
 	/* We check whether the state is currently set to the given value, and
@@ -161,8 +234,8 @@ static char *error_path(struct xenbus_de
 }
 
 
-void _dev_error(struct xenbus_device *dev, int err, const char *fmt,
-		va_list ap)
+static void _dev_error(struct xenbus_device *dev, int err,
+			const char *fmt, va_list ap)
 {
 	int ret;
 	unsigned int len;
@@ -183,14 +256,16 @@ void _dev_error(struct xenbus_device *de
 	path_buffer = error_path(dev);
 
 	if (path_buffer == NULL) {
-		printk("xenbus: failed to write error node for %s (%s)\n",
-		       dev->nodename, printf_buffer);
+		dev_err(&dev->dev,
+		        "xenbus: failed to write error node for %s (%s)\n",
+		        dev->nodename, printf_buffer);
 		goto fail;
 	}
 
 	if (xenbus_write(XBT_NIL, path_buffer, "error", printf_buffer) != 0) {
-		printk("xenbus: failed to write error node for %s (%s)\n",
-		       dev->nodename, printf_buffer);
+		dev_err(&dev->dev,
+		        "xenbus: failed to write error node for %s (%s)\n",
+		        dev->nodename, printf_buffer);
 		goto fail;
 	}
 
@@ -200,6 +275,15 @@ fail:
 }
 
 
+/**
+ * xenbus_dev_error
+ * @dev: xenbus device
+ * @err: error to report
+ * @fmt: error message format
+ *
+ * Report the given negative errno into the store, along with the given
+ * formatted message.
+ */
 void xenbus_dev_error(struct xenbus_device *dev, int err, const char *fmt, ...)
 {
 	va_list ap;
@@ -211,6 +295,16 @@ void xenbus_dev_error(struct xenbus_devi
 EXPORT_SYMBOL_GPL(xenbus_dev_error);
 
 
+/**
+ * xenbus_dev_fatal
+ * @dev: xenbus device
+ * @err: error to report
+ * @fmt: error message format
+ *
+ * Equivalent to xenbus_dev_error(dev, err, fmt, args), followed by
+ * xenbus_switch_state(dev, NULL, XenbusStateClosing) to schedule an orderly
+ * closedown of this driver and its peer.
+ */
 void xenbus_dev_fatal(struct xenbus_device *dev, int err, const char *fmt, ...)
 {
 	va_list ap;
@@ -224,6 +318,15 @@ void xenbus_dev_fatal(struct xenbus_devi
 EXPORT_SYMBOL_GPL(xenbus_dev_fatal);
 
 
+/**
+ * xenbus_grant_ring
+ * @dev: xenbus device
+ * @ring_mfn: mfn of ring to grant
+ *
+ * Grant access to the given @ring_mfn to the peer of the given device.  Return
+ * 0 on success, or -errno on error.  On error, the device will switch to
+ * XenbusStateClosing, and the error will be saved in the store.
+ */
 int xenbus_grant_ring(struct xenbus_device *dev, unsigned long ring_mfn)
 {
 	int err = gnttab_grant_foreign_access(dev->otherend_id, ring_mfn, 0);
@@ -234,6 +337,12 @@ int xenbus_grant_ring(struct xenbus_devi
 EXPORT_SYMBOL_GPL(xenbus_grant_ring);
 
 
+/**
+ * Allocate an event channel for the given xenbus_device, assigning the newly
+ * created local port to *port.  Return 0 on success, or -errno on error.  On
+ * error, the device will switch to XenbusStateClosing, and the error will be
+ * saved in the store.
+ */
 int xenbus_alloc_evtchn(struct xenbus_device *dev, int *port)
 {
 	struct evtchn_alloc_unbound alloc_unbound;
@@ -254,6 +363,38 @@ int xenbus_alloc_evtchn(struct xenbus_de
 EXPORT_SYMBOL_GPL(xenbus_alloc_evtchn);
 
 
+#if 0 /* !defined(CONFIG_XEN) && !defined(MODULE) */
+/**
+ * Bind to an existing interdomain event channel in another domain. Returns 0
+ * on success and stores the local port in *port. On error, returns -errno,
+ * switches the device to XenbusStateClosing, and saves the error in XenStore.
+ */
+int xenbus_bind_evtchn(struct xenbus_device *dev, int remote_port, int *port)
+{
+	struct evtchn_bind_interdomain bind_interdomain;
+	int err;
+
+	bind_interdomain.remote_dom = dev->otherend_id;
+	bind_interdomain.remote_port = remote_port;
+
+	err = HYPERVISOR_event_channel_op(EVTCHNOP_bind_interdomain,
+					  &bind_interdomain);
+	if (err)
+		xenbus_dev_fatal(dev, err,
+				 "binding to event channel %d from domain %d",
+				 remote_port, dev->otherend_id);
+	else
+		*port = bind_interdomain.local_port;
+
+	return err;
+}
+EXPORT_SYMBOL_GPL(xenbus_bind_evtchn);
+#endif
+
+
+/**
+ * Free an existing event channel. Returns 0 on success or -errno on error.
+ */
 int xenbus_free_evtchn(struct xenbus_device *dev, int port)
 {
 	struct evtchn_close close;
@@ -270,6 +411,191 @@ int xenbus_free_evtchn(struct xenbus_dev
 EXPORT_SYMBOL_GPL(xenbus_free_evtchn);
 
 
+#if 0 /* !defined(CONFIG_XEN) && !defined(MODULE) */
+/**
+ * xenbus_map_ring_valloc
+ * @dev: xenbus device
+ * @gnt_ref: grant reference
+ * @vaddr: pointer to address to be filled out by mapping
+ *
+ * Based on Rusty Russell's skeleton driver's map_page.
+ * Map a page of memory into this domain from another domain's grant table.
+ * xenbus_map_ring_valloc allocates a page of virtual address space, maps the
+ * page to that address, and sets *vaddr to that address.
+ * Returns 0 on success, and GNTST_* (see xen/include/interface/grant_table.h)
+ * or -ENOMEM on error. If an error is returned, device will switch to
+ * XenbusStateClosing and the error message will be saved in XenStore.
+ */
+int xenbus_map_ring_valloc(struct xenbus_device *dev, int gnt_ref, void **vaddr)
+{
+	struct gnttab_map_grant_ref op = {
+		.flags = GNTMAP_host_map,
+		.ref   = gnt_ref,
+		.dom   = dev->otherend_id,
+	};
+	struct vm_struct *area;
+
+	*vaddr = NULL;
+
+	area = alloc_vm_area(PAGE_SIZE);
+	if (!area)
+		return -ENOMEM;
+
+	op.host_addr = (unsigned long)area->addr;
+
+	if (HYPERVISOR_grant_table_op(GNTTABOP_map_grant_ref, &op, 1))
+		BUG();
+
+	if (op.status != GNTST_okay) {
+		free_vm_area(area);
+		xenbus_dev_fatal(dev, op.status,
+				 "mapping in shared page %d from domain %d",
+				 gnt_ref, dev->otherend_id);
+		return op.status;
+	}
+
+	/* Stuff the handle in an unused field */
+	area->phys_addr = (unsigned long)op.handle;
+
+	*vaddr = area->addr;
+	return 0;
+}
+EXPORT_SYMBOL_GPL(xenbus_map_ring_valloc);
+
+
+/**
+ * xenbus_map_ring
+ * @dev: xenbus device
+ * @gnt_ref: grant reference
+ * @handle: pointer to grant handle to be filled
+ * @vaddr: address to be mapped to
+ *
+ * Map a page of memory into this domain from another domain's grant table.
+ * xenbus_map_ring does not allocate the virtual address space (you must do
+ * this yourself!). It only maps in the page to the specified address.
+ * Returns 0 on success, and GNTST_* (see xen/include/interface/grant_table.h)
+ * or -ENOMEM on error. If an error is returned, device will switch to
+ * XenbusStateClosing and the error message will be saved in XenStore.
+ */
+int xenbus_map_ring(struct xenbus_device *dev, int gnt_ref,
+		    grant_handle_t *handle, void *vaddr)
+{
+	struct gnttab_map_grant_ref op = {
+		.host_addr = (unsigned long)vaddr,
+		.flags     = GNTMAP_host_map,
+		.ref       = gnt_ref,
+		.dom       = dev->otherend_id,
+	};
+
+	if (HYPERVISOR_grant_table_op(GNTTABOP_map_grant_ref, &op, 1))
+		BUG();
+
+	if (op.status != GNTST_okay) {
+		xenbus_dev_fatal(dev, op.status,
+				 "mapping in shared page %d from domain %d",
+				 gnt_ref, dev->otherend_id);
+	} else
+		*handle = op.handle;
+
+	return op.status;
+}
+EXPORT_SYMBOL_GPL(xenbus_map_ring);
+
+
+/**
+ * xenbus_unmap_ring_vfree
+ * @dev: xenbus device
+ * @vaddr: addr to unmap
+ *
+ * Based on Rusty Russell's skeleton driver's unmap_page.
+ * Unmap a page of memory in this domain that was imported from another domain.
+ * Use xenbus_unmap_ring_vfree if you mapped in your memory with
+ * xenbus_map_ring_valloc (it will free the virtual address space).
+ * Returns 0 on success and returns GNTST_* on error
+ * (see xen/include/interface/grant_table.h).
+ */
+int xenbus_unmap_ring_vfree(struct xenbus_device *dev, void *vaddr)
+{
+	struct vm_struct *area;
+	struct gnttab_unmap_grant_ref op = {
+		.host_addr = (unsigned long)vaddr,
+	};
+
+	/* It'd be nice if linux/vmalloc.h provided a find_vm_area(void *addr)
+	 * method so that we don't have to muck with vmalloc internals here.
+	 * We could force the user to hang on to their struct vm_struct from
+	 * xenbus_map_ring_valloc, but these 6 lines considerably simplify
+	 * this API.
+	 */
+	read_lock(&vmlist_lock);
+	for (area = vmlist; area != NULL; area = area->next) {
+		if (area->addr == vaddr)
+			break;
+	}
+	read_unlock(&vmlist_lock);
+
+	if (!area) {
+		xenbus_dev_error(dev, -ENOENT,
+				 "can't find mapped virtual address %p", vaddr);
+		return GNTST_bad_virt_addr;
+	}
+
+	op.handle = (grant_handle_t)area->phys_addr;
+
+	if (HYPERVISOR_grant_table_op(GNTTABOP_unmap_grant_ref, &op, 1))
+		BUG();
+
+	if (op.status == GNTST_okay)
+		free_vm_area(area);
+	else
+		xenbus_dev_error(dev, op.status,
+				 "unmapping page at handle %d error %d",
+				 (int16_t)area->phys_addr, op.status);
+
+	return op.status;
+}
+EXPORT_SYMBOL_GPL(xenbus_unmap_ring_vfree);
+
+
+/**
+ * xenbus_unmap_ring
+ * @dev: xenbus device
+ * @handle: grant handle
+ * @vaddr: addr to unmap
+ *
+ * Unmap a page of memory in this domain that was imported from another domain.
+ * Returns 0 on success and returns GNTST_* on error
+ * (see xen/include/interface/grant_table.h).
+ */
+int xenbus_unmap_ring(struct xenbus_device *dev,
+		      grant_handle_t handle, void *vaddr)
+{
+	struct gnttab_unmap_grant_ref op = {
+		.host_addr = (unsigned long)vaddr,
+		.handle    = handle,
+	};
+
+	if (HYPERVISOR_grant_table_op(GNTTABOP_unmap_grant_ref, &op, 1))
+		BUG();
+
+	if (op.status != GNTST_okay)
+		xenbus_dev_error(dev, op.status,
+				 "unmapping page at handle %d error %d",
+				 handle, op.status);
+
+	return op.status;
+}
+EXPORT_SYMBOL_GPL(xenbus_unmap_ring);
+#endif
+
+
+/**
+ * xenbus_read_driver_state
+ * @path: path for driver
+ *
+ * Return the state of the driver rooted at the given store path, or
+ * XenbusStateUnknown if no state can be read.
+ */
 enum xenbus_state xenbus_read_driver_state(const char *path)
 {
 	enum xenbus_state result;
--- head-2011-03-17.orig/drivers/xen/xenbus/xenbus_comms.c	2011-01-31 17:32:16.000000000 +0100
+++ head-2011-03-17/drivers/xen/xenbus/xenbus_comms.c	2011-01-31 17:49:31.000000000 +0100
@@ -34,12 +34,15 @@
 #include <linux/interrupt.h>
 #include <linux/sched.h>
 #include <linux/err.h>
-#include <linux/ptrace.h>
-#include <linux/workqueue.h>
-#include <xen/evtchn.h>
 #include <xen/xenbus.h>
-
+#if defined(CONFIG_XEN) || defined(MODULE)
+#include <xen/evtchn.h>
 #include <asm/hypervisor.h>
+#else
+#include <asm/xen/hypervisor.h>
+#include <xen/events.h>
+#include <xen/page.h>
+#endif
 
 #include "xenbus_comms.h"
 
@@ -49,7 +52,6 @@
 
 static int xenbus_irq;
 
-extern void xenbus_probe(struct work_struct *);
 static DECLARE_WORK(probe_work, xenbus_probe);
 
 static DECLARE_WAIT_QUEUE_HEAD(xb_waitq);
@@ -112,6 +114,13 @@ static const void *get_input_chunk(XENST
 	return buf + MASK_XENSTORE_IDX(cons);
 }
 
+/**
+ * xb_write - low level write
+ * @data: buffer to send
+ * @len: length of buffer
+ *
+ * Returns 0 on success, error otherwise.
+ */
 int xb_write(const void *data, unsigned len)
 {
 	struct xenstore_domain_interface *intf = xen_store_interface;
@@ -220,7 +229,9 @@ int xb_read(void *data, unsigned len)
 	return 0;
 }
 
-/* Set up interrupt handler off store event channel. */
+/**
+ * xb_init_comms - Set up interrupt handler off store event channel.
+ */
 int xb_init_comms(void)
 {
 	struct xenstore_domain_interface *intf = xen_store_interface;
@@ -240,7 +251,11 @@ int xb_init_comms(void)
 	if (xenbus_irq)
 		unbind_from_irqhandler(xenbus_irq, &xb_waitq);
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 	err = bind_caller_port_to_irqhandler(
+#else
+	err = bind_evtchn_to_irqhandler(
+#endif
 		xen_store_evtchn, wake_waiting,
 		0, "xenbus", &xb_waitq);
 	if (err <= 0) {
--- head-2011-03-17.orig/drivers/xen/xenbus/xenbus_probe.c	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/drivers/xen/xenbus/xenbus_probe.c	2011-01-31 17:49:31.000000000 +0100
@@ -43,21 +43,26 @@
 #include <linux/mm.h>
 #include <linux/notifier.h>
 #include <linux/mutex.h>
-#include <linux/module.h>
-#include <xen/gnttab.h>
+#include <linux/io.h>
 
-#include <asm/io.h>
 #include <asm/page.h>
-#include <asm/maddr.h>
 #include <asm/pgtable.h>
+#if defined(CONFIG_XEN) || defined(MODULE)
 #include <asm/hypervisor.h>
 #include <xen/xenbus.h>
 #include <xen/xen_proc.h>
 #include <xen/evtchn.h>
 #include <xen/features.h>
+#include <xen/gnttab.h>
 #ifdef MODULE
 #include <xen/hvm.h>
 #endif
+#else
+#include <asm/xen/hypervisor.h>
+#include <xen/xenbus.h>
+#include <xen/events.h>
+#include <xen/page.h>
+#endif
 
 #include "xenbus_comms.h"
 #include "xenbus_probe.h"
@@ -170,7 +175,7 @@ static int read_backend_details(struct x
 	return read_otherend_details(xendev, "backend-id", "backend");
 }
 
-#if LINUX_VERSION_CODE >= KERNEL_VERSION(2,6,16)
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(2,6,16) && (defined(CONFIG_XEN) || defined(MODULE))
 static int xenbus_uevent_frontend(struct device *dev, char **envp,
 				  int num_envp, char *buffer, int buffer_size)
 {
@@ -209,12 +214,16 @@ static struct xen_bus_type xenbus_fronte
 		.probe    = xenbus_dev_probe,
 		.remove   = xenbus_dev_remove,
 		.shutdown = xenbus_dev_shutdown,
+#if defined(CONFIG_XEN) || defined(MODULE)
 		.uevent   = xenbus_uevent_frontend,
 #endif
+#endif
 	},
+#if defined(CONFIG_XEN) || defined(MODULE)
 	.dev = {
 		.bus_id = "xen",
 	},
+#endif
 };
 
 static void otherend_changed(struct xenbus_watch *watch,
@@ -230,14 +239,15 @@ static void otherend_changed(struct xenb
 	if (!dev->otherend ||
 	    strncmp(dev->otherend, vec[XS_WATCH_PATH],
 		    strlen(dev->otherend))) {
-		DPRINTK("Ignoring watch at %s", vec[XS_WATCH_PATH]);
+		dev_dbg(&dev->dev, "Ignoring watch at %s", vec[XS_WATCH_PATH]);
 		return;
 	}
 
 	state = xenbus_read_driver_state(dev->otherend);
 
-	DPRINTK("state is %d (%s), %s, %s", state, xenbus_strstate(state),
-		dev->otherend_watch.node, vec[XS_WATCH_PATH]);
+	dev_dbg(&dev->dev, "state is %d (%s), %s, %s",
+		state, xenbus_strstate(state), dev->otherend_watch.node,
+		vec[XS_WATCH_PATH]);
 
 #if LINUX_VERSION_CODE >= KERNEL_VERSION(2,6,16)
 	/*
@@ -274,8 +284,13 @@ static int talk_to_otherend(struct xenbu
 
 static int watch_otherend(struct xenbus_device *dev)
 {
+#if defined(CONFIG_XEN) || defined(MODULE)
 	return xenbus_watch_path2(dev, dev->otherend, "state",
 				  &dev->otherend_watch, otherend_changed);
+#else
+	return xenbus_watch_pathfmt(dev, &dev->otherend_watch, otherend_changed,
+				    "%s/%s", dev->otherend, "state");
+#endif
 }
 
 
@@ -301,9 +316,9 @@ int xenbus_dev_probe(struct device *_dev
 
 	err = talk_to_otherend(dev);
 	if (err) {
-		printk(KERN_WARNING
-		       "xenbus_probe: talk_to_otherend on %s failed.\n",
-		       dev->nodename);
+		dev_warn(&dev->dev,
+		         "xenbus_probe: talk_to_otherend on %s failed.\n",
+		         dev->nodename);
 		return err;
 	}
 
@@ -313,9 +328,9 @@ int xenbus_dev_probe(struct device *_dev
 
 	err = watch_otherend(dev);
 	if (err) {
-		printk(KERN_WARNING
-		       "xenbus_probe: watch_otherend on %s failed.\n",
-		       dev->nodename);
+		dev_warn(&dev->dev,
+		         "xenbus_probe: watch_otherend on %s failed.\n",
+		         dev->nodename);
 		return err;
 	}
 
@@ -360,8 +375,8 @@ static void xenbus_dev_shutdown(struct d
 
 	get_device(&dev->dev);
 	if (dev->state != XenbusStateConnected) {
-		printk("%s: %s: %s != Connected, skipping\n", __FUNCTION__,
-		       dev->nodename, xenbus_strstate(dev->state));
+		dev_info(&dev->dev, "%s: %s: %s != Connected, skipping\n", __FUNCTION__,
+		         dev->nodename, xenbus_strstate(dev->state));
 		goto out;
 	}
 	xenbus_switch_state(dev, XenbusStateClosing);
@@ -371,7 +386,8 @@ static void xenbus_dev_shutdown(struct d
 
 	timeout = wait_for_completion_timeout(&dev->down, timeout);
 	if (!timeout)
-		printk("%s: %s timeout closing device\n", __FUNCTION__, dev->nodename);
+		dev_info(&dev->dev, "%s: %s timeout closing device\n",
+		         __FUNCTION__, dev->nodename);
  out:
 	put_device(&dev->dev);
 }
@@ -559,7 +575,9 @@ int xenbus_probe_node(struct xen_bus_typ
 	xendev->devicetype = tmpstring;
 	init_completion(&xendev->down);
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 	xendev->dev.parent = &bus->dev;
+#endif
 	xendev->dev.bus = &bus->bus;
 	xendev->dev.release = xenbus_dev_release;
 
@@ -574,15 +592,16 @@ int xenbus_probe_node(struct xen_bus_typ
 
 	err = device_create_file(&xendev->dev, &dev_attr_nodename);
 	if (err)
-		goto unregister;
+		goto fail_unregister;
+
 	err = device_create_file(&xendev->dev, &dev_attr_devtype);
 	if (err)
-		goto unregister;
+		goto fail_remove_file;
 
 	return 0;
-unregister:
+fail_remove_file:
 	device_remove_file(&xendev->dev, &dev_attr_nodename);
-	device_remove_file(&xendev->dev, &dev_attr_devtype);
+fail_unregister:
 	device_unregister(&xendev->dev);
 fail:
 	kfree(xendev);
@@ -598,7 +617,8 @@ static int xenbus_probe_frontend(const c
 	if (!strcmp(type, "console"))
 		return 0;
 
-	nodename = kasprintf(GFP_KERNEL, "%s/%s/%s", xenbus_frontend.root, type, name);
+	nodename = kasprintf(GFP_KERNEL, "%s/%s/%s",
+			     xenbus_frontend.root, type, name);
 	if (!nodename)
 		return -ENOMEM;
 
@@ -676,7 +696,7 @@ static int strsep_len(const char *str, c
 	return (len == 0) ? i : -ERANGE;
 }
 
-void dev_changed(const char *node, struct xen_bus_type *bus)
+void xenbus_dev_changed(const char *node, struct xen_bus_type *bus)
 {
 	int exists, rootlen;
 	struct xenbus_device *dev;
@@ -684,7 +704,7 @@ void dev_changed(const char *node, struc
 	const char *p, *root;
 
 	if (bus->error || char_count(node, '/') < 2)
- 		return;
+		return;
 
 	exists = xenbus_exists(XBT_NIL, node, "");
 	if (!exists) {
@@ -718,7 +738,7 @@ static void frontend_changed(struct xenb
 {
 	DPRINTK("");
 
-	dev_changed(vec[XS_WATCH_PATH], &xenbus_frontend);
+	xenbus_dev_changed(vec[XS_WATCH_PATH], &xenbus_frontend);
 }
 
 /* We watch for devices appearing and vanishing. */
@@ -943,6 +963,7 @@ static int xsd_port_read(char *page, cha
 }
 #endif
 
+#if defined(CONFIG_XEN_XENBUS_DEV) || defined(MODULE)
 static int xb_free_port(evtchn_port_t port)
 {
 	struct evtchn_close close;
@@ -958,7 +979,7 @@ int xenbus_conn(domid_t remote_dom, unsi
 	BUG_ON(atomic_read(&xenbus_xsd_state) != XENBUS_XSD_FOREIGN_INIT);
 	BUG_ON(!is_initial_xendomain());
 
-#if defined(CONFIG_PROC_FS) && defined(CONFIG_XEN_PRIVILEGED_GUEST)
+#ifdef CONFIG_XEN_PRIVILEGED_GUEST
 	remove_xen_proc_entry("xsd_kva");
 	remove_xen_proc_entry("xsd_port");
 #endif
@@ -998,11 +1019,18 @@ fail0:
 	xen_store_evtchn = -1;
 	return rc;
 }
+#endif
 
-static int xenbus_probe_init(void)
+#ifndef MODULE
+static int __init xenbus_probe_init(void)
+#else
+static int __devinit xenbus_probe_init(void)
+#endif
 {
 	int err = 0;
+#if defined(CONFIG_XEN) || defined(MODULE)
 	unsigned long page = 0;
+#endif
 
 	DPRINTK("");
 
@@ -1021,6 +1049,7 @@ static int xenbus_probe_init(void)
 	 * Domain0 doesn't have a store_evtchn or store_mfn yet.
 	 */
 	if (is_initial_xendomain()) {
+#if defined(CONFIG_XEN) || defined(MODULE)
 		struct evtchn_alloc_unbound alloc_unbound;
 
 		/* Allocate Xenstore page */
@@ -1059,10 +1088,13 @@ static int xenbus_probe_init(void)
 		if (xsd_port_intf)
 			xsd_port_intf->read_proc = xsd_port_read;
 #endif
+#else
+		/* dom0 not yet supported */
+#endif
 		xen_store_interface = mfn_to_virt(xen_store_mfn);
 	} else {
 		atomic_set(&xenbus_xsd_state, XENBUS_XSD_FOREIGN_READY);
-#ifdef CONFIG_XEN
+#ifndef MODULE
 		xen_store_evtchn = xen_start_info->store_evtchn;
 		xen_store_mfn = xen_start_info->store_mfn;
 		xen_store_interface = mfn_to_virt(xen_store_mfn);
@@ -1078,7 +1110,9 @@ static int xenbus_probe_init(void)
 			goto err;
 	}
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 	xenbus_dev_init();
+#endif
 
 	/* Initialize the interface to xenstore. */
 	err = xs_init();
@@ -1088,6 +1122,7 @@ static int xenbus_probe_init(void)
 		goto err;
 	}
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 	/* Register ourselves with the kernel device subsystem */
 	if (!xenbus_frontend.error) {
 		xenbus_frontend.error = device_register(&xenbus_frontend.dev);
@@ -1098,6 +1133,7 @@ static int xenbus_probe_init(void)
 			       xenbus_frontend.error);
 		}
 	}
+#endif
 	xenbus_backend_device_register();
 
 	if (!is_initial_xendomain())
@@ -1112,16 +1148,22 @@ static int xenbus_probe_init(void)
 	 * registered.
 	 */
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 	if (page != 0)
 		free_page(page);
+#endif
 	return err;
 }
 
-#ifdef CONFIG_XEN
+#ifndef MODULE
 postcore_initcall(xenbus_probe_init);
+#ifdef CONFIG_XEN
 MODULE_LICENSE("Dual BSD/GPL");
 #else
-int xenbus_init(void)
+MODULE_LICENSE("GPL");
+#endif
+#else
+int __devinit xenbus_init(void)
 {
 	return xenbus_probe_init();
 }
--- head-2011-03-17.orig/drivers/xen/xenbus/xenbus_probe.h	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/drivers/xen/xenbus/xenbus_probe.h	2011-01-31 17:49:31.000000000 +0100
@@ -62,7 +62,9 @@ struct xen_bus_type
 	int (*get_bus_id)(char bus_id[XEN_BUS_ID_SIZE], const char *nodename);
 	int (*probe)(const char *type, const char *dir);
 	struct bus_type bus;
+#if defined(CONFIG_XEN) || defined(MODULE)
 	struct device dev;
+#endif
 };
 
 extern int xenbus_match(struct device *_dev, struct device_driver *_drv);
@@ -77,6 +79,6 @@ extern int xenbus_probe_node(struct xen_
 			     const char *nodename);
 extern int xenbus_probe_devices(struct xen_bus_type *bus);
 
-extern void dev_changed(const char *node, struct xen_bus_type *bus);
+extern void xenbus_dev_changed(const char *node, struct xen_bus_type *bus);
 
 #endif
--- head-2011-03-17.orig/drivers/xen/xenbus/xenbus_probe_backend.c	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/drivers/xen/xenbus/xenbus_probe_backend.c	2011-01-31 17:49:31.000000000 +0100
@@ -236,7 +236,7 @@ static void backend_changed(struct xenbu
 {
 	DPRINTK("");
 
-	dev_changed(vec[XS_WATCH_PATH], &xenbus_backend);
+	xenbus_dev_changed(vec[XS_WATCH_PATH], &xenbus_backend);
 }
 
 static struct xenbus_watch be_watch = {
--- head-2011-03-17.orig/drivers/xen/xenbus/xenbus_xs.c	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/drivers/xen/xenbus/xenbus_xs.c	2011-01-31 17:49:31.000000000 +0100
@@ -662,7 +662,9 @@ void unregister_xenbus_watch(struct xenb
 	char token[sizeof(watch) * 2 + 1];
 	int err;
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 	BUG_ON(watch->flags & XBWF_new_thread);
+#endif
 
 	sprintf(token, "%lX", (long)watch);
 
@@ -681,6 +683,11 @@ void unregister_xenbus_watch(struct xenb
 
 	up_read(&xs_state.watch_mutex);
 
+	/* Make sure there are no callbacks running currently (unless
+	   its us) */
+	if (current->pid != xenwatch_pid)
+		mutex_lock(&xenwatch_mutex);
+
 	/* Cancel pending watch events. */
 	spin_lock(&watch_events_lock);
 	list_for_each_entry_safe(msg, tmp, &watch_events, list) {
@@ -692,11 +699,8 @@ void unregister_xenbus_watch(struct xenb
 	}
 	spin_unlock(&watch_events_lock);
 
-	/* Flush any currently-executing callback, unless we are it. :-) */
-	if (current->pid != xenwatch_pid) {
-		mutex_lock(&xenwatch_mutex);
+	if (current->pid != xenwatch_pid)
 		mutex_unlock(&xenwatch_mutex);
-	}
 }
 EXPORT_SYMBOL_GPL(unregister_xenbus_watch);
 
@@ -734,6 +738,7 @@ void xs_suspend_cancel(void)
 	mutex_unlock(&xs_state.transaction_mutex);
 }
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 static int xenwatch_handle_callback(void *data)
 {
 	struct xs_stored_msg *msg = data;
@@ -751,6 +756,7 @@ static int xenwatch_handle_callback(void
 
 	return 0;
 }
+#endif
 
 static int xenwatch_thread(void *unused)
 {
@@ -780,6 +786,7 @@ static int xenwatch_thread(void *unused)
 
 		msg = list_entry(ent, struct xs_stored_msg, list);
 
+#if defined(CONFIG_XEN) || defined(MODULE)
 		/*
 		 * Unlock the mutex before running an XBWF_new_thread
 		 * handler. kthread_run can block which can deadlock
@@ -796,6 +803,15 @@ static int xenwatch_thread(void *unused)
 			xenwatch_handle_callback(msg);
 			mutex_unlock(&xenwatch_mutex);
 		}
+#else
+		msg->u.watch.handle->callback(
+			msg->u.watch.handle,
+			(const char **)msg->u.watch.vec,
+			msg->u.watch.vec_size);
+		mutex_unlock(&xenwatch_mutex);
+		kfree(msg->u.watch.vec);
+		kfree(msg);
+#endif
 	}
 
 	return 0;
--- head-2011-03-17.orig/drivers/xen/xenoprof/xenoprofile.c	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/drivers/xen/xenoprof/xenoprofile.c	2011-01-31 17:49:31.000000000 +0100
@@ -26,7 +26,6 @@
 #include <asm/pgtable.h>
 #include <xen/evtchn.h>
 #include <xen/xenoprof.h>
-#include <xen/driver_util.h>
 #include <xen/interface/xen.h>
 #include <xen/interface/xenoprof.h>
 #include "../../../drivers/oprofile/cpu_buffer.h"
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/fixmap_32.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/fixmap_32.h	2011-01-31 17:49:31.000000000 +0100
@@ -53,6 +53,8 @@ extern unsigned long __FIXADDR_TOP;
 enum fixed_addresses {
 	FIX_HOLE,
 	FIX_VDSO,
+	FIX_DBGP_BASE,
+	FIX_EARLYCON_MEM_BASE,
 #ifdef CONFIG_X86_LOCAL_APIC
 	FIX_APIC_BASE,	/* local (CPU) APIC) -- required for SMP or not */
 #endif
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/highmem.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/highmem.h	2011-01-31 17:49:31.000000000 +0100
@@ -75,8 +75,7 @@ struct page *kmap_atomic_to_page(void *p
 
 #define kmap_atomic_pte(page, type) \
 	kmap_atomic_prot(page, type, \
-	                 test_bit(PG_pinned, &(page)->flags) \
-	                 ? PAGE_KERNEL_RO : kmap_prot)
+	                 PagePinned(page) ? PAGE_KERNEL_RO : kmap_prot)
 
 #define flush_cache_kmaps()	do { } while (0)
 
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/maddr_32.h	2008-04-02 12:34:02.000000000 +0200
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/maddr_32.h	2011-01-31 17:49:31.000000000 +0100
@@ -155,6 +155,7 @@ static inline paddr_t pte_machine_to_phy
 
 #ifdef CONFIG_X86_PAE
 #define __pte_ma(x)	((pte_t) { (x), (maddr_t)(x) >> 32 } )
+extern unsigned long long __supported_pte_mask;
 static inline pte_t pfn_pte_ma(unsigned long page_nr, pgprot_t pgprot)
 {
 	pte_t pte;
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/mmu_context_32.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/mmu_context_32.h	2011-01-31 17:49:31.000000000 +0100
@@ -16,7 +16,7 @@ void mm_pin_all(void);
 static inline void xen_activate_mm(struct mm_struct *prev,
 				   struct mm_struct *next)
 {
-	if (!test_bit(PG_pinned, &virt_to_page(next->pgd)->flags))
+	if (!PagePinned(virt_to_page(next->pgd)))
 		mm_pin(next);
 }
 
@@ -51,6 +51,8 @@ static inline void __prepare_arch_switch
 		: : "r" (0) );
 }
 
+void leave_mm(unsigned long cpu);
+
 static inline void switch_mm(struct mm_struct *prev,
 			     struct mm_struct *next,
 			     struct task_struct *tsk)
@@ -60,7 +62,7 @@ static inline void switch_mm(struct mm_s
 
 	if (likely(prev != next)) {
 		BUG_ON(!xen_feature(XENFEAT_writable_page_tables) &&
-		       !test_bit(PG_pinned, &virt_to_page(next->pgd)->flags));
+		       !PagePinned(virt_to_page(next->pgd)));
 
 		/* stop flush ipis for the previous mm */
 		cpu_clear(cpu, prev->cpu_vm_mask);
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/pgalloc_32.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/pgalloc_32.h	2011-01-31 17:49:31.000000000 +0100
@@ -5,7 +5,7 @@
 #include <linux/mm.h>		/* for struct page */
 #include <asm/io.h>		/* for phys_to_virt and page_to_pseudophys */
 
-#define paravirt_alloc_pt(pfn) do { } while (0)
+#define paravirt_alloc_pt(mm, pfn) do { } while (0)
 #define paravirt_alloc_pd(pfn) do { } while (0)
 #define paravirt_alloc_pd(pfn) do { } while (0)
 #define paravirt_alloc_pd_clone(pfn, clonepfn, start, count) do { } while (0)
@@ -14,15 +14,15 @@
 
 #define pmd_populate_kernel(mm, pmd, pte)			\
 do {								\
-	paravirt_alloc_pt(__pa(pte) >> PAGE_SHIFT);		\
+	paravirt_alloc_pt(mm, __pa(pte) >> PAGE_SHIFT);		\
 	set_pmd(pmd, __pmd(_PAGE_TABLE + __pa(pte)));		\
 } while (0)
 
 #define pmd_populate(mm, pmd, pte) 					\
 do {									\
 	unsigned long pfn = page_to_pfn(pte);				\
-	paravirt_alloc_pt(pfn);						\
-	if (test_bit(PG_pinned, &virt_to_page((mm)->pgd)->flags)) {	\
+	paravirt_alloc_pt(mm, pfn);					\
+	if (PagePinned(virt_to_page((mm)->pgd))) {			\
 		if (!PageHighMem(pte))					\
 			BUG_ON(HYPERVISOR_update_va_mapping(		\
 			  (unsigned long)__va(pfn << PAGE_SHIFT),	\
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/pgtable_32.h	2011-02-07 15:38:07.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/pgtable_32.h	2011-02-07 15:38:23.000000000 +0100
@@ -26,9 +26,6 @@
 #include <linux/spinlock.h>
 #include <linux/sched.h>
 
-/* Is this pagetable pinned? */
-#define PG_pinned	PG_arch_1
-
 struct vm_area_struct;
 
 /*
@@ -82,7 +79,7 @@ void paging_init(void);
  * area for the same reason. ;)
  */
 #define VMALLOC_OFFSET	(8*1024*1024)
-#define VMALLOC_START	(((unsigned long) high_memory + vmalloc_earlyreserve + \
+#define VMALLOC_START	(((unsigned long) high_memory + \
 			2*VMALLOC_OFFSET-1) & ~(VMALLOC_OFFSET-1))
 #ifdef CONFIG_HIGHMEM
 # define VMALLOC_END	(PKMAP_BASE-2*PAGE_SIZE)
@@ -231,8 +228,6 @@ extern unsigned long pg0[];
  * The following only work if pte_present() is true.
  * Undefined behaviour if not..
  */
-static inline int pte_user(pte_t pte)		{ return (pte).pte_low & _PAGE_USER; }
-static inline int pte_read(pte_t pte)		{ return (pte).pte_low & _PAGE_USER; }
 static inline int pte_dirty(pte_t pte)		{ return (pte).pte_low & _PAGE_DIRTY; }
 static inline int pte_young(pte_t pte)		{ return (pte).pte_low & _PAGE_ACCESSED; }
 static inline int pte_write(pte_t pte)		{ return (pte).pte_low & _PAGE_RW; }
@@ -243,13 +238,9 @@ static inline int pte_huge(pte_t pte)		{
  */
 static inline int pte_file(pte_t pte)		{ return (pte).pte_low & _PAGE_FILE; }
 
-static inline pte_t pte_rdprotect(pte_t pte)	{ (pte).pte_low &= ~_PAGE_USER; return pte; }
-static inline pte_t pte_exprotect(pte_t pte)	{ (pte).pte_low &= ~_PAGE_USER; return pte; }
 static inline pte_t pte_mkclean(pte_t pte)	{ (pte).pte_low &= ~_PAGE_DIRTY; return pte; }
 static inline pte_t pte_mkold(pte_t pte)	{ (pte).pte_low &= ~_PAGE_ACCESSED; return pte; }
 static inline pte_t pte_wrprotect(pte_t pte)	{ (pte).pte_low &= ~_PAGE_RW; return pte; }
-static inline pte_t pte_mkread(pte_t pte)	{ (pte).pte_low |= _PAGE_USER; return pte; }
-static inline pte_t pte_mkexec(pte_t pte)	{ (pte).pte_low |= _PAGE_USER; return pte; }
 static inline pte_t pte_mkdirty(pte_t pte)	{ (pte).pte_low |= _PAGE_DIRTY; return pte; }
 static inline pte_t pte_mkyoung(pte_t pte)	{ (pte).pte_low |= _PAGE_ACCESSED; return pte; }
 static inline pte_t pte_mkwrite(pte_t pte)	{ (pte).pte_low |= _PAGE_RW; return pte; }
@@ -295,22 +286,20 @@ static inline pte_t xen_local_ptep_get_a
 #define ptep_set_access_flags(vma, address, ptep, entry, dirty)		\
 ({									\
 	int __changed = !pte_same(*(ptep), entry);			\
-	if (__changed && (dirty))					\
-		ptep_establish(vma, address, ptep, entry);		\
+	if (__changed && (dirty)) {					\
+		if ( likely((vma)->vm_mm == current->mm) ) {		\
+			BUG_ON(HYPERVISOR_update_va_mapping(address,	\
+				entry,					\
+				(unsigned long)(vma)->vm_mm->cpu_vm_mask.bits| \
+					UVMF_INVLPG|UVMF_MULTI));	\
+		} else {						\
+			xen_l1_entry_update(ptep, entry);		\
+			flush_tlb_page(vma, address);			\
+		}							\
+	}								\
 	__changed;							\
 })
 
-#define __HAVE_ARCH_PTEP_TEST_AND_CLEAR_DIRTY
-#define ptep_test_and_clear_dirty(vma, addr, ptep) ({			\
-	int __ret = 0;							\
-	if (pte_dirty(*(ptep)))						\
-		__ret = test_and_clear_bit(_PAGE_BIT_DIRTY,		\
-						&(ptep)->pte_low);	\
-	if (__ret)							\
-		pte_update((vma)->vm_mm, addr, ptep);			\
-	__ret;								\
-})
-
 #define __HAVE_ARCH_PTEP_TEST_AND_CLEAR_YOUNG
 #define ptep_test_and_clear_young(vma, addr, ptep) ({			\
 	int __ret = 0;							\
@@ -322,44 +311,13 @@ static inline pte_t xen_local_ptep_get_a
 	__ret;								\
 })
 
-/*
- * Rules for using ptep_establish: the pte MUST be a user pte, and
- * must be a present->present transition.
- */
-#define __HAVE_ARCH_PTEP_ESTABLISH
-#define ptep_establish(vma, address, ptep, pteval)			\
-do {									\
-	if ( likely((vma)->vm_mm == current->mm) ) {			\
-		BUG_ON(HYPERVISOR_update_va_mapping(address,		\
-			pteval,						\
-			(unsigned long)(vma)->vm_mm->cpu_vm_mask.bits|	\
-				UVMF_INVLPG|UVMF_MULTI));		\
-	} else {							\
-		xen_l1_entry_update(ptep, pteval);			\
-		flush_tlb_page(vma, address);				\
-	}								\
-} while (0)
-
-#define __HAVE_ARCH_PTEP_CLEAR_DIRTY_FLUSH
-#define ptep_clear_flush_dirty(vma, address, ptep)			\
-({									\
-	pte_t __pte = *(ptep);						\
-	int __dirty = pte_dirty(__pte);					\
-	__pte = pte_mkclean(__pte);					\
-	if (test_bit(PG_pinned, &virt_to_page((vma)->vm_mm->pgd)->flags)) \
-		(void)ptep_set_access_flags(vma, address, ptep, __pte, __dirty); \
-	else if (__dirty)						\
-		(ptep)->pte_low = __pte.pte_low;			\
-	__dirty;							\
-})
-
 #define __HAVE_ARCH_PTEP_CLEAR_YOUNG_FLUSH
 #define ptep_clear_flush_young(vma, address, ptep)			\
 ({									\
 	pte_t __pte = *(ptep);						\
 	int __young = pte_young(__pte);					\
 	__pte = pte_mkold(__pte);					\
-	if (test_bit(PG_pinned, &virt_to_page((vma)->vm_mm->pgd)->flags)) \
+	if (PagePinned(virt_to_page((vma)->vm_mm->pgd)))		\
 		(void)ptep_set_access_flags(vma, address, ptep, __pte, __young); \
 	else if (__young)						\
 		(ptep)->pte_low = __pte.pte_low;			\
@@ -383,7 +341,7 @@ static inline pte_t ptep_get_and_clear(s
 #define ptep_get_and_clear_full(mm, addr, ptep, full)			\
 	((full) ? ({							\
 		pte_t __res = *(ptep);					\
-		if (test_bit(PG_pinned, &virt_to_page((mm)->pgd)->flags)) \
+		if (PagePinned(virt_to_page((mm)->pgd)))		\
 			xen_l1_entry_update(ptep, __pte(0));		\
 		else							\
 			*(ptep) = __pte(0);				\
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/pgtable-3level.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/pgtable-3level.h	2011-01-31 17:49:31.000000000 +0100
@@ -23,26 +23,11 @@
 #define pud_present(pud)			1
 
 /*
- * Is the pte executable?
- */
-static inline int pte_x(pte_t pte)
-{
-	return !(__pte_val(pte) & _PAGE_NX);
-}
-
-/*
- * All present user-pages with !NX bit are user-executable:
- */
-static inline int pte_exec(pte_t pte)
-{
-	return pte_user(pte) && pte_x(pte);
-}
-/*
  * All present pages with !NX bit are kernel-executable:
  */
 static inline int pte_exec_kernel(pte_t pte)
 {
-	return pte_x(pte);
+	return !(__pte_val(pte) & _PAGE_NX);
 }
 
 /* Rules for using set_pte: the pte being assigned *must* be
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/processor_32.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/processor_32.h	2011-01-31 17:49:31.000000000 +0100
@@ -89,7 +89,6 @@ struct cpuinfo_x86 {
 #define X86_VENDOR_UMC 3
 #define X86_VENDOR_NEXGEN 4
 #define X86_VENDOR_CENTAUR 5
-#define X86_VENDOR_RISE 6
 #define X86_VENDOR_TRANSMETA 7
 #define X86_VENDOR_NSC 8
 #define X86_VENDOR_NUM 9
@@ -122,6 +121,7 @@ void __init cpu_detect(struct cpuinfo_x8
 extern void identify_boot_cpu(void);
 extern void identify_secondary_cpu(struct cpuinfo_x86 *);
 extern void print_cpu_info(struct cpuinfo_x86 *);
+extern void init_scattered_cpuid_features(struct cpuinfo_x86 *c);
 extern unsigned int init_intel_cacheinfo(struct cpuinfo_x86 *c);
 extern unsigned short num_cache_leaves;
 
@@ -171,17 +171,6 @@ static inline void clear_in_cr4 (unsigne
 	write_cr4(cr4);
 }
 
-/*
- *      NSC/Cyrix CPU indexed register access macros
- */
-
-#define getCx86(reg) ({ outb((reg), 0x22); inb(0x23); })
-
-#define setCx86(reg, data) do { \
-	outb((reg), 0x22); \
-	outb((data), 0x23); \
-} while (0)
-
 /* Stop speculative execution */
 static inline void sync_core(void)
 {
@@ -230,6 +219,10 @@ extern int bootloader_type;
 
 #define HAVE_ARCH_PICK_MMAP_LAYOUT
 
+extern void hard_disable_TSC(void);
+extern void disable_TSC(void);
+extern void hard_enable_TSC(void);
+
 /*
  * Size of io_bitmap.
  */
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/system_32.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/system_32.h	2011-01-31 17:49:31.000000000 +0100
@@ -205,11 +205,6 @@ static inline unsigned long get_limit(un
  */
  
 
-/* 
- * Actually only lfence would be needed for mb() because all stores done 
- * by the kernel should be already ordered. But keep a full barrier for now. 
- */
-
 #define mb() alternative("lock; addl $0,0(%%esp)", "mfence", X86_FEATURE_XMM2)
 #define rmb() alternative("lock; addl $0,0(%%esp)", "lfence", X86_FEATURE_XMM2)
 
@@ -301,15 +296,6 @@ void enable_hlt(void);
 extern int es7000_plat;
 void cpu_idle_wait(void);
 
-/*
- * On SMP systems, when the scheduler does migration-cost autodetection,
- * it needs a way to flush as much of the CPU's caches as possible:
- */
-static inline void sched_cacheflush(void)
-{
-	wbinvd();
-}
-
 extern unsigned long arch_align_stack(unsigned long sp);
 extern void free_init_pages(char *what, unsigned long begin, unsigned long end);
 
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/tlbflush_32.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/tlbflush_32.h	2011-01-31 17:49:31.000000000 +0100
@@ -91,7 +91,11 @@ struct tlb_state
 DECLARE_PER_CPU(struct tlb_state, cpu_tlbstate);
 #endif	/* SMP */
 
-#define flush_tlb_kernel_range(start, end) flush_tlb_all()
+static inline void flush_tlb_kernel_range(unsigned long start,
+					unsigned long end)
+{
+	flush_tlb_all();
+}
 
 static inline void flush_tlb_pgtables(struct mm_struct *mm,
 				      unsigned long start, unsigned long end)
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/fixmap_64.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/fixmap_64.h	2011-01-31 17:49:31.000000000 +0100
@@ -23,9 +23,9 @@
  * compile time, but to set the physical address only
  * in the boot process.
  *
- * these 'compile-time allocated' memory buffers are
- * fixed-size 4k pages. (or larger if used with an increment
- * highger than 1) use fixmap_set(idx,phys) to associate
+ * These 'compile-time allocated' memory buffers are
+ * fixed-size 4k pages (or larger if used with an increment
+ * higher than 1). Use set_fixmap(idx,phys) to associate
  * physical memory with fixmap indices.
  *
  * TLB entries of such buffers will not be flushed across
@@ -36,6 +36,8 @@ enum fixed_addresses {
 	VSYSCALL_LAST_PAGE,
 	VSYSCALL_FIRST_PAGE = VSYSCALL_LAST_PAGE + ((VSYSCALL_END-VSYSCALL_START) >> PAGE_SHIFT) - 1,
 	VSYSCALL_HPET,
+	FIX_DBGP_BASE,
+	FIX_EARLYCON_MEM_BASE,
 	FIX_HPET_BASE,
 #ifdef CONFIG_X86_LOCAL_APIC
 	FIX_APIC_BASE,	/* local (CPU) APIC) -- required for SMP or not */
@@ -105,7 +107,7 @@ static __always_inline unsigned long fix
 	if (idx >= __end_of_fixed_addresses)
 		__this_fixmap_does_not_exist();
 
-        return __fix_to_virt(idx);
+	return __fix_to_virt(idx);
 }
 
 #endif
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/mmu_context_64.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/mmu_context_64.h	2011-01-31 17:49:31.000000000 +0100
@@ -76,7 +76,7 @@ static inline void switch_mm(struct mm_s
 
 	if (likely(prev != next)) {
 		BUG_ON(!xen_feature(XENFEAT_writable_page_tables) &&
-		       !next->context.pinned);
+		       !PagePinned(virt_to_page(next->pgd)));
 
 		/* stop flush ipis for the previous mm */
 		cpu_clear(cpu, prev->cpu_vm_mask);
@@ -131,7 +131,7 @@ static inline void switch_mm(struct mm_s
 
 static inline void activate_mm(struct mm_struct *prev, struct mm_struct *next)
 {
-	if (!next->context.pinned)
+	if (!PagePinned(virt_to_page(next->pgd)))
 		mm_pin(next);
 	switch_mm(prev, next, NULL);
 }
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/pgalloc_64.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/pgalloc_64.h	2011-01-31 17:49:31.000000000 +0100
@@ -21,7 +21,7 @@ static inline void pmd_populate_kernel(s
 
 static inline void pmd_populate(struct mm_struct *mm, pmd_t *pmd, struct page *pte)
 {
-	if (unlikely((mm)->context.pinned)) {
+	if (unlikely(PagePinned(virt_to_page((mm)->pgd)))) {
 		BUG_ON(HYPERVISOR_update_va_mapping(
 			       (unsigned long)__va(page_to_pfn(pte) << PAGE_SHIFT),
 			       pfn_pte(page_to_pfn(pte), PAGE_KERNEL_RO), 0));
@@ -33,7 +33,7 @@ static inline void pmd_populate(struct m
 
 static inline void pud_populate(struct mm_struct *mm, pud_t *pud, pmd_t *pmd)
 {
-	if (unlikely((mm)->context.pinned)) {
+	if (unlikely(PagePinned(virt_to_page((mm)->pgd)))) {
 		BUG_ON(HYPERVISOR_update_va_mapping(
 			       (unsigned long)pmd,
 			       pfn_pte(virt_to_phys(pmd)>>PAGE_SHIFT, 
@@ -50,7 +50,7 @@ static inline void pud_populate(struct m
  */
 static inline void pgd_populate(struct mm_struct *mm, pgd_t *pgd, pud_t *pud)
 {
-	if (unlikely((mm)->context.pinned)) {
+	if (unlikely(PagePinned(virt_to_page((mm)->pgd)))) {
 		BUG_ON(HYPERVISOR_update_va_mapping(
 			       (unsigned long)pud,
 			       pfn_pte(virt_to_phys(pud)>>PAGE_SHIFT, 
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/pgtable_64.h	2011-02-07 15:38:08.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/pgtable_64.h	2011-02-07 15:38:18.000000000 +0100
@@ -304,7 +304,7 @@ static inline pte_t ptep_get_and_clear_f
 {
 	if (full) {
 		pte_t pte = *ptep;
-		if (mm->context.pinned)
+		if (PagePinned(virt_to_page(mm->pgd)))
 			xen_l1_entry_update(ptep, __pte(0));
 		else
 			*ptep = __pte(0);
@@ -333,21 +333,15 @@ static inline pte_t ptep_get_and_clear_f
  * Undefined behaviour if not..
  */
 #define __LARGE_PTE (_PAGE_PSE|_PAGE_PRESENT)
-static inline int pte_user(pte_t pte)		{ return __pte_val(pte) & _PAGE_USER; }
-static inline int pte_read(pte_t pte)		{ return __pte_val(pte) & _PAGE_USER; }
-static inline int pte_exec(pte_t pte)		{ return !(__pte_val(pte) & _PAGE_NX); }
 static inline int pte_dirty(pte_t pte)		{ return __pte_val(pte) & _PAGE_DIRTY; }
 static inline int pte_young(pte_t pte)		{ return __pte_val(pte) & _PAGE_ACCESSED; }
 static inline int pte_write(pte_t pte)		{ return __pte_val(pte) & _PAGE_RW; }
 static inline int pte_file(pte_t pte)		{ return __pte_val(pte) & _PAGE_FILE; }
 static inline int pte_huge(pte_t pte)		{ return __pte_val(pte) & _PAGE_PSE; }
 
-static inline pte_t pte_rdprotect(pte_t pte)	{ __pte_val(pte) &= ~_PAGE_USER; return pte; }
-static inline pte_t pte_exprotect(pte_t pte)	{ __pte_val(pte) &= ~_PAGE_USER; return pte; }
 static inline pte_t pte_mkclean(pte_t pte)	{ __pte_val(pte) &= ~_PAGE_DIRTY; return pte; }
 static inline pte_t pte_mkold(pte_t pte)	{ __pte_val(pte) &= ~_PAGE_ACCESSED; return pte; }
 static inline pte_t pte_wrprotect(pte_t pte)	{ __pte_val(pte) &= ~_PAGE_RW; return pte; }
-static inline pte_t pte_mkread(pte_t pte)	{ __pte_val(pte) |= _PAGE_USER; return pte; }
 static inline pte_t pte_mkexec(pte_t pte)	{ __pte_val(pte) &= ~_PAGE_NX; return pte; }
 static inline pte_t pte_mkdirty(pte_t pte)	{ __pte_val(pte) |= _PAGE_DIRTY; return pte; }
 static inline pte_t pte_mkyoung(pte_t pte)	{ __pte_val(pte) |= _PAGE_ACCESSED; return pte; }
@@ -355,13 +349,6 @@ static inline pte_t pte_mkwrite(pte_t pt
 static inline pte_t pte_mkhuge(pte_t pte)	{ __pte_val(pte) |= _PAGE_PSE; return pte; }
 static inline pte_t pte_clrhuge(pte_t pte)	{ __pte_val(pte) &= ~_PAGE_PSE; return pte; }
 
-static inline int ptep_test_and_clear_dirty(struct vm_area_struct *vma, unsigned long addr, pte_t *ptep)
-{
-	if (!pte_dirty(*ptep))
-		return 0;
-	return test_and_clear_bit(_PAGE_BIT_DIRTY, &ptep->pte);
-}
-
 static inline int ptep_test_and_clear_young(struct vm_area_struct *vma, unsigned long addr, pte_t *ptep)
 {
 	if (!pte_young(*ptep))
@@ -500,26 +487,13 @@ static inline pte_t pte_modify(pte_t pte
 	__changed;							\
 })
 
-#define __HAVE_ARCH_PTEP_CLEAR_DIRTY_FLUSH
-#define ptep_clear_flush_dirty(vma, address, ptep)			\
-({									\
-	pte_t __pte = *(ptep);						\
-	int __dirty = pte_dirty(__pte);					\
-	__pte = pte_mkclean(__pte);					\
-	if ((vma)->vm_mm->context.pinned)				\
-		(void)ptep_set_access_flags(vma, address, ptep, __pte, __dirty); \
-	else if (__dirty)						\
-		set_pte(ptep, __pte);					\
-	__dirty;							\
-})
-
 #define __HAVE_ARCH_PTEP_CLEAR_YOUNG_FLUSH
 #define ptep_clear_flush_young(vma, address, ptep)			\
 ({									\
 	pte_t __pte = *(ptep);						\
 	int __young = pte_young(__pte);					\
 	__pte = pte_mkold(__pte);					\
-	if ((vma)->vm_mm->context.pinned)				\
+	if (PagePinned(virt_to_page((vma)->vm_mm->pgd)))		\
 		(void)ptep_set_access_flags(vma, address, ptep, __pte, __young); \
 	else if (__young)						\
 		set_pte(ptep, __pte);					\
@@ -566,6 +540,8 @@ int xen_change_pte_range(struct mm_struc
 #define arch_change_pte_range(mm, pmd, addr, end, newprot, dirty_accountable) \
 	xen_change_pte_range(mm, pmd, addr, end, newprot, dirty_accountable)
 
+pte_t *lookup_address(unsigned long addr);
+
 #define io_remap_pfn_range(vma, vaddr, pfn, size, prot)		\
 		direct_remap_pfn_range(vma,vaddr,pfn,size,prot,DOMID_IO)
 
@@ -583,7 +559,6 @@ int xen_change_pte_range(struct mm_struc
    (((o) & (1UL << (__VIRTUAL_MASK_SHIFT-1))) ? ((o) | (~__VIRTUAL_MASK)) : (o))
 
 #define __HAVE_ARCH_PTEP_TEST_AND_CLEAR_YOUNG
-#define __HAVE_ARCH_PTEP_TEST_AND_CLEAR_DIRTY
 #define __HAVE_ARCH_PTEP_GET_AND_CLEAR
 #define __HAVE_ARCH_PTEP_GET_AND_CLEAR_FULL
 #define __HAVE_ARCH_PTEP_CLEAR_FLUSH
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/processor_64.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/processor_64.h	2011-01-31 17:49:31.000000000 +0100
@@ -83,7 +83,6 @@ struct cpuinfo_x86 {
 #define X86_VENDOR_UMC 3
 #define X86_VENDOR_NEXGEN 4
 #define X86_VENDOR_CENTAUR 5
-#define X86_VENDOR_RISE 6
 #define X86_VENDOR_TRANSMETA 7
 #define X86_VENDOR_NUM 8
 #define X86_VENDOR_UNKNOWN 0xff
@@ -100,6 +99,7 @@ extern char ignore_irq13;
 
 extern void identify_cpu(struct cpuinfo_x86 *);
 extern void print_cpu_info(struct cpuinfo_x86 *);
+extern void init_scattered_cpuid_features(struct cpuinfo_x86 *c);
 extern unsigned int init_intel_cacheinfo(struct cpuinfo_x86 *c);
 extern unsigned short num_cache_leaves;
 
@@ -377,12 +377,10 @@ static inline void sync_core(void)
 	asm volatile("cpuid" : "=a" (tmp) : "0" (1) : "ebx","ecx","edx","memory");
 } 
 
-#define cpu_has_fpu 1
-
 #define ARCH_HAS_PREFETCH
 static inline void prefetch(void *x) 
 { 
-	asm volatile("prefetcht0 %0" :: "m" (*(unsigned long *)x));
+	asm volatile("prefetcht0 (%0)" :: "r" (x));
 } 
 
 #define ARCH_HAS_PREFETCHW 1
@@ -400,17 +398,6 @@ static inline void prefetchw(void *x) 
 
 #define cpu_relax()   rep_nop()
 
-/*
- *      NSC/Cyrix CPU indexed register access macros
- */
-
-#define getCx86(reg) ({ outb((reg), 0x22); inb(0x23); })
-
-#define setCx86(reg, data) do { \
-	outb((reg), 0x22); \
-	outb((data), 0x23); \
-} while (0)
-
 static inline void serialize_cpu(void)
 {
 	__asm__ __volatile__ ("cpuid" : : : "ax", "bx", "cx", "dx");
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/system_64.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/system_64.h	2011-01-31 17:49:31.000000000 +0100
@@ -79,12 +79,16 @@ static inline unsigned long read_cr0(voi
 	unsigned long cr0;
 	asm volatile("movq %%cr0,%0" : "=r" (cr0));
 	return cr0;
-} 
+}
 
 static inline void write_cr0(unsigned long val) 
 { 
 	asm volatile("movq %0,%%cr0" :: "r" (val));
-} 
+}
+
+#define read_cr2() current_vcpu_info()->arch.cr2
+
+#define write_cr2(val) ((void)(current_vcpu_info()->arch.cr2 = (val)))
 
 #define read_cr3() ({ \
 	unsigned long __dummy; \
@@ -103,27 +107,28 @@ static inline unsigned long read_cr4(voi
 	unsigned long cr4;
 	asm("movq %%cr4,%0" : "=r" (cr4));
 	return cr4;
-} 
+}
 
 static inline void write_cr4(unsigned long val)
 { 
 	asm volatile("movq %0,%%cr4" :: "r" (val) : "memory");
-} 
-
-#define stts() (HYPERVISOR_fpu_taskswitch(1))
+}
 
-#define wbinvd() \
-	__asm__ __volatile__ ("wbinvd": : :"memory");
+static inline unsigned long read_cr8(void)
+{
+	return 0;
+}
 
-/*
- * On SMP systems, when the scheduler does migration-cost autodetection,
- * it needs a way to flush as much of the CPU's caches as possible.
- */
-static inline void sched_cacheflush(void)
+static inline void write_cr8(unsigned long val)
 {
-	wbinvd();
+	BUG_ON(val);
 }
 
+#define stts() (HYPERVISOR_fpu_taskswitch(1))
+
+#define wbinvd() \
+	__asm__ __volatile__ ("wbinvd": : :"memory")
+
 #endif	/* __KERNEL__ */
 
 #define nop() __asm__ __volatile__ ("nop")
--- head-2011-03-17.orig/arch/x86/include/mach-xen/asm/tlbflush_64.h	2011-01-31 17:32:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/mach-xen/asm/tlbflush_64.h	2011-01-31 17:49:31.000000000 +0100
@@ -89,7 +89,11 @@ static inline void flush_tlb_range(struc
 
 #endif
 
-#define flush_tlb_kernel_range(start, end) flush_tlb_all()
+static inline void flush_tlb_kernel_range(unsigned long start,
+					unsigned long end)
+{
+	flush_tlb_all();
+}
 
 static inline void flush_tlb_pgtables(struct mm_struct *mm,
 				      unsigned long start, unsigned long end)
--- head-2011-03-17.orig/arch/x86/include/asm/thread_info.h	2011-01-31 17:02:29.000000000 +0100
+++ head-2011-03-17/arch/x86/include/asm/thread_info.h	2011-01-31 17:49:31.000000000 +0100
@@ -151,7 +151,8 @@ struct thread_info {
 #define _TIF_WORK_CTXSW_PREV (_TIF_WORK_CTXSW|_TIF_USER_RETURN_NOTIFY)
 #define _TIF_WORK_CTXSW_NEXT (_TIF_WORK_CTXSW|_TIF_DEBUG)
 #else
-#define _TIF_WORK_CTXSW _TIF_DEBUG
+#define _TIF_WORK_CTXSW_NEXT (_TIF_NOTSC | _TIF_DEBUG)
+#define _TIF_WORK_CTXSW_PREV (_TIF_NOTSC)
 #endif
 
 #define PREEMPT_ACTIVE		0x10000000
--- head-2011-03-17.orig/arch/x86/include/asm/xen/interface.h	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/arch/x86/include/asm/xen/interface.h	2011-01-31 17:49:31.000000000 +0100
@@ -10,17 +10,20 @@
 #define _ASM_X86_XEN_INTERFACE_H
 
 #ifdef __XEN__
-#define __DEFINE_GUEST_HANDLE(name, type) \
+#define ___DEFINE_XEN_GUEST_HANDLE(name, type) \
     typedef struct { type *p; } __guest_handle_ ## name
 #else
-#define __DEFINE_GUEST_HANDLE(name, type) \
+#define ___DEFINE_XEN_GUEST_HANDLE(name, type) \
     typedef type * __guest_handle_ ## name
 #endif
 
+#define __DEFINE_XEN_GUEST_HANDLE(name, type) \
+    ___DEFINE_XEN_GUEST_HANDLE(name, type);   \
+    ___DEFINE_XEN_GUEST_HANDLE(const_##name, const type)
 #define DEFINE_GUEST_HANDLE_STRUCT(name) \
-	__DEFINE_GUEST_HANDLE(name, struct name)
-#define DEFINE_GUEST_HANDLE(name) __DEFINE_GUEST_HANDLE(name, name)
-#define GUEST_HANDLE(name)        __guest_handle_ ## name
+	__DEFINE_XEN_GUEST_HANDLE(name, struct name)
+#define DEFINE_XEN_GUEST_HANDLE(name) __DEFINE_XEN_GUEST_HANDLE(name, name)
+#define XEN_GUEST_HANDLE(name)        __guest_handle_ ## name
 
 #ifdef __XEN__
 #if defined(__i386__)
@@ -47,14 +50,8 @@
 #endif
 
 #ifndef __ASSEMBLY__
-/* Guest handles for primitive C types. */
-__DEFINE_GUEST_HANDLE(uchar, unsigned char);
-__DEFINE_GUEST_HANDLE(uint,  unsigned int);
-__DEFINE_GUEST_HANDLE(ulong, unsigned long);
-DEFINE_GUEST_HANDLE(char);
-DEFINE_GUEST_HANDLE(int);
-DEFINE_GUEST_HANDLE(long);
-DEFINE_GUEST_HANDLE(void);
+typedef unsigned long xen_pfn_t;
+typedef unsigned long xen_ulong_t;
 #endif
 
 #ifndef HYPERVISOR_VIRT_START
@@ -66,7 +63,7 @@ DEFINE_GUEST_HANDLE(void);
 #define MACH2PHYS_NR_ENTRIES  ((MACH2PHYS_VIRT_END-MACH2PHYS_VIRT_START)>>__MACH2PHYS_SHIFT)
 
 /* Maximum number of virtual CPUs in multi-processor guests. */
-#define MAX_VIRT_CPUS 32
+#define XEN_LEGACY_MAX_VCPUS 32
 
 /*
  * SEGMENT DESCRIPTOR TABLES
--- head-2011-03-17.orig/include/linux/elfnote.h	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/include/linux/elfnote.h	2011-01-31 17:49:31.000000000 +0100
@@ -52,7 +52,7 @@
 4484:.balign 4				;	\
 .popsection				;
 
-#define ELFNOTE(name, type, desc)		\
+#define ELFNOTE(name, type, desc...)		\
 	ELFNOTE_START(name, type, "")		\
 		desc			;	\
 	ELFNOTE_END
--- head-2011-03-17.orig/include/linux/page-flags.h	2011-01-31 17:01:49.000000000 +0100
+++ head-2011-03-17/include/linux/page-flags.h	2011-01-31 17:49:31.000000000 +0100
@@ -125,8 +125,15 @@ enum pageflags {
 	PG_fscache = PG_private_2,	/* page backed by cache */
 
 	/* XEN */
+#ifdef CONFIG_XEN
+	PG_pinned = PG_locked,	/* Cannot alias with PG_owner_priv_1 since
+				 * bad_page() checks should include this bit.
+				 * Also cannot use PG_arch_1 since that now
+				 * has a different purpose on x86. */
+#else
 	PG_pinned = PG_owner_priv_1,
 	PG_savepinned = PG_dirty,
+#endif
 
 	/* SLOB */
 	PG_slob_free = PG_private,
@@ -491,10 +498,8 @@ static inline int PageTransCompound(stru
 #define __PG_COMPOUND_LOCK		0
 #endif
 
-#if !defined(CONFIG_XEN)
+#ifndef CONFIG_XEN
 # define __PG_XEN		0
-#elif defined(CONFIG_X86)
-# define __PG_XEN		((1 << PG_pinned) | (1 << PG_foreign))
 #else
 # define __PG_XEN		(1 << PG_foreign)
 #endif
--- head-2011-03-17.orig/include/xen/driver_util.h	2007-06-12 13:14:19.000000000 +0200
+++ head-2011-03-17/include/xen/driver_util.h	2011-01-31 17:49:31.000000000 +0100
@@ -1,14 +1,8 @@
+#ifndef __XEN_DRIVER_UTIL_H__
+#define __XEN_DRIVER_UTIL_H__
 
-#ifndef __ASM_XEN_DRIVER_UTIL_H__
-#define __ASM_XEN_DRIVER_UTIL_H__
-
-#include <linux/vmalloc.h>
 #include <linux/device.h>
 
-/* Allocate/destroy a 'vmalloc' VM area. */
-extern struct vm_struct *alloc_vm_area(unsigned long size);
-extern void free_vm_area(struct vm_struct *area);
-
 extern struct class *get_xen_class(void);
 
-#endif /* __ASM_XEN_DRIVER_UTIL_H__ */
+#endif /* __XEN_DRIVER_UTIL_H__ */
--- head-2011-03-17.orig/include/xen/features.h	2011-03-17 13:45:28.000000000 +0100
+++ head-2011-03-17/include/xen/features.h	2011-01-31 17:49:31.000000000 +0100
@@ -10,6 +10,7 @@
 #define __XEN_FEATURES_H__
 
 #include <xen/interface/features.h>
+#include <xen/interface/version.h>
 
 void xen_setup_features(void);
 
@@ -20,4 +21,4 @@ static inline int xen_feature(int flag)
 	return xen_features[flag];
 }
 
-#endif /* __ASM_XEN_FEATURES_H__ */
+#endif /* __XEN_FEATURES_H__ */
--- head-2011-03-17.orig/include/xen/interface/arch-x86/xen.h	2011-03-17 13:50:24.000000000 +0100
+++ head-2011-03-17/include/xen/interface/arch-x86/xen.h	2011-03-17 14:11:48.000000000 +0100
@@ -50,6 +50,9 @@
 #endif
 #define set_xen_guest_handle(hnd, val) set_xen_guest_handle_raw(hnd, val)
 
+/* Allow co-existing Linux 2.6.23+ Xen interface definitions. */
+#define DEFINE_GUEST_HANDLE_STRUCT(name) struct name
+
 #if defined(__i386__)
 #include "xen-x86_32.h"
 #elif defined(__x86_64__)
--- head-2011-03-17.orig/include/xen/interface/event_channel.h	2011-01-31 15:14:12.000000000 +0100
+++ head-2011-03-17/include/xen/interface/event_channel.h	2011-01-31 17:49:31.000000000 +0100
@@ -250,6 +250,7 @@ struct evtchn_op {
         struct evtchn_unmask           unmask;
     } u;
 };
+DEFINE_GUEST_HANDLE_STRUCT(evtchn_op);
 typedef struct evtchn_op evtchn_op_t;
 DEFINE_XEN_GUEST_HANDLE(evtchn_op_t);
 
--- head-2011-03-17.orig/include/xen/interface/io/netif.h	2011-01-31 15:14:12.000000000 +0100
+++ head-2011-03-17/include/xen/interface/io/netif.h	2011-01-31 17:49:31.000000000 +0100
@@ -183,8 +183,22 @@ typedef struct netif_rx_response netif_r
  * Generate netif ring structures and types.
  */
 
+#if defined(CONFIG_XEN) || defined(HAVE_XEN_PLATFORM_COMPAT_H)
 DEFINE_RING_TYPES(netif_tx, struct netif_tx_request, struct netif_tx_response);
 DEFINE_RING_TYPES(netif_rx, struct netif_rx_request, struct netif_rx_response);
+#else
+#define xen_netif_tx_request netif_tx_request
+#define xen_netif_rx_request netif_rx_request
+#define xen_netif_tx_response netif_tx_response
+#define xen_netif_rx_response netif_rx_response
+DEFINE_RING_TYPES(xen_netif_tx,
+		  struct xen_netif_tx_request,
+		  struct xen_netif_tx_response);
+DEFINE_RING_TYPES(xen_netif_rx,
+		  struct xen_netif_rx_request,
+		  struct xen_netif_rx_response);
+#define xen_netif_extra_info netif_extra_info
+#endif
 
 #define NETIF_RSP_DROPPED         -2
 #define NETIF_RSP_ERROR           -1
--- head-2011-03-17.orig/include/xen/interface/memory.h	2011-01-31 15:14:12.000000000 +0100
+++ head-2011-03-17/include/xen/interface/memory.h	2011-01-31 17:49:31.000000000 +0100
@@ -88,6 +88,7 @@ struct xen_memory_reservation {
      */
     domid_t        domid;
 };
+DEFINE_GUEST_HANDLE_STRUCT(xen_memory_reservation);
 typedef struct xen_memory_reservation xen_memory_reservation_t;
 DEFINE_XEN_GUEST_HANDLE(xen_memory_reservation_t);
 
@@ -181,6 +182,7 @@ struct xen_machphys_mfn_list {
      */
     unsigned int nr_extents;
 };
+DEFINE_GUEST_HANDLE_STRUCT(xen_machphys_mfn_list);
 typedef struct xen_machphys_mfn_list xen_machphys_mfn_list_t;
 DEFINE_XEN_GUEST_HANDLE(xen_machphys_mfn_list_t);
 
@@ -222,6 +224,7 @@ struct xen_add_to_physmap {
     /* GPFN where the source mapping page should appear. */
     xen_pfn_t     gpfn;
 };
+DEFINE_GUEST_HANDLE_STRUCT(xen_add_to_physmap);
 typedef struct xen_add_to_physmap xen_add_to_physmap_t;
 DEFINE_XEN_GUEST_HANDLE(xen_add_to_physmap_t);
 
--- head-2011-03-17.orig/include/xen/interface/sched.h	2011-01-31 15:14:12.000000000 +0100
+++ head-2011-03-17/include/xen/interface/sched.h	2011-01-31 17:49:31.000000000 +0100
@@ -67,6 +67,7 @@
 struct sched_shutdown {
     unsigned int reason; /* SHUTDOWN_* */
 };
+DEFINE_GUEST_HANDLE_STRUCT(sched_shutdown);
 typedef struct sched_shutdown sched_shutdown_t;
 DEFINE_XEN_GUEST_HANDLE(sched_shutdown_t);
 
@@ -81,6 +82,7 @@ struct sched_poll {
     unsigned int nr_ports;
     uint64_t timeout;
 };
+DEFINE_GUEST_HANDLE_STRUCT(sched_poll);
 typedef struct sched_poll sched_poll_t;
 DEFINE_XEN_GUEST_HANDLE(sched_poll_t);
 
--- head-2011-03-17.orig/include/xen/interface/version.h	2011-01-31 15:14:12.000000000 +0100
+++ head-2011-03-17/include/xen/interface/version.h	2011-01-31 17:49:31.000000000 +0100
@@ -36,6 +36,9 @@
 /* arg == xen_extraversion_t. */
 #define XENVER_extraversion 1
 typedef char xen_extraversion_t[16];
+struct xen_extraversion {
+    xen_extraversion_t extraversion;
+};
 #define XEN_EXTRAVERSION_LEN (sizeof(xen_extraversion_t))
 
 /* arg == xen_compile_info_t. */
@@ -50,10 +53,16 @@ typedef struct xen_compile_info xen_comp
 
 #define XENVER_capabilities 3
 typedef char xen_capabilities_info_t[1024];
+struct xen_capabilities_info {
+    xen_capabilities_info_t info;
+};
 #define XEN_CAPABILITIES_INFO_LEN (sizeof(xen_capabilities_info_t))
 
 #define XENVER_changeset 4
 typedef char xen_changeset_info_t[64];
+struct xen_changeset_info {
+    xen_changeset_info_t info;
+};
 #define XEN_CHANGESET_INFO_LEN (sizeof(xen_changeset_info_t))
 
 #define XENVER_platform_parameters 5
--- head-2011-03-17.orig/include/xen/interface/xen.h	2011-03-17 13:50:24.000000000 +0100
+++ head-2011-03-17/include/xen/interface/xen.h	2011-03-17 14:12:10.000000000 +0100
@@ -32,7 +32,9 @@
 #include <asm/pvclock-abi.h>
 #endif
 
-#if defined(__i386__) || defined(__x86_64__)
+#if defined(CONFIG_PARAVIRT_XEN) && !defined(HAVE_XEN_PLATFORM_COMPAT_H)
+#include <asm/xen/interface.h>
+#elif defined(__i386__) || defined(__x86_64__)
 #include "arch-x86/xen.h"
 #elif defined(__ia64__)
 #include "arch-ia64.h"
@@ -112,7 +114,7 @@ DEFINE_XEN_GUEST_HANDLE(xen_pfn_t);
  */
 
 /* New sched_op hypercall introduced in 0x00030101. */
-#if __XEN_INTERFACE_VERSION__ < 0x00030101
+#if __XEN_INTERFACE_VERSION__ < 0x00030101 || (defined(CONFIG_PARAVIRT_XEN) && !defined(HAVE_XEN_PLATFORM_COMPAT_H))
 #undef __HYPERVISOR_sched_op
 #define __HYPERVISOR_sched_op __HYPERVISOR_sched_op_compat
 #else
@@ -128,7 +130,7 @@ DEFINE_XEN_GUEST_HANDLE(xen_pfn_t);
 #endif
 
 /* New platform_op hypercall introduced in 0x00030204. */
-#if __XEN_INTERFACE_VERSION__ < 0x00030204
+#if __XEN_INTERFACE_VERSION__ < 0x00030204 || (defined(CONFIG_PARAVIRT_XEN) && !defined(HAVE_XEN_PLATFORM_COMPAT_H))
 #define __HYPERVISOR_dom0_op __HYPERVISOR_platform_op
 #endif
 
@@ -307,6 +309,7 @@ struct mmuext_op {
         xen_pfn_t src_mfn;
     } arg2;
 };
+DEFINE_GUEST_HANDLE_STRUCT(mmuext_op);
 typedef struct mmuext_op mmuext_op_t;
 DEFINE_XEN_GUEST_HANDLE(mmuext_op_t);
 #endif
@@ -399,6 +402,7 @@ struct mmu_update {
     uint64_t ptr;       /* Machine address of PTE. */
     uint64_t val;       /* New contents of PTE.    */
 };
+DEFINE_GUEST_HANDLE_STRUCT(mmu_update);
 typedef struct mmu_update mmu_update_t;
 DEFINE_XEN_GUEST_HANDLE(mmu_update_t);
 
@@ -407,9 +411,15 @@ DEFINE_XEN_GUEST_HANDLE(mmu_update_t);
  * NB. The fields are natural register size for this architecture.
  */
 struct multicall_entry {
-    unsigned long op, result;
+    unsigned long op;
+#if !defined(CONFIG_PARAVIRT_XEN) || defined(HAVE_XEN_PLATFORM_COMPAT_H)
+    unsigned long result;
+#else
+    long result;
+#endif
     unsigned long args[6];
 };
+DEFINE_GUEST_HANDLE_STRUCT(multicall_entry);
 typedef struct multicall_entry multicall_entry_t;
 DEFINE_XEN_GUEST_HANDLE(multicall_entry_t);
 
--- head-2011-03-17.orig/include/xen/xenbus.h	2011-01-31 17:32:22.000000000 +0100
+++ head-2011-03-17/include/xen/xenbus.h	2011-01-31 17:49:31.000000000 +0100
@@ -57,16 +57,20 @@ struct xenbus_watch
 	void (*callback)(struct xenbus_watch *,
 			 const char **vec, unsigned int len);
 
+#if defined(CONFIG_XEN) || defined(HAVE_XEN_PLATFORM_COMPAT_H)
 	/* See XBWF_ definitions below. */
 	unsigned long flags;
+#endif
 };
 
+#if defined(CONFIG_XEN) || defined(HAVE_XEN_PLATFORM_COMPAT_H)
 /*
  * Execute callback in its own kthread. Useful if the callback is long
  * running or heavily serialised, to avoid taking out the main xenwatch thread
  * for a long period of time (or even unwittingly causing a deadlock).
  */
 #define XBWF_new_thread	1
+#endif
 
 /* A xenbus device. */
 struct xenbus_device {
@@ -184,6 +188,9 @@ void xs_suspend_cancel(void);
 /* Used by xenbus_dev to borrow kernel's store connection. */
 void *xenbus_dev_request_and_reply(struct xsd_sockmsg *msg);
 
+struct work_struct;
+void xenbus_probe(struct work_struct *);
+
 /* Prepare for domain suspend: then resume or cancel the suspend. */
 void xenbus_suspend(void);
 void xenbus_resume(void);
@@ -214,6 +221,7 @@ int xenbus_watch_path(struct xenbus_devi
 				       const char **, unsigned int));
 
 
+#if defined(CONFIG_XEN) || defined(HAVE_XEN_PLATFORM_COMPAT_H)
 /**
  * Register a watch on the given path/path2, using the given xenbus_watch
  * structure for storage, and the given callback function as the callback.
@@ -227,7 +235,13 @@ int xenbus_watch_path2(struct xenbus_dev
 		       const char *path2, struct xenbus_watch *watch,
 		       void (*callback)(struct xenbus_watch *,
 					const char **, unsigned int));
-
+#else
+int xenbus_watch_pathfmt(struct xenbus_device *dev, struct xenbus_watch *watch,
+			 void (*callback)(struct xenbus_watch *,
+					  const char **, unsigned int),
+			 const char *pathfmt, ...)
+	__attribute__ ((format (printf, 4, 5)));
+#endif
 
 /**
  * Advertise in the store a change of the given driver to the given new_state.
