From: Peter Zijlstra <a.p.zijlstra@chello.nl> 
Subject: [PATCH 22/31] netvm: skb processing
Patch-mainline: Not yet

In order to make sure emergency packets receive all memory needed to proceed
ensure processing of emergency SKBs happens under PF_MEMALLOC.

Use the (new) sk_backlog_rcv() wrapper to ensure this for backlog processing.

Skip taps, since those are user-space again.

Signed-off-by: Peter Zijlstra <a.p.zijlstra@chello.nl>
Signed-off-by: Suresh Jayaraman <sjayaraman@suse.de>
---
 include/net/sock.h |    5 ++++
 net/core/dev.c     |   57 ++++++++++++++++++++++++++++++++++++++++++++++++-----
 net/core/sock.c    |   16 ++++++++++++++
 3 files changed, 73 insertions(+), 5 deletions(-)

--- a/include/net/sock.h
+++ b/include/net/sock.h
@@ -660,8 +660,13 @@ static inline __must_check int sk_add_ba
 	return 0;
 }
 
+extern int __sk_backlog_rcv(struct sock *sk, struct sk_buff *skb);
+
 static inline int sk_backlog_rcv(struct sock *sk, struct sk_buff *skb)
 {
+	if (skb_emergency(skb))
+		return __sk_backlog_rcv(sk, skb);
+
 	return sk->sk_backlog_rcv(sk, skb);
 }
 
--- a/net/core/dev.c
+++ b/net/core/dev.c
@@ -2464,6 +2464,30 @@ void netif_nit_deliver(struct sk_buff *s
 	rcu_read_unlock();
 }
 
+/*
+ * Filter the protocols for which the reserves are adequate.
+ *
+ * Before adding a protocol make sure that it is either covered by the existing
+ * reserves, or add reserves covering the memory need of the new protocol's
+ * packet processing.
+ */
+static int skb_emergency_protocol(struct sk_buff *skb)
+{
+	if (skb_emergency(skb))
+		switch (skb->protocol) {
+		case __constant_htons(ETH_P_ARP):
+		case __constant_htons(ETH_P_IP):
+		case __constant_htons(ETH_P_IPV6):
+		case __constant_htons(ETH_P_8021Q):
+			break;
+
+		default:
+			return 0;
+		}
+
+	return 1;
+}
+
 /**
  *	netif_receive_skb - process receive buffer from network
  *	@skb: buffer to process
@@ -2487,6 +2511,7 @@ int netif_receive_skb(struct sk_buff *sk
 	struct net_device *null_or_bond;
 	int ret = NET_RX_DROP;
 	__be16 type;
+	unsigned long pflags = current->flags;
 
 	if (!skb->tstamp.tv64)
 		net_timestamp(skb);
@@ -2494,9 +2519,21 @@ int netif_receive_skb(struct sk_buff *sk
 	if (vlan_tx_tag_present(skb) && vlan_hwaccel_do_receive(skb))
 		return NET_RX_SUCCESS;
 
+	/* Emergency skb are special, they should
+	 * - be delivered to SOCK_MEMALLOC sockets only
+	 * - stay away from userspace
+	 * - have bounded memory usage
+	 *
+	 * Use PF_MEMALLOC as a poor mans memory pool - the grouping kind.
+	 * This saves us from propagating the allocation context down to all
+	 * allocation sites.
+	 */
+	if (skb_emergency(skb))
+		current->flags |= PF_MEMALLOC;
+
 	/* if we've gotten here through NAPI, check netpoll */
 	if (netpoll_receive_skb(skb))
-		return NET_RX_DROP;
+		goto out;
 
 	if (!skb->skb_iif)
 		skb->skb_iif = skb->dev->ifindex;
@@ -2527,6 +2564,9 @@ int netif_receive_skb(struct sk_buff *sk
 	}
 #endif
 
+	if (skb_emergency(skb))
+		goto skip_taps;
+
 	list_for_each_entry_rcu(ptype, &ptype_all, list) {
 		if (ptype->dev == null_or_orig || ptype->dev == skb->dev ||
 		    ptype->dev == orig_dev) {
@@ -2536,19 +2576,23 @@ int netif_receive_skb(struct sk_buff *sk
 		}
 	}
 
+skip_taps:
 #ifdef CONFIG_NET_CLS_ACT
 	skb = handle_ing(skb, &pt_prev, &ret, orig_dev);
 	if (!skb)
-		goto out;
+		goto unlock;
 ncls:
 #endif
 
+	if (!skb_emergency_protocol(skb))
+		goto drop;
+
 	skb = handle_bridge(skb, &pt_prev, &ret, orig_dev);
 	if (!skb)
-		goto out;
+		goto unlock;
 	skb = handle_macvlan(skb, &pt_prev, &ret, orig_dev);
 	if (!skb)
-		goto out;
+		goto unlock;
 
 	/*
 	 * Make sure frames received on VLAN interfaces stacked on
@@ -2577,6 +2621,7 @@ ncls:
 	if (pt_prev) {
 		ret = pt_prev->func(skb, skb->dev, pt_prev, orig_dev);
 	} else {
+drop:
 		kfree_skb(skb);
 		/* Jamal, now you will not able to escape explaining
 		 * me how you were going to use this. :-)
@@ -2584,8 +2629,10 @@ ncls:
 		ret = NET_RX_DROP;
 	}
 
-out:
+unlock:
 	rcu_read_unlock();
+out:
+	tsk_restore_flags(current, pflags, PF_MEMALLOC);
 	return ret;
 }
 EXPORT_SYMBOL(netif_receive_skb);
--- a/net/core/sock.c
+++ b/net/core/sock.c
@@ -315,6 +315,22 @@ int sk_clear_memalloc(struct sock *sk)
 	return set;
 }
 EXPORT_SYMBOL_GPL(sk_clear_memalloc);
+
+int __sk_backlog_rcv(struct sock *sk, struct sk_buff *skb)
+{
+	int ret;
+	unsigned long pflags = current->flags;
+
+	/* these should have been dropped before queueing */
+	BUG_ON(!sk_has_memalloc(sk));
+
+	current->flags |= PF_MEMALLOC;
+	ret = sk->sk_backlog_rcv(sk, skb);
+	tsk_restore_flags(current, pflags, PF_MEMALLOC);
+
+	return ret;
+}
+EXPORT_SYMBOL(__sk_backlog_rcv);
 #endif
 
 static int sock_set_timeout(long *timeo_p, char __user *optval, int optlen)
