From: Thomas Renninger <trenn@suse.de>
Subject: x86 platform drivers: hp-wmi Add media key 0x20e8
References: bnc#598059
Patch-Mainline: submitted

Signed-off-by: Thomas Renninger <trenn@suse.de>
CC: mjg@redhat.com
CC: linux-acpi@vger.kernel.org

---
 drivers/platform/x86/hp-wmi.c |    1 +
 1 file changed, 1 insertion(+)

Index: linux-2.6.33-master/drivers/platform/x86/hp-wmi.c
===================================================================
--- linux-2.6.33-master.orig/drivers/platform/x86/hp-wmi.c
+++ linux-2.6.33-master/drivers/platform/x86/hp-wmi.c
@@ -96,6 +96,7 @@ static struct key_entry hp_wmi_keymap[]
 	{KE_KEY, 0x02, KEY_BRIGHTNESSUP},
 	{KE_KEY, 0x03, KEY_BRIGHTNESSDOWN},
 	{KE_KEY, 0x20e6, KEY_PROG1},
+	{KE_KEY, 0x20e8, KEY_MEDIA},
 	{KE_KEY, 0x2142, KEY_MEDIA},
 	{KE_KEY, 0x213b, KEY_INFO},
 	{KE_KEY, 0x2169, KEY_DIRECTION},
