From: Jeff Mahoney <jeffm@suse.com>
Subject: tioca: Fix assignment from incompatible pointer warnings
Patch-mainline: not yet

 The prototype for sn_pci_provider->{dma_map,dma_map_consistent} expects
 an unsigned long instead of a u64.

Signed-off-by: Jeff Mahoney <jeffm@suse.com>
---
 arch/ia64/sn/pci/tioca_provider.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/ia64/sn/pci/tioca_provider.c
+++ b/arch/ia64/sn/pci/tioca_provider.c
@@ -508,7 +508,7 @@ tioca_dma_unmap(struct pci_dev *pdev, dm
  * use the GART mapped mode.
  */
 static u64
-tioca_dma_map(struct pci_dev *pdev, u64 paddr, size_t byte_count, int dma_flags)
+tioca_dma_map(struct pci_dev *pdev, unsigned long paddr, size_t byte_count, int dma_flags)
 {
 	u64 mapaddr;
 
