From: Andi Kleen <andi@firstfloor.org>
Subject: x86, mce: Xeon75xx specific interface to get corrected memory error information
Patch-Mainline: submitted to x86-tip, added but reverted due to a minor compile issue
		which gets fixed by this patch
References: bnc#573380, fate#307738

http://lkml.org/lkml/2010/1/23/50

Signed-off-by: Thomas Renninger <trenn@suse.de>

---
 arch/x86/Kconfig |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/x86/Kconfig
+++ b/arch/x86/Kconfig
@@ -921,7 +921,7 @@ config X86_MCE_INTEL
 
 config X86_MCE_XEON75XX
 	tristate "Intel Xeon 7500 series corrected memory error driver"
-	depends on X86_MCE_INTEL
+	depends on X86_MCE_INTEL && PCI
 	---help---
 	   Add support for a Intel Xeon 7500 series specific memory error driver.
 	   This allows to report the DIMM and physical address on a corrected
