From: Jeff Mahoney <jeffm@suse.com>
Subject: dmar: Fix section mismatch
Patch-mainline: Next linux-next sync
Git-repo: git://git.kernel.org/pub/scm/linux/kernel/git/sfr/linux-next.git
Git-commit: 0b8973a81876d90f916507ac40d1381068dc986a

 dmar_ir_support uses dmar_tbl, which is __initdata. dmar_ir_support is
 only called by intr_remapping_supported, which is __init. So, we mark
 dmar_ir_support as __init as well.

Signed-off-by: Jeff Mahoney <jeffm@suse.com>
---
 drivers/pci/dmar.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/pci/dmar.c
+++ b/drivers/pci/dmar.c
@@ -1456,7 +1456,7 @@ int dmar_reenable_qi(struct intel_iommu
 /*
  * Check interrupt remapping support in DMAR table description.
  */
-int dmar_ir_support(void)
+int __init dmar_ir_support(void)
 {
 	struct acpi_table_dmar *dmar;
 	dmar = (struct acpi_table_dmar *)dmar_tbl;
