From: Rafael J. Wysocki <rjw@suse.de>
Subject: net (tg3): Fix failure to enable WoL by default when possible
References: bnc#447371
Patch-mainline: not yet

tg3 is supposed to enable WoL by default on adapters which support
that, but it fails to do so unless the adapter's
/sys/devices/.../power/wakeup file contains 'enabled' during the
initialization of the adapter.  Fix that by making tg3 update the
device's 'should_wakeup' bit automatically whenever WoL should be
enabled by default.

Signed-off-by: Rafael J. Wysocki <rjw@suse.de>
---
 drivers/net/tg3.c |    8 ++++++--
 1 file changed, 6 insertions(+), 2 deletions(-)

--- a/drivers/net/tg3.c
+++ b/drivers/net/tg3.c
@@ -12048,8 +12048,10 @@ static void __devinit tg3_get_eeprom_hw_
 		if (val & VCPU_CFGSHDW_ASPM_DBNC)
 			tp->tg3_flags |= TG3_FLAG_ASPM_WORKAROUND;
 		if ((val & VCPU_CFGSHDW_WOL_ENABLE) &&
-		    (val & VCPU_CFGSHDW_WOL_MAGPKT))
+		    (val & VCPU_CFGSHDW_WOL_MAGPKT)) {
 			tp->tg3_flags |= TG3_FLAG_WOL_ENABLE;
+			device_set_wakeup_enable(&tp->pdev->dev, true);
+		}
 		goto done;
 	}
 
@@ -12182,8 +12184,10 @@ static void __devinit tg3_get_eeprom_hw_
 			tp->tg3_flags &= ~TG3_FLAG_WOL_CAP;
 
 		if ((tp->tg3_flags & TG3_FLAG_WOL_CAP) &&
-		    (nic_cfg & NIC_SRAM_DATA_CFG_WOL_ENABLE))
+		    (nic_cfg & NIC_SRAM_DATA_CFG_WOL_ENABLE)) {
 			tp->tg3_flags |= TG3_FLAG_WOL_ENABLE;
+			device_set_wakeup_enable(&tp->pdev->dev, true);
+		}
 
 		if (cfg2 & (1 << 17))
 			tp->phy_flags |= TG3_PHYFLG_CAPACITIVE_COUPLING;
