From: Kurt Garloff <garloff@suse.de>
Subject: Add BLIST_REPORTLUN2 to EMC SYMMETRIX
Patch-mainline: not yet
References: bnc#185164, bnc#191648, bnc#505578

All EMC SYMMETRIX support REPORT_LUNS, even if configured to report
SCSI-2 for whatever reason.

Signed-off-by: Kurt Garloff <garloff@suse.de>
Signed-off-by: Hannes Reinecke <hare@suse.de>

---
 drivers/scsi/scsi_devinfo.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/scsi/scsi_devinfo.c
+++ b/drivers/scsi/scsi_devinfo.c
@@ -160,7 +160,7 @@ static struct {
 	{"DGC", "RAID", NULL, BLIST_SPARSELUN},	/* Dell PV 650F, storage on LUN 0 */
 	{"DGC", "DISK", NULL, BLIST_SPARSELUN},	/* Dell PV 650F, no storage on LUN 0 */
 	{"EMC",  "Invista", "*", BLIST_SPARSELUN | BLIST_LARGELUN},
-	{"EMC", "SYMMETRIX", NULL, BLIST_SPARSELUN | BLIST_LARGELUN | BLIST_FORCELUN},
+	{"EMC", "SYMMETRIX", NULL, BLIST_SPARSELUN | BLIST_LARGELUN | BLIST_REPORTLUN2},
 	{"EMULEX", "MD21/S2     ESDI", NULL, BLIST_SINGLELUN},
 	{"easyRAID", "16P", NULL, BLIST_NOREPORTLUN},
 	{"easyRAID", "X6P", NULL, BLIST_NOREPORTLUN},
