From: Jeff Mahoney <jeffm@suse.com>
Subject: dmraid45: dm_get_device takes fewer arguments
Patch-mainline: Whenever dmraid45 is

 With 2.6.34-rc1, dm_get_device takes 4 args instead of 6.

Signed-off-by: Jeff Mahoney <jeffm@suse.com>
Acked-by: Jeff Mahoney <jeffm@suse.com>
---
 drivers/md/dm-raid45.c |    5 ++---
 1 file changed, 2 insertions(+), 3 deletions(-)

--- a/drivers/md/dm-raid45.c
+++ b/drivers/md/dm-raid45.c
@@ -3810,9 +3810,8 @@ DMINFO("rs->set.sectors_per_dev=%llu", (
 			TI_ERR("Invalid RAID device offset parameter");
 
 		dev->start = tmp;
-		r = dm_get_device(ti, argv[0], dev->start,
-				  rs->set.sectors_per_dev,
-				  dm_table_get_mode(ti->table), &dev->dev);
+		r = dm_get_device(ti, argv[0], dm_table_get_mode(ti->table),
+				  &dev->dev);
 		if (r)
 			TI_ERR_RET("RAID device lookup failure", r);
 
