From: someone at intel <someone@intel.com>
Subject: make kms happen after sata
Patch-mainline: not yet

I guess this speeds something up, would be nice if we had some descriptions here...


Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>


---
 drivers/Makefile |   14 +++++++-------
 1 file changed, 7 insertions(+), 7 deletions(-)

--- a/drivers/Makefile
+++ b/drivers/Makefile
@@ -28,15 +28,8 @@ obj-$(CONFIG_REGULATOR)		+= regulator/
 obj-y				+= tty/
 obj-y				+= char/
 
-# gpu/ comes after char for AGP vs DRM startup
-obj-y				+= gpu/
-
 obj-$(CONFIG_CONNECTOR)		+= connector/
 
-# i810fb and intelfb depend on char/agp/
-obj-$(CONFIG_FB_I810)           += video/i810/
-obj-$(CONFIG_FB_INTEL)          += video/intelfb/
-
 obj-$(CONFIG_PARPORT)		+= parport/
 obj-y				+= base/ block/ misc/ mfd/ nfc/
 obj-$(CONFIG_NUBUS)		+= nubus/
@@ -48,6 +41,13 @@ obj-$(CONFIG_ATA)		+= ata/
 obj-$(CONFIG_MTD)		+= mtd/
 obj-$(CONFIG_SPI)		+= spi/
 obj-y				+= net/
+
+# gpu/ comes after char for AGP vs DRM startup
+obj-y				+= gpu/
+# i810fb and intelfb depend on char/agp/
+obj-$(CONFIG_FB_I810)           += video/i810/
+obj-$(CONFIG_FB_INTEL)          += video/intelfb/
+
 obj-$(CONFIG_ATM)		+= atm/
 obj-$(CONFIG_FUSION)		+= message/
 obj-y				+= firewire/
