From foo@baz Wed Feb  9 13:35:10 PST 2011
Date: Wed, 09 Feb 2011 13:35:10 -0800
To: Greg KH <greg@kroah.com>
From: Greg Kroah-Hartman <gregkh@suse.de>
Subject: Staging: samsung-laptop: add support for lots of laptops
References: bnc#661682
Patch-mainline: 2.6.39

This is a backport of the upstream version of the driver that added support for
all samsung laptop devices.

Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>

diff --git a/drivers/staging/samsung-laptop/samsung-laptop.c b/drivers/staging/samsung-laptop/samsung-laptop.c
index 701e8d5..51ec621 100644
--- a/drivers/staging/samsung-laptop/samsung-laptop.c
+++ b/drivers/staging/samsung-laptop/samsung-laptop.c
@@ -1,5 +1,5 @@
 /*
- * Samsung N130 Laptop driver
+ * Samsung Laptop driver
  *
  * Copyright (C) 2009 Greg Kroah-Hartman (gregkh@suse.de)
  * Copyright (C) 2009 Novell Inc.
@@ -33,51 +33,6 @@
  */
 #define MAX_BRIGHT	0x07
 
-/* Brightness is 0 - 8, as described above.  Value 0 is for the BIOS to use */
-#define GET_BRIGHTNESS			0x00
-#define SET_BRIGHTNESS			0x01
-
-/* first byte:
- * 0x00 - wireless is off
- * 0x01 - wireless is on
- * second byte:
- * 0x02 - 3G is off
- * 0x03 - 3G is on
- * TODO, verify 3G is correct, that doesn't seem right...
- */
-#define GET_WIRELESS_BUTTON		0x02
-#define SET_WIRELESS_BUTTON		0x03
-
-/* 0 is off, 1 is on */
-#define GET_BACKLIGHT			0x04
-#define SET_BACKLIGHT			0x05
-
-/*
- * 0x80 or 0x00 - no action
- * 0x81 - recovery key pressed
- */
-#define GET_RECOVERY_METHOD		0x06
-#define SET_RECOVERY_METHOD		0x07
-
-/* 0 is low, 1 is high */
-#define GET_PERFORMANCE_LEVEL		0x08
-#define SET_PERFORMANCE_LEVEL		0x09
-
-/*
- * Tell the BIOS that Linux is running on this machine.
- * 81 is on, 80 is off
- */
-#define SET_LINUX			0x0a
-
-
-#define MAIN_FUNCTION			0x4c49
-
-#define SABI_HEADER_PORT		0x00
-#define SABI_HEADER_RE_MEM		0x02
-#define SABI_HEADER_IFACEFUNC		0x03
-#define SABI_HEADER_EN_MEM		0x04
-#define SABI_HEADER_DATA_OFFSET		0x05
-#define SABI_HEADER_DATA_SEGMENT	0x07
 
 #define SABI_IFACE_MAIN			0x00
 #define SABI_IFACE_SUB			0x02
@@ -89,6 +44,173 @@ struct sabi_retval {
 	u8 retval[20];
 };
 
+struct sabi_header_offsets {
+	u8 port;
+	u8 re_mem;
+	u8 iface_func;
+	u8 en_mem;
+	u8 data_offset;
+	u8 data_segment;
+};
+
+struct sabi_commands {
+	/*
+	 * Brightness is 0 - 8, as described above.
+	 * Value 0 is for the BIOS to use
+	 */
+	u8 get_brightness;
+	u8 set_brightness;
+
+	/*
+	 * first byte:
+	 * 0x00 - wireless is off
+	 * 0x01 - wireless is on
+	 * second byte:
+	 * 0x02 - 3G is off
+	 * 0x03 - 3G is on
+	 * TODO, verify 3G is correct, that doesn't seem right...
+	 */
+	u8 get_wireless_button;
+	u8 set_wireless_button;
+
+	/* 0 is off, 1 is on */
+	u8 get_backlight;
+	u8 set_backlight;
+
+	/*
+	 * 0x80 or 0x00 - no action
+	 * 0x81 - recovery key pressed
+	 */
+	u8 get_recovery_mode;
+	u8 set_recovery_mode;
+
+	/*
+	 * on seclinux: 0 is low, 1 is high,
+	 * on swsmi: 0 is normal, 1 is silent, 2 is turbo
+	 */
+	u8 get_performance_level;
+	u8 set_performance_level;
+
+	/*
+	 * Tell the BIOS that Linux is running on this machine.
+	 * 81 is on, 80 is off
+	 */
+	u8 set_linux;
+};
+
+struct sabi_performance_level {
+	const char *name;
+	u8 value;
+};
+
+struct sabi_config {
+	const char *test_string;
+	u16 main_function;
+	struct sabi_header_offsets header_offsets;
+	struct sabi_commands commands;
+	struct sabi_performance_level performance_levels[4];
+};
+
+static struct sabi_config sabi_configs[] = {
+	{
+		.test_string = "SECLINUX",
+
+		.main_function = 0x4c59,
+
+		.header_offsets = {
+			.port = 0x00,
+			.re_mem = 0x02,
+			.iface_func = 0x03,
+			.en_mem = 0x04,
+			.data_offset = 0x05,
+			.data_segment = 0x07,
+		},
+
+		.commands = {
+			.get_brightness = 0x00,
+			.set_brightness = 0x01,
+
+			.get_wireless_button = 0x02,
+			.set_wireless_button = 0x03,
+
+			.get_backlight = 0x04,
+			.set_backlight = 0x05,
+
+			.get_recovery_mode = 0x06,
+			.set_recovery_mode = 0x07,
+
+			.get_performance_level = 0x08,
+			.set_performance_level = 0x09,
+
+			.set_linux = 0x0a,
+		},
+
+		.performance_levels = {
+			{
+				.name = "silent",
+				.value = 0,
+			},
+			{
+				.name = "normal",
+				.value = 1,
+			},
+			{ },
+		},
+	},
+	{
+		.test_string = "SwSmi@",
+
+		.main_function = 0x5843,
+
+		.header_offsets = {
+			.port = 0x00,
+			.re_mem = 0x04,
+			.iface_func = 0x02,
+			.en_mem = 0x03,
+			.data_offset = 0x05,
+			.data_segment = 0x07,
+		},
+
+		.commands = {
+			.get_brightness = 0x10,
+			.set_brightness = 0x11,
+
+			.get_wireless_button = 0x12,
+			.set_wireless_button = 0x13,
+
+			.get_backlight = 0x2d,
+			.set_backlight = 0x2e,
+
+			.get_recovery_mode = 0xff,
+			.set_recovery_mode = 0xff,
+
+			.get_performance_level = 0x31,
+			.set_performance_level = 0x32,
+
+			.set_linux = 0xff,
+		},
+
+		.performance_levels = {
+			{
+				.name = "normal",
+				.value = 0,
+			},
+			{
+				.name = "silent",
+				.value = 1,
+			},
+			{
+				.name = "overclock",
+				.value = 2,
+			},
+			{ },
+		},
+	},
+	{ },
+};
+
+static struct sabi_config *sabi_config;
+
 static void __iomem *sabi;
 static void __iomem *sabi_iface;
 static void __iomem *f0000_segment;
@@ -109,21 +231,21 @@ MODULE_PARM_DESC(debug, "Debug enabled or not");
 static int sabi_get_command(u8 command, struct sabi_retval *sretval)
 {
 	int retval = 0;
-	u16 port = readw(sabi + SABI_HEADER_PORT);
+	u16 port = readw(sabi + sabi_config->header_offsets.port);
 
 	mutex_lock(&sabi_mutex);
 
 	/* enable memory to be able to write to it */
-	outb(readb(sabi + SABI_HEADER_EN_MEM), port);
+	outb(readb(sabi + sabi_config->header_offsets.en_mem), port);
 
 	/* write out the command */
-	writew(MAIN_FUNCTION, sabi_iface + SABI_IFACE_MAIN);
+	writew(sabi_config->main_function, sabi_iface + SABI_IFACE_MAIN);
 	writew(command, sabi_iface + SABI_IFACE_SUB);
 	writeb(0, sabi_iface + SABI_IFACE_COMPLETE);
-	outb(readb(sabi + SABI_HEADER_IFACEFUNC), port);
+	outb(readb(sabi + sabi_config->header_offsets.iface_func), port);
 
 	/* write protect memory to make it safe */
-	outb(readb(sabi + SABI_HEADER_RE_MEM), port);
+	outb(readb(sabi + sabi_config->header_offsets.re_mem), port);
 
 	/* see if the command actually succeeded */
 	if (readb(sabi_iface + SABI_IFACE_COMPLETE) == 0xaa &&
@@ -156,22 +278,22 @@ exit:
 static int sabi_set_command(u8 command, u8 data)
 {
 	int retval = 0;
-	u16 port = readw(sabi + SABI_HEADER_PORT);
+	u16 port = readw(sabi + sabi_config->header_offsets.port);
 
 	mutex_lock(&sabi_mutex);
 
 	/* enable memory to be able to write to it */
-	outb(readb(sabi + SABI_HEADER_EN_MEM), port);
+	outb(readb(sabi + sabi_config->header_offsets.en_mem), port);
 
 	/* write out the command */
-	writew(MAIN_FUNCTION, sabi_iface + SABI_IFACE_MAIN);
+	writew(sabi_config->main_function, sabi_iface + SABI_IFACE_MAIN);
 	writew(command, sabi_iface + SABI_IFACE_SUB);
 	writeb(0, sabi_iface + SABI_IFACE_COMPLETE);
 	writeb(data, sabi_iface + SABI_IFACE_DATA);
-	outb(readb(sabi + SABI_HEADER_IFACEFUNC), port);
+	outb(readb(sabi + sabi_config->header_offsets.iface_func), port);
 
 	/* write protect memory to make it safe */
-	outb(readb(sabi + SABI_HEADER_RE_MEM), port);
+	outb(readb(sabi + sabi_config->header_offsets.re_mem), port);
 
 	/* see if the command actually succeeded */
 	if (readb(sabi_iface + SABI_IFACE_COMPLETE) == 0xaa &&
@@ -194,21 +316,21 @@ static void test_backlight(void)
 {
 	struct sabi_retval sretval;
 
-	sabi_get_command(GET_BACKLIGHT, &sretval);
+	sabi_get_command(sabi_config->commands.get_backlight, &sretval);
 	printk(KERN_DEBUG "backlight = 0x%02x\n", sretval.retval[0]);
 
-	sabi_set_command(SET_BACKLIGHT, 0);
+	sabi_set_command(sabi_config->commands.set_backlight, 0);
 	printk(KERN_DEBUG "backlight should be off\n");
 
-	sabi_get_command(GET_BACKLIGHT, &sretval);
+	sabi_get_command(sabi_config->commands.get_backlight, &sretval);
 	printk(KERN_DEBUG "backlight = 0x%02x\n", sretval.retval[0]);
 
 	msleep(1000);
 
-	sabi_set_command(SET_BACKLIGHT, 1);
+	sabi_set_command(sabi_config->commands.set_backlight, 1);
 	printk(KERN_DEBUG "backlight should be on\n");
 
-	sabi_get_command(GET_BACKLIGHT, &sretval);
+	sabi_get_command(sabi_config->commands.get_backlight, &sretval);
 	printk(KERN_DEBUG "backlight = 0x%02x\n", sretval.retval[0]);
 }
 
@@ -216,21 +338,21 @@ static void test_wireless(void)
 {
 	struct sabi_retval sretval;
 
-	sabi_get_command(GET_WIRELESS_BUTTON, &sretval);
+	sabi_get_command(sabi_config->commands.get_wireless_button, &sretval);
 	printk(KERN_DEBUG "wireless led = 0x%02x\n", sretval.retval[0]);
 
-	sabi_set_command(SET_WIRELESS_BUTTON, 0);
+	sabi_set_command(sabi_config->commands.set_wireless_button, 0);
 	printk(KERN_DEBUG "wireless led should be off\n");
 
-	sabi_get_command(GET_WIRELESS_BUTTON, &sretval);
+	sabi_get_command(sabi_config->commands.get_wireless_button, &sretval);
 	printk(KERN_DEBUG "wireless led = 0x%02x\n", sretval.retval[0]);
 
 	msleep(1000);
 
-	sabi_set_command(SET_WIRELESS_BUTTON, 1);
+	sabi_set_command(sabi_config->commands.set_wireless_button, 1);
 	printk(KERN_DEBUG "wireless led should be on\n");
 
-	sabi_get_command(GET_WIRELESS_BUTTON, &sretval);
+	sabi_get_command(sabi_config->commands.get_wireless_button, &sretval);
 	printk(KERN_DEBUG "wireless led = 0x%02x\n", sretval.retval[0]);
 }
 
@@ -240,7 +362,8 @@ static u8 read_brightness(void)
 	int user_brightness = 0;
 	int retval;
 
-	retval = sabi_get_command(GET_BRIGHTNESS, &sretval);
+	retval = sabi_get_command(sabi_config->commands.get_brightness,
+				  &sretval);
 	if (!retval)
 		user_brightness = sretval.retval[0];
 		if (user_brightness != 0)
@@ -250,7 +373,8 @@ static u8 read_brightness(void)
 
 static void set_brightness(u8 user_brightness)
 {
-	sabi_set_command(SET_BRIGHTNESS, user_brightness + 1);
+	sabi_set_command(sabi_config->commands.set_brightness,
+			 user_brightness + 1);
 }
 
 static int get_brightness(struct backlight_device *bd)
@@ -263,9 +387,9 @@ static int update_status(struct backlight_device *bd)
 	set_brightness(bd->props.brightness);
 
 	if (bd->props.power == FB_BLANK_UNBLANK)
-		sabi_set_command(SET_BACKLIGHT, 1);
+		sabi_set_command(sabi_config->commands.set_backlight, 1);
 	else
-		sabi_set_command(SET_BACKLIGHT, 0);
+		sabi_set_command(sabi_config->commands.set_backlight, 0);
 	return 0;
 }
 
@@ -282,9 +406,9 @@ static int rfkill_set(void *data, bool blocked)
 	 * blocked == true is off
 	 */
 	if (blocked)
-		sabi_set_command(SET_WIRELESS_BUTTON, 0);
+		sabi_set_command(sabi_config->commands.set_wireless_button, 0);
 	else
-		sabi_set_command(SET_WIRELESS_BUTTON, 1);
+		sabi_set_command(sabi_config->commands.set_wireless_button, 1);
 
 	return 0;
 }
@@ -317,47 +441,49 @@ static void destroy_wireless(void)
 	rfkill_destroy(rfk);
 }
 
-static ssize_t get_silent_state(struct device *dev,
-				struct device_attribute *attr, char *buf)
+static ssize_t get_performance_level(struct device *dev,
+				     struct device_attribute *attr, char *buf)
 {
 	struct sabi_retval sretval;
 	int retval;
+	int i;
 
 	/* Read the state */
-	retval = sabi_get_command(GET_PERFORMANCE_LEVEL, &sretval);
+	retval = sabi_get_command(sabi_config->commands.get_performance_level,
+				  &sretval);
 	if (retval)
 		return retval;
 
 	/* The logic is backwards, yeah, lots of fun... */
-	if (sretval.retval[0] == 0)
-		retval = 1;
-	else
-		retval = 0;
-	return sprintf(buf, "%d\n", retval);
+	for (i = 0; sabi_config->performance_levels[i].name; ++i) {
+		if (sretval.retval[0] == sabi_config->performance_levels[i].value)
+			return sprintf(buf, "%s\n", sabi_config->performance_levels[i].name);
+	}
+	return sprintf(buf, "%s\n", "unknown");
 }
 
-static ssize_t set_silent_state(struct device *dev,
+static ssize_t set_performance_level(struct device *dev,
 				struct device_attribute *attr, const char *buf,
 				size_t count)
 {
-	char value;
-
 	if (count >= 1) {
-		value = buf[0];
-		if ((value == '0') || (value == 'n') || (value == 'N')) {
-			/* Turn speed up */
-			sabi_set_command(SET_PERFORMANCE_LEVEL, 0x01);
-		} else if ((value == '1') || (value == 'y') || (value == 'Y')) {
-			/* Turn speed down */
-			sabi_set_command(SET_PERFORMANCE_LEVEL, 0x00);
-		} else {
-			return -EINVAL;
+		int i;
+		for (i = 0; sabi_config->performance_levels[i].name; ++i) {
+			struct sabi_performance_level *level =
+				&sabi_config->performance_levels[i];
+			if (!strncasecmp(level->name, buf, strlen(level->name))) {
+				sabi_set_command(sabi_config->commands.set_performance_level,
+						 level->value);
+				break;
+			}
 		}
+		if (!sabi_config->performance_levels[i].name)
+			return -EINVAL;
 	}
 	return count;
 }
-static DEVICE_ATTR(silent, S_IWUSR | S_IRUGO,
-		   get_silent_state, set_silent_state);
+static DEVICE_ATTR(performance_level, S_IWUSR | S_IRUGO,
+		   get_performance_level, set_performance_level);
 
 
 static int __init dmi_check_cb(const struct dmi_system_id *id)
@@ -388,18 +514,113 @@ static struct dmi_system_id __initdata samsung_dmi_table[] = {
 		},
 		.callback = dmi_check_cb,
 	},
+	{
+		.ident = "X125",
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR,
+					"SAMSUNG ELECTRONICS CO., LTD."),
+			DMI_MATCH(DMI_PRODUCT_NAME, "X125"),
+			DMI_MATCH(DMI_BOARD_NAME, "X125"),
+		},
+		.callback = dmi_check_cb,
+	},
+	{
+		.ident = "NC10",
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR,
+					"SAMSUNG ELECTRONICS CO., LTD."),
+			DMI_MATCH(DMI_PRODUCT_NAME, "NC10"),
+			DMI_MATCH(DMI_BOARD_NAME, "NC10"),
+		},
+		.callback = dmi_check_cb,
+	},
+		{
+		.ident = "NP-Q45",
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR,
+					"SAMSUNG ELECTRONICS CO., LTD."),
+			DMI_MATCH(DMI_PRODUCT_NAME, "SQ45S70S"),
+			DMI_MATCH(DMI_BOARD_NAME, "SQ45S70S"),
+		},
+		.callback = dmi_check_cb,
+		},
+	{
+		.ident = "X360",
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR,
+					"SAMSUNG ELECTRONICS CO., LTD."),
+			DMI_MATCH(DMI_PRODUCT_NAME, "X360"),
+			DMI_MATCH(DMI_BOARD_NAME, "X360"),
+		},
+		.callback = dmi_check_cb,
+	},
+	{
+		.ident = "R518",
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR,
+					"SAMSUNG ELECTRONICS CO., LTD."),
+			DMI_MATCH(DMI_PRODUCT_NAME, "R518"),
+			DMI_MATCH(DMI_BOARD_NAME, "R518"),
+		},
+		.callback = dmi_check_cb,
+	},
+	{
+		.ident = "N150/N210/N220",
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR,
+					"SAMSUNG ELECTRONICS CO., LTD."),
+			DMI_MATCH(DMI_PRODUCT_NAME, "N150/N210/N220"),
+			DMI_MATCH(DMI_BOARD_NAME, "N150/N210/N220"),
+		},
+		.callback = dmi_check_cb,
+	},
+	{
+		.ident = "R530/R730",
+		.matches = {
+		      DMI_MATCH(DMI_SYS_VENDOR, "SAMSUNG ELECTRONICS CO., LTD."),
+		      DMI_MATCH(DMI_PRODUCT_NAME, "R530/R730"),
+		      DMI_MATCH(DMI_BOARD_NAME, "R530/R730"),
+		},
+		.callback = dmi_check_cb,
+	},
+	{
+		.ident = "NF110/NF210/NF310",
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "SAMSUNG ELECTRONICS CO., LTD."),
+			DMI_MATCH(DMI_PRODUCT_NAME, "NF110/NF210/NF310"),
+			DMI_MATCH(DMI_BOARD_NAME, "NF110/NF210/NF310"),
+		},
+		.callback = dmi_check_cb,
+	},
 	{ },
 };
 MODULE_DEVICE_TABLE(dmi, samsung_dmi_table);
 
+static int find_signature(void __iomem *memcheck, const char *testStr)
+{
+	int i = 0;
+	int loca;
+
+	for (loca = 0; loca < 0xffff; loca++) {
+		char temp = readb(memcheck + loca);
+
+		if (temp == testStr[i]) {
+			if (i == strlen(testStr)-1)
+				break;
+			++i;
+		} else {
+			i = 0;
+		}
+	}
+	return loca;
+}
+
 static int __init samsung_init(void)
 {
 	struct backlight_properties props;
 	struct sabi_retval sretval;
-	const char *testStr = "SECLINUX";
-	void __iomem *memcheck;
 	unsigned int ifaceP;
-	int pStr;
+	int i;
 	int loca;
 	int retval;
 
@@ -414,50 +635,44 @@ static int __init samsung_init(void)
 		return -EINVAL;
 	}
 
-	/* Try to find the signature "SECLINUX" in memory to find the header */
-	pStr = 0;
-	memcheck = f0000_segment;
-	for (loca = 0; loca < 0xffff; loca++) {
-		char temp = readb(memcheck + loca);
-
-		if (temp == testStr[pStr]) {
-			if (pStr == strlen(testStr)-1)
-				break;
-			++pStr;
-		} else {
-			pStr = 0;
-		}
+	/* Try to find one of the signatures in memory to find the header */
+	for (i = 0; sabi_configs[i].test_string != 0; ++i) {
+		sabi_config = &sabi_configs[i];
+		loca = find_signature(f0000_segment, sabi_config->test_string);
+		if (loca != 0xffff)
+			break;
 	}
+
 	if (loca == 0xffff) {
 		printk(KERN_ERR "This computer does not support SABI\n");
 		goto error_no_signature;
-		}
+	}
 
 	/* point to the SMI port Number */
 	loca += 1;
-	sabi = (memcheck + loca);
+	sabi = (f0000_segment + loca);
 
 	if (debug) {
 		printk(KERN_DEBUG "This computer supports SABI==%x\n",
 			loca + 0xf0000 - 6);
 		printk(KERN_DEBUG "SABI header:\n");
 		printk(KERN_DEBUG " SMI Port Number = 0x%04x\n",
-			readw(sabi + SABI_HEADER_PORT));
+			readw(sabi + sabi_config->header_offsets.port));
 		printk(KERN_DEBUG " SMI Interface Function = 0x%02x\n",
-			readb(sabi + SABI_HEADER_IFACEFUNC));
+			readb(sabi + sabi_config->header_offsets.iface_func));
 		printk(KERN_DEBUG " SMI enable memory buffer = 0x%02x\n",
-			readb(sabi + SABI_HEADER_EN_MEM));
+			readb(sabi + sabi_config->header_offsets.en_mem));
 		printk(KERN_DEBUG " SMI restore memory buffer = 0x%02x\n",
-			readb(sabi + SABI_HEADER_RE_MEM));
+			readb(sabi + sabi_config->header_offsets.re_mem));
 		printk(KERN_DEBUG " SABI data offset = 0x%04x\n",
-			readw(sabi + SABI_HEADER_DATA_OFFSET));
+			readw(sabi + sabi_config->header_offsets.data_offset));
 		printk(KERN_DEBUG " SABI data segment = 0x%04x\n",
-			readw(sabi + SABI_HEADER_DATA_SEGMENT));
+			readw(sabi + sabi_config->header_offsets.data_segment));
 	}
 
 	/* Get a pointer to the SABI Interface */
-	ifaceP = (readw(sabi + SABI_HEADER_DATA_SEGMENT) & 0x0ffff) << 4;
-	ifaceP += readw(sabi + SABI_HEADER_DATA_OFFSET) & 0x0ffff;
+	ifaceP = (readw(sabi + sabi_config->header_offsets.data_segment) & 0x0ffff) << 4;
+	ifaceP += readw(sabi + sabi_config->header_offsets.data_offset) & 0x0ffff;
 	sabi_iface = ioremap(ifaceP, 16);
 	if (!sabi_iface) {
 		printk(KERN_ERR "Can't remap %x\n", ifaceP);
@@ -470,15 +685,19 @@ static int __init samsung_init(void)
 		test_backlight();
 		test_wireless();
 
-		retval = sabi_get_command(GET_BRIGHTNESS, &sretval);
+		retval = sabi_get_command(sabi_config->commands.get_brightness,
+					  &sretval);
 		printk(KERN_DEBUG "brightness = 0x%02x\n", sretval.retval[0]);
 	}
 
 	/* Turn on "Linux" mode in the BIOS */
-	retval = sabi_set_command(SET_LINUX, 0x81);
-	if (retval) {
-		printk(KERN_ERR KBUILD_MODNAME ": Linux mode was not set!\n");
-		goto error_no_platform;
+	if (sabi_config->commands.set_linux != 0xff) {
+		retval = sabi_set_command(sabi_config->commands.set_linux,
+					  0x81);
+		if (retval) {
+			printk(KERN_ERR KBUILD_MODNAME ": Linux mode was not set!\n");
+			goto error_no_platform;
+		}
 	}
 
 	/* knock up a platform device to hang stuff off of */
@@ -503,7 +722,7 @@ static int __init samsung_init(void)
 	if (retval)
 		goto error_no_rfk;
 
-	retval = device_create_file(&sdev->dev, &dev_attr_silent);
+	retval = device_create_file(&sdev->dev, &dev_attr_performance_level);
 	if (retval)
 		goto error_file_create;
 
@@ -530,9 +749,10 @@ error_no_signature:
 static void __exit samsung_exit(void)
 {
 	/* Turn off "Linux" mode in the BIOS */
-	sabi_set_command(SET_LINUX, 0x80);
+	if (sabi_config->commands.set_linux != 0xff)
+		sabi_set_command(sabi_config->commands.set_linux, 0x80);
 
-	device_remove_file(&sdev->dev, &dev_attr_silent);
+	device_remove_file(&sdev->dev, &dev_attr_performance_level);
 	backlight_device_unregister(backlight_device);
 	destroy_wireless();
 	iounmap(sabi_iface);
