0000000000000000 f3410f12fd                      MOVSLDUP  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000005 f2410f12fd                      MOVDDUP   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000000A f3410f16fd                      MOVSHDUP  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000000F 66410f7cfd                      HADDPD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000014 f2410f7cfd                      HADDPS    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000019 66410f7dfd                      HSUBPD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000001E f2410f7dfd                      HSUBPS    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000023 66410fd0fd                      ADDSUBPD  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000028 f2410fd0fd                      ADDSUBPS  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000002D f20ff03b                        LDDQU     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000031 66410f3800fd                    PSHUFB    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000037 66410f3801fd                    PHADDW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000003D 66410f3802fd                    PHADDD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000043 66410f3803fd                    PHADDSW   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000049 66410f3804fd                    PMADDUBSW xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000004F 66410f3805fd                    PHSUBW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000055 66410f3806fd                    PHSUBD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000005B 66410f3807fd                    PHSUBSW   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000061 66410f3808fd                    PSIGNB    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000067 66410f3809fd                    PSIGNW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000006D 66410f380afd                    PSIGND    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000073 66410f380bfd                    PMULHRSW  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000079 66410f381cfd                    PABSB     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000007F 66410f381dfd                    PABSW     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000085 66410f381efd                    PABSD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000008B 66410f3a0ffd0a                  PALIGNR   xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000092 f30f123b                        MOVSLDUP  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000096 f20f123b                        MOVDDUP   xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000009A f30f163b                        MOVSHDUP  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000009E 660f7c3b                        HADDPD    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000A2 f20f7c3b                        HADDPS    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000A6 660f7d3b                        HSUBPD    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000AA f20f7d3b                        HSUBPS    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000AE 660fd03b                        ADDSUBPD  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000B2 f20fd03b                        ADDSUBPS  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000B6 f20ff03b                        LDDQU     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 0
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000BA 660f38003b                      PSHUFB    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000BF 660f38013b                      PHADDW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000C4 660f38023b                      PHADDD    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000C9 660f38033b                      PHADDSW   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000CE 660f38043b                      PMADDUBSW xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000D3 660f38053b                      PHSUBW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000D8 660f38063b                      PHSUBD    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000DD 660f38073b                      PHSUBSW   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000E2 660f38083b                      PSIGNB    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000E7 660f38093b                      PSIGNW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000EC 660f380a3b                      PSIGND    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000F1 660f380b3b                      PMULHRSW  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000F6 660f381c3b                      PABSB     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000FB 660f381d3b                      PABSW     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000100 660f381e3b                      PABSD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000105 660f3a0f3b0a                    PALIGNR   xmm7, xmmword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSSE3, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 9
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

