0000000000000000 f20f01c6                        RDMSRLIST
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: MSRLIST, Ins cat: SYSTEM, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 27
        Valid modes
                R0: yes, R1: no, R2: no, R3: no
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size: 512, RawSize: 512, Encoding: S, 
                Base: 6, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size: 512, RawSize: 512, Encoding: S, 
                Base: 7, 
        Operand: 2, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 1, RegCount: 1

0000000000000004 f30f01c6                        WRMSRLIST
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: MSRLIST, Ins cat: SYSTEM, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 27
        Valid modes
                R0: yes, R1: no, R2: no, R3: no
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size: 512, RawSize: 512, Encoding: S, 
                Base: 6, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 512, RawSize: 512, Encoding: S, 
                Base: 7, 
        Operand: 2, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 1, RegCount: 1

0000000000000008 0f01c6                          WRMSRNS
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: WRMSRNS, Ins cat: SYSTEM, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 19
        Valid modes
                R0: yes, R1: no, R2: no, R3: no
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 3, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: E, RegType:   Model Specific, RegSize:  8, RegId: 0xffffffff, RegCount: 1

