0000000000000000 c4e27ab100                      VBCSTNEBF162PS xmm0, word ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 0, 

0000000000000005 c4e27eb100                      VBCSTNEBF162PS ymm0, word ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 0, 

000000000000000A c4e279b100                      VBCSTNESH2PS xmm0, word ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 0, 

000000000000000F c4e27db100                      VBCSTNESH2PS ymm0, word ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 0, 

0000000000000014 c4e27ab000                      VCVTNEEBF162PS xmm0, xmmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 0, 

0000000000000019 c4e27eb000                      VCVTNEEBF162PS ymm0, ymmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 0, 

000000000000001E c4e279b000                      VCVTNEEPH2PS xmm0, xmmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 0, 

0000000000000023 c4e27db000                      VCVTNEEPH2PS ymm0, ymmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 0, 

0000000000000028 c4e27bb000                      VCVTNEOBF162PS xmm0, xmmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 0, 

000000000000002D c4e27fb000                      VCVTNEOBF162PS ymm0, ymmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 0, 

0000000000000032 c4e278b000                      VCVTNEOPH2PS xmm0, xmmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 0, 

0000000000000037 c4e27cb000                      VCVTNEOPH2PS ymm0, ymmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 0, 

000000000000003C c4e27a72c1                      VCVTNEPS2BF16 xmm0, xmm1
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 1, RegCount: 1

0000000000000041 c4e27e72c1                      VCVTNEPS2BF16 ymm0, ymm1
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 1, RegCount: 1

0000000000000046 c4e27a7200                      VCVTNEPS2BF16 xmm0, xmmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 0, 

000000000000004B c4e27e7200                      VCVTNEPS2BF16 ymm0, ymmword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXNECONVERT, Ins cat: AVXNECONVERT, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: edx, bit: 5
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 0, 

