0000000000000000 62f2450850d0                    VPDPBUSD  xmm2, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000006 62f245085013                    VPDPBUSD  xmm2, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000000C 62f245185013                    VPDPBUSD  xmm2, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

0000000000000012 62b245085054db10                VPDPBUSD  xmm2, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

000000000000001A 62b245085054dbf0                VPDPBUSD  xmm2, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

0000000000000022 62f2450d50d0                    VPDPBUSD  xmm2{k5}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000028 62f2450d5013                    VPDPBUSD  xmm2{k5}, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000002E 62f2451d5013                    VPDPBUSD  xmm2{k5}, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

0000000000000034 62b2450d5054db10                VPDPBUSD  xmm2{k5}, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

000000000000003C 62b2450d5054dbf0                VPDPBUSD  xmm2{k5}, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

0000000000000044 62f2458d50d0                    VPDPBUSD  xmm2{k5}{z}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000004A 62f2458d5013                    VPDPBUSD  xmm2{k5}{z}, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000050 62f2459d5013                    VPDPBUSD  xmm2{k5}{z}, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

0000000000000056 62b2458d5054db10                VPDPBUSD  xmm2{k5}{z}, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

000000000000005E 62b2458d5054dbf0                VPDPBUSD  xmm2{k5}{z}, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

0000000000000066 62c2152850c7                    VPDPBUSD  ymm16, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

000000000000006C 62e215285003                    VPDPBUSD  ymm16, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000072 62e215385003                    VPDPBUSD  ymm16, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

0000000000000078 62a215285044db08                VPDPBUSD  ymm16, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

0000000000000080 62a215285044dbf8                VPDPBUSD  ymm16, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

0000000000000088 62c2152d50c7                    VPDPBUSD  ymm16{k5}, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

000000000000008E 62e2152d5003                    VPDPBUSD  ymm16{k5}, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000094 62e2153d5003                    VPDPBUSD  ymm16{k5}, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

000000000000009A 62a2152d5044db08                VPDPBUSD  ymm16{k5}, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

00000000000000A2 62a2152d5044dbf8                VPDPBUSD  ymm16{k5}, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

00000000000000AA 62c215ad50c7                    VPDPBUSD  ymm16{k5}{z}, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

00000000000000B0 62e215ad5003                    VPDPBUSD  ymm16{k5}{z}, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000B6 62e215bd5003                    VPDPBUSD  ymm16{k5}{z}, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

00000000000000BC 62a215ad5044db08                VPDPBUSD  ymm16{k5}{z}, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

00000000000000C4 62a215ad5044dbf8                VPDPBUSD  ymm16{k5}{z}, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

00000000000000CC 62023d4050c7                    VPDPBUSD  zmm24, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000000D2 62623d405003                    VPDPBUSD  zmm24, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000D8 62623d505003                    VPDPBUSD  zmm24, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

00000000000000DE 62223d405044db04                VPDPBUSD  zmm24, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000000E6 62223d405044dbfc                VPDPBUSD  zmm24, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000000EE 62023d4550c7                    VPDPBUSD  zmm24{k5}, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000000F4 62623d455003                    VPDPBUSD  zmm24{k5}, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000FA 62623d555003                    VPDPBUSD  zmm24{k5}, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000100 62223d455044db04                VPDPBUSD  zmm24{k5}, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000108 62223d455044dbfc                VPDPBUSD  zmm24{k5}, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000110 62023dc550c7                    VPDPBUSD  zmm24{k5}{z}, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000116 62623dc55003                    VPDPBUSD  zmm24{k5}{z}, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000011C 62623dd55003                    VPDPBUSD  zmm24{k5}{z}, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000122 62223dc55044db04                VPDPBUSD  zmm24{k5}{z}, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

000000000000012A 62223dc55044dbfc                VPDPBUSD  zmm24{k5}{z}, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000132 62f2450851d0                    VPDPBUSDS xmm2, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000138 62f245085113                    VPDPBUSDS xmm2, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000013E 62f245185113                    VPDPBUSDS xmm2, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

0000000000000144 62b245085154db10                VPDPBUSDS xmm2, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

000000000000014C 62b245085154dbf0                VPDPBUSDS xmm2, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

0000000000000154 62f2450d51d0                    VPDPBUSDS xmm2{k5}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000015A 62f2450d5113                    VPDPBUSDS xmm2{k5}, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000160 62f2451d5113                    VPDPBUSDS xmm2{k5}, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

0000000000000166 62b2450d5154db10                VPDPBUSDS xmm2{k5}, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

000000000000016E 62b2450d5154dbf0                VPDPBUSDS xmm2{k5}, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

0000000000000176 62f2458d51d0                    VPDPBUSDS xmm2{k5}{z}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000017C 62f2458d5113                    VPDPBUSDS xmm2{k5}{z}, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000182 62f2459d5113                    VPDPBUSDS xmm2{k5}{z}, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

0000000000000188 62b2458d5154db10                VPDPBUSDS xmm2{k5}{z}, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

0000000000000190 62b2458d5154dbf0                VPDPBUSDS xmm2{k5}{z}, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

0000000000000198 62c2152851c7                    VPDPBUSDS ymm16, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

000000000000019E 62e215285103                    VPDPBUSDS ymm16, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000001A4 62e215385103                    VPDPBUSDS ymm16, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

00000000000001AA 62a215285144db08                VPDPBUSDS ymm16, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

00000000000001B2 62a215285144dbf8                VPDPBUSDS ymm16, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

00000000000001BA 62c2152d51c7                    VPDPBUSDS ymm16{k5}, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

00000000000001C0 62e2152d5103                    VPDPBUSDS ymm16{k5}, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000001C6 62e2153d5103                    VPDPBUSDS ymm16{k5}, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

00000000000001CC 62a2152d5144db08                VPDPBUSDS ymm16{k5}, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

00000000000001D4 62a2152d5144dbf8                VPDPBUSDS ymm16{k5}, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

00000000000001DC 62c215ad51c7                    VPDPBUSDS ymm16{k5}{z}, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

00000000000001E2 62e215ad5103                    VPDPBUSDS ymm16{k5}{z}, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000001E8 62e215bd5103                    VPDPBUSDS ymm16{k5}{z}, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

00000000000001EE 62a215ad5144db08                VPDPBUSDS ymm16{k5}{z}, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

00000000000001F6 62a215ad5144dbf8                VPDPBUSDS ymm16{k5}{z}, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

00000000000001FE 62023d4051c7                    VPDPBUSDS zmm24, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000204 62623d405103                    VPDPBUSDS zmm24, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000020A 62623d505103                    VPDPBUSDS zmm24, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000210 62223d405144db04                VPDPBUSDS zmm24, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000218 62223d405144dbfc                VPDPBUSDS zmm24, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000220 62023d4551c7                    VPDPBUSDS zmm24{k5}, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000226 62623d455103                    VPDPBUSDS zmm24{k5}, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000022C 62623d555103                    VPDPBUSDS zmm24{k5}, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000232 62223d455144db04                VPDPBUSDS zmm24{k5}, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

000000000000023A 62223d455144dbfc                VPDPBUSDS zmm24{k5}, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000242 62023dc551c7                    VPDPBUSDS zmm24{k5}{z}, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000248 62623dc55103                    VPDPBUSDS zmm24{k5}{z}, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000024E 62623dd55103                    VPDPBUSDS zmm24{k5}{z}, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000254 62223dc55144db04                VPDPBUSDS zmm24{k5}{z}, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

000000000000025C 62223dc55144dbfc                VPDPBUSDS zmm24{k5}{z}, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000264 62f2450852d0                    VPDPWSSD  xmm2, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000026A 62f245085213                    VPDPWSSD  xmm2, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000270 62f245185213                    VPDPWSSD  xmm2, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

0000000000000276 62b245085254db10                VPDPWSSD  xmm2, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

000000000000027E 62b245085254dbf0                VPDPWSSD  xmm2, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

0000000000000286 62f2450d52d0                    VPDPWSSD  xmm2{k5}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000028C 62f2450d5213                    VPDPWSSD  xmm2{k5}, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000292 62f2451d5213                    VPDPWSSD  xmm2{k5}, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

0000000000000298 62b2450d5254db10                VPDPWSSD  xmm2{k5}, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

00000000000002A0 62b2450d5254dbf0                VPDPWSSD  xmm2{k5}, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

00000000000002A8 62f2458d52d0                    VPDPWSSD  xmm2{k5}{z}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000002AE 62f2458d5213                    VPDPWSSD  xmm2{k5}{z}, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002B4 62f2459d5213                    VPDPWSSD  xmm2{k5}{z}, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

00000000000002BA 62b2458d5254db10                VPDPWSSD  xmm2{k5}{z}, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

00000000000002C2 62b2458d5254dbf0                VPDPWSSD  xmm2{k5}{z}, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

00000000000002CA 62c2152852c7                    VPDPWSSD  ymm16, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

00000000000002D0 62e215285203                    VPDPWSSD  ymm16, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002D6 62e215385203                    VPDPWSSD  ymm16, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

00000000000002DC 62a215285244db08                VPDPWSSD  ymm16, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

00000000000002E4 62a215285244dbf8                VPDPWSSD  ymm16, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

00000000000002EC 62c2152d52c7                    VPDPWSSD  ymm16{k5}, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

00000000000002F2 62e2152d5203                    VPDPWSSD  ymm16{k5}, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002F8 62e2153d5203                    VPDPWSSD  ymm16{k5}, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

00000000000002FE 62a2152d5244db08                VPDPWSSD  ymm16{k5}, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

0000000000000306 62a2152d5244dbf8                VPDPWSSD  ymm16{k5}, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

000000000000030E 62c215ad52c7                    VPDPWSSD  ymm16{k5}{z}, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

0000000000000314 62e215ad5203                    VPDPWSSD  ymm16{k5}{z}, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000031A 62e215bd5203                    VPDPWSSD  ymm16{k5}{z}, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

0000000000000320 62a215ad5244db08                VPDPWSSD  ymm16{k5}{z}, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

0000000000000328 62a215ad5244dbf8                VPDPWSSD  ymm16{k5}{z}, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

0000000000000330 62023d4052c7                    VPDPWSSD  zmm24, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000336 62623d405203                    VPDPWSSD  zmm24, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000033C 62623d505203                    VPDPWSSD  zmm24, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000342 62223d405244db04                VPDPWSSD  zmm24, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

000000000000034A 62223d405244dbfc                VPDPWSSD  zmm24, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000352 62023d4552c7                    VPDPWSSD  zmm24{k5}, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000358 62623d455203                    VPDPWSSD  zmm24{k5}, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000035E 62623d555203                    VPDPWSSD  zmm24{k5}, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000364 62223d455244db04                VPDPWSSD  zmm24{k5}, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

000000000000036C 62223d455244dbfc                VPDPWSSD  zmm24{k5}, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000374 62023dc552c7                    VPDPWSSD  zmm24{k5}{z}, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000037A 62623dc55203                    VPDPWSSD  zmm24{k5}{z}, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000380 62623dd55203                    VPDPWSSD  zmm24{k5}{z}, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000386 62223dc55244db04                VPDPWSSD  zmm24{k5}{z}, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

000000000000038E 62223dc55244dbfc                VPDPWSSD  zmm24{k5}{z}, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000396 62f2450853d0                    VPDPWSSDS xmm2, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000039C 62f245085313                    VPDPWSSDS xmm2, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003A2 62f245185313                    VPDPWSSDS xmm2, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

00000000000003A8 62b245085354db10                VPDPWSSDS xmm2, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

00000000000003B0 62b245085354dbf0                VPDPWSSDS xmm2, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

00000000000003B8 62f2450d53d0                    VPDPWSSDS xmm2{k5}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000003BE 62f2450d5313                    VPDPWSSDS xmm2{k5}, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003C4 62f2451d5313                    VPDPWSSDS xmm2{k5}, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

00000000000003CA 62b2450d5354db10                VPDPWSSDS xmm2{k5}, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

00000000000003D2 62b2450d5354dbf0                VPDPWSSDS xmm2{k5}, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

00000000000003DA 62f2458d53d0                    VPDPWSSDS xmm2{k5}{z}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000003E0 62f2458d5313                    VPDPWSSDS xmm2{k5}{z}, xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003E6 62f2459d5313                    VPDPWSSDS xmm2{k5}{z}, xmm7, dword ptr [rbx]{1to4}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 4 times

00000000000003EC 62b2458d5354db10                VPDPWSSDS xmm2{k5}{z}, xmm7, xmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000010, 

00000000000003F4 62b2458d5354dbf0                VPDPWSSDS xmm2{k5}{z}, xmm7, xmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff0, 

00000000000003FC 62c2152853c7                    VPDPWSSDS ymm16, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

0000000000000402 62e215285303                    VPDPWSSDS ymm16, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000408 62e215385303                    VPDPWSSDS ymm16, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

000000000000040E 62a215285344db08                VPDPWSSDS ymm16, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

0000000000000416 62a215285344dbf8                VPDPWSSDS ymm16, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

000000000000041E 62c2152d53c7                    VPDPWSSDS ymm16{k5}, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

0000000000000424 62e2152d5303                    VPDPWSSDS ymm16{k5}, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000042A 62e2153d5303                    VPDPWSSDS ymm16{k5}, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

0000000000000430 62a2152d5344db08                VPDPWSSDS ymm16{k5}, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

0000000000000438 62a2152d5344dbf8                VPDPWSSDS ymm16{k5}, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

0000000000000440 62c215ad53c7                    VPDPWSSDS ymm16{k5}{z}, ymm13, ymm15
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1

0000000000000446 62e215ad5303                    VPDPWSSDS ymm16{k5}{z}, ymm13, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000044C 62e215bd5303                    VPDPWSSDS ymm16{k5}{z}, ymm13, dword ptr [rbx]{1to8}
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 8 times

0000000000000452 62a215ad5344db08                VPDPWSSDS ymm16{k5}{z}, ymm13, ymmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000008, 

000000000000045A 62a215ad5344dbf8                VPDPWSSDS ymm16{k5}{z}, ymm13, ymmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 16, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffff8, 

0000000000000462 62023d4053c7                    VPDPWSSDS zmm24, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000468 62623d405303                    VPDPWSSDS zmm24, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000046E 62623d505303                    VPDPWSSDS zmm24, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000474 62223d405344db04                VPDPWSSDS zmm24, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

000000000000047C 62223d405344dbfc                VPDPWSSDS zmm24, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000484 62023d4553c7                    VPDPWSSDS zmm24{k5}, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000048A 62623d455303                    VPDPWSSDS zmm24{k5}, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000490 62623d555303                    VPDPWSSDS zmm24{k5}, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000496 62223d455344db04                VPDPWSSDS zmm24{k5}, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

000000000000049E 62223d455344dbfc                VPDPWSSDS zmm24{k5}, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000004A6 62023dc553c7                    VPDPWSSDS zmm24{k5}{z}, zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000004AC 62623dc55303                    VPDPWSSDS zmm24{k5}{z}, zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004B2 62623dd55303                    VPDPWSSDS zmm24{k5}{z}, zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

00000000000004B8 62223dc55344db04                VPDPWSSDS zmm24{k5}{z}, zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000004C0 62223dc55344dbfc                VPDPWSSDS zmm24{k5}{z}, zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512VNNI, Ins cat: VNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 11
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

