0000000000000000 f30f0128                        RSTORSSP  qword ptr [rax]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Shadow stack: 1, 
                Segment: 3, Base: 0, 
        Operand: 1, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:              SSP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000004 f30f01ea                        SAVEPREVSSP
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Shadow stack: 2, 
                
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:              SSP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000008 f30f01e8                        SETSSBSY
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 4, 
                
        Operand: 1, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:              SSP, RegSize:  8, RegId: 0, RegCount: 1

000000000000000C f30f1ec8                        RDSSPD    eax
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:              SSP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000010 f3480f1ec8                      RDSSPQ    rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:              SSP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000015 f30f1efa                        ENDBR64
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: CET_IBT, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: edx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no

0000000000000019 f30f1efb                        ENDBR32
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: CET_IBT, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: edx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no

000000000000001D 660f38f500                      WRUSSD    dword ptr [rax], eax
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Shadow stack: 1, 
                Segment: 3, Base: 0, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1

0000000000000022 66480f38f500                    WRUSSQ    qword ptr [rax], rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Shadow stack: 1, 
                Segment: 3, Base: 0, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1

0000000000000028 0f38f600                        WRSSD     dword ptr [rax], eax
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Shadow stack: 1, 
                Segment: 3, Base: 0, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1

000000000000002C 480f38f600                      WRSSQ     qword ptr [rax], rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: CET_SS, Ins cat: CET, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Shadow stack: 1, 
                Segment: 3, Base: 0, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1

