0000000000000000 6650                            PUSH      ax
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: O, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000002 6658                            POP       ax
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: O, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000004 50                              PUSH      rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: O, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000005 58                              POP       rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: O, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000006 666a7f                          PUSH      0x007f
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  2, RawSize:  1, Encoding: I
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000009 68ff7f0000                      PUSH      0x0000000000007fff
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  8, RawSize:  4, Encoding: I
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000000E 68ffffff7f                      PUSH      0x000000007fffffff
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  8, RawSize:  4, Encoding: I
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000013 66ff33                          PUSH      word ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000016 668f03                          POP       word ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000019 6667ff33                        PUSH      word ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000001D 66678f03                        POP       word ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000021 ff33                            PUSH      qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000023 8f03                            POP       qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000025 67ff33                          PUSH      qword ptr [ebx]
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000028 678f03                          POP       qword ptr [ebx]
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000002B c8100020                        ENTER     0x0010, 0x20
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I186, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  2, RawSize:  2, Encoding: I
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I
        Operand: 2, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 3, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 4, RegCount: 1
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000002F c9                              LEAVE
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I186, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 1, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 4, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000030 0fa0                            PUSH      fs
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 4, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000032 0fa1                            POP       fs
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000034 0fa8                            PUSH      gs
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000036 0fa9                            POP       gs
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000038 669c                            PUSHFW    
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000003A 669d                            POPFW     
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000003C 9c                              PUSHFQ    
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000003D 9d                              POPFQ     
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

