0000000000000000 66410f10fd                      MOVUPD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000005 f2410f10fd                      MOVSD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000000A 66440f10ef                      MOVUPD    xmm13, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

000000000000000F f2440f10ef                      MOVSD     xmm13, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000014 660f123b                        MOVLPD    xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000018 660f133b                        MOVLPD    qword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

000000000000001C 66410f14fd                      UNPCKLPD  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000021 66410f15fd                      UNPCKHPD  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000026 660f163b                        MOVHPD    xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000002A 660f173b                        MOVHPD    qword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

000000000000002E 66410f28fd                      MOVAPD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000033 66440f28ef                      MOVAPD    xmm13, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000038 f20f2afa                        CVTSI2SD  xmm7, edx
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1

000000000000003C f2480f2afa                      CVTSI2SD  xmm7, rdx
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1

0000000000000041 660f2b3b                        MOVNTPD   xmmword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000045 f2410f2cd5                      CVTTSD2SI edx, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000004A f2490f2cd5                      CVTTSD2SI rdx, xmm13
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000004F f2410f2dd5                      CVTSD2SI  edx, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000054 f2490f2dd5                      CVTSD2SI  rdx, xmm13
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000059 66410f2efd                      UCOMISD   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE2, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        FLAGS access
                CF: m, PF: m, ZF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

000000000000005E 66410f2ffd                      COMISD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE2, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        FLAGS access
                CF: m, PF: m, ZF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000063 660f50c7                        MOVMSKPD  eax, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000067 66410f51fd                      SQRTPD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000006C f2410f51fd                      SQRTSD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000071 66410f54fd                      ANDPD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL_FP, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000076 66410f55fd                      ANDNPD    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL_FP, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000007B 66410f56fd                      ORPD      xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL_FP, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000080 66410f57fd                      XORPD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL_FP, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000085 66410f58fd                      ADDPD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000008A f2410f58fd                      ADDSD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000008F 66410f59fd                      MULPD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000094 f2410f59fd                      MULSD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000099 410f5afd                        CVTPS2PD  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000009D 66410f5afd                      CVTPD2PS  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000A2 f3410f5afd                      CVTSS2SD  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000A7 f2410f5afd                      CVTSD2SS  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000AC 410f5bfd                        CVTDQ2PS  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000B0 66410f5bfd                      CVTPS2DQ  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000B5 f3410f5bfd                      CVTTPS2DQ xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000BA 66410f5cfd                      SUBPD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000BF f2410f5cfd                      SUBSD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000C4 66410f5dfd                      MINPD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000C9 f2410f5dfd                      MINSD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000CE 66410f5efd                      DIVPD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000D3 f2410f5efd                      DIVSD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000D8 66410f5ffd                      MAXPD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000DD f2410f5ffd                      MAXSD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000E2 66410f60fd                      PUNPCKLBW xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000E7 66410f61fd                      PUNPCKLWD xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000EC 66410f62fd                      PUNPCKLDQ xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000F1 66410f63fd                      PACKSSWB  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000F6 66410f64fd                      PCMPGTB   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000000FB 66410f65fd                      PCMPGTW   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000100 66410f66fd                      PCMPGTD   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000105 66410f67fd                      PACKUSWB  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000010A 66410f68fd                      PUNPCKHBW xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000010F 66410f69fd                      PUNPCKHWD xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000114 66410f6afd                      PUNPCKHDQ xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000119 66410f6bfd                      PACKSSDW  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000011E 66410f6cfd                      PUNPCKLQDQ xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000123 66410f6dfd                      PUNPCKHQDQ xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000128 660f6efa                        MOVD      xmm7, edx
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1

000000000000012C 66480f6efa                      MOVQ      xmm7, rdx
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1

0000000000000131 66410f6ffd                      MOVDQA    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000136 f3410f6ffd                      MOVDQU    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000013B 66410f70fd0a                    PSHUFD    xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000141 f3410f70fd0a                    PSHUFHW   xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000147 f2410f70fd0a                    PSHUFLW   xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000014D 660f71d70a                      PSRLW     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000152 660f71e70a                      PSRAW     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000157 660f71f70a                      PSLLW     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000015C 660f72d70a                      PSRLD     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000161 660f72e70a                      PSRAD     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000166 660f72f70a                      PSLLD     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000016B 660f73d70a                      PSRLQ     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000170 660f73df0a                      PSRLDQ    xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000175 660f73f70a                      PSLLQ     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000017A 660f73ff0a                      PSLLDQ    xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000017F 66410f74fd                      PCMPEQB   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000184 66410f75fd                      PCMPEQW   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000189 66410f76fd                      PCMPEQD   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000018E 660f7efa                        MOVD      edx, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000192 66480f7efa                      MOVQ      rdx, xmm7
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000197 f3410f7efd                      MOVQ      xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000019C 66440f6fef                      MOVDQA    xmm13, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000001A1 f3440f6fef                      MOVDQU    xmm13, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000001A6 66410fc2fd0a                    CMPPD     xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000001AC f2410fc2fd0a                    CMPSD     xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000001B2 0fc313                          MOVNTI    dword ptr [rbx], edx
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1

00000000000001B5 660fc4fa0a                      PINSRW    xmm7, edx, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000001BA 660fc43b0a                      PINSRW    xmm7, word ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000001BF 660fc5d70a                      PEXTRW    edx, xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000001C4 66480fc5d70a                    PEXTRW    rdx, xmm7, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000001CA 66410fc6fd0a                    SHUFPD    xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000001D0 66410fd1fd                      PSRLW     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000001D5 66410fd2fd                      PSRLD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000001DA 66410fd3fd                      PSRLQ     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000001DF 66410fd4fd                      PADDQ     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000001E4 66410fd5fd                      PMULLW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000001E9 f3440f7eef                      MOVQ      xmm13, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000001EE f30fd6f8                        MOVQ2DQ   xmm7, mm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1

00000000000001F2 660fd7d7                        PMOVMSKB  edx, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000001F6 66410fd8fd                      PSUBUSB   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000001FB 66410fd9fd                      PSUBUSW   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000200 66410fdafd                      PMINUB    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000205 66410fdbfd                      PAND      xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000020A 66410fdcfd                      PADDUSB   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000020F 66410fddfd                      PADDUSW   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000214 66410fdefd                      PMAXUB    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000219 66410fdffd                      PANDN     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000021E 66410fe0fd                      PAVGB     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000223 66410fe1fd                      PSRAW     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000228 66410fe2fd                      PSRAD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000022D 66410fe3fd                      PAVGW     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000232 66410fe4fd                      PMULHUW   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000237 66410fe5fd                      PMULHW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000023C 66410fe6fd                      CVTTPD2DQ xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000241 f3410fe6fd                      CVTDQ2PD  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000246 f2410fe6fd                      CVTPD2DQ  xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000024B 660fe73b                        MOVNTDQ   xmmword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

000000000000024F 66410fe8fd                      PSUBSB    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000254 66410fe9fd                      PSUBSW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000259 66410feafd                      PMINSW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000025E 66410febfd                      POR       xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000263 66410fecfd                      PADDSB    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000268 66410fedfd                      PADDSW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000026D 66410feefd                      PMAXSW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000272 66410feffd                      PXOR      xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000277 66410ff1fd                      PSLLW     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000027C 66410ff2fd                      PSLLD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000281 66410ff3fd                      PSLLQ     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000286 66410ff4fd                      PMULUDQ   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000028B 66410ff5fd                      PMADDWD   xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000290 66410ff6fd                      PSADBW    xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000295 660ff7ff                        MASKMOVDQU xmm7, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: S, 
                Segment: 3, Base: 7, 

0000000000000299 66410ff8fd                      PSUBB     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000029E 66410ff9fd                      PSUBW     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000002A3 66410ffafd                      PSUBD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000002A8 66410ffbfd                      PSUBQ     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000002AD 66410ffcfd                      PADDB     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000002B2 66410ffdfd                      PADDW     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000002B7 66410ffefd                      PADDD     xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

00000000000002BC 660f103b                        MOVUPD    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002C0 f20f103b                        MOVSD     xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002C4 660f113b                        MOVUPD    xmmword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000002C8 f20f113b                        MOVSD     qword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000002CC 660f123b                        MOVLPD    xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002D0 660f133b                        MOVLPD    qword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000002D4 660f143b                        UNPCKLPD  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002D8 660f153b                        UNPCKHPD  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002DC 660f163b                        MOVHPD    xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002E0 660f173b                        MOVHPD    qword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000002E4 660f283b                        MOVAPD    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002E8 660f293b                        MOVAPD    xmmword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000002EC f20f2afa                        CVTSI2SD  xmm7, edx
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1

00000000000002F0 f2480f2afa                      CVTSI2SD  xmm7, rdx
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1

00000000000002F5 660f2b3b                        MOVNTPD   xmmword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000002F9 f20f2c13                        CVTTSD2SI edx, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002FD f2480f2c13                      CVTTSD2SI rdx, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000302 f20f2d13                        CVTSD2SI  edx, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000306 f2480f2d13                      CVTSD2SI  rdx, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000030B 660f2e3b                        UCOMISD   xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE2, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        FLAGS access
                CF: m, PF: m, ZF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

000000000000030F 660f2f3b                        COMISD    xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE2, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        FLAGS access
                CF: m, PF: m, ZF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000313 660f50c7                        MOVMSKPD  eax, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000317 660f513b                        SQRTPD    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000031B f20f513b                        SQRTSD    xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000031F 660f543b                        ANDPD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL_FP, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000323 660f553b                        ANDNPD    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL_FP, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000327 660f563b                        ORPD      xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL_FP, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000032B 660f573b                        XORPD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL_FP, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000032F 660f583b                        ADDPD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000333 f20f583b                        ADDSD     xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000337 660f593b                        MULPD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000033B f20f593b                        MULSD     xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000033F 0f5a3b                          CVTPS2PD  xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000342 660f5a3b                        CVTPD2PS  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000346 f30f5a3b                        CVTSS2SD  xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000034A f20f5a3b                        CVTSD2SS  xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000034E 0f5b3b                          CVTDQ2PS  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000351 660f5b3b                        CVTPS2DQ  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000355 f30f5b3b                        CVTTPS2DQ xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000359 660f5c3b                        SUBPD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000035D f20f5c3b                        SUBSD     xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000361 660f5d3b                        MINPD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000365 f20f5d3b                        MINSD     xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000369 660f5e3b                        DIVPD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000036D f20f5e3b                        DIVSD     xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000371 660f5f3b                        MAXPD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000375 f20f5f3b                        MAXSD     xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000379 660f603b                        PUNPCKLBW xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000037D 660f613b                        PUNPCKLWD xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000381 660f623b                        PUNPCKLDQ xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000385 660f633b                        PACKSSWB  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000389 660f643b                        PCMPGTB   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000038D 660f653b                        PCMPGTW   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000391 660f663b                        PCMPGTD   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000395 660f673b                        PACKUSWB  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000399 660f683b                        PUNPCKHBW xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000039D 660f693b                        PUNPCKHWD xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003A1 660f6a3b                        PUNPCKHDQ xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003A5 660f6b3b                        PACKSSDW  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003A9 660f6c3b                        PUNPCKLQDQ xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003AD 660f6d3b                        PUNPCKHQDQ xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003B1 660f6efa                        MOVD      xmm7, edx
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1

00000000000003B5 66480f6efa                      MOVQ      xmm7, rdx
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1

00000000000003BA 660f6f3b                        MOVDQA    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003BE f30f6f3b                        MOVDQU    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003C2 660f703b0a                      PSHUFD    xmm7, xmmword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003C7 f30f703b0a                      PSHUFHW   xmm7, xmmword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003CC f20f703b0a                      PSHUFLW   xmm7, xmmword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003D1 660f71d70a                      PSRLW     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003D6 660f71e70a                      PSRAW     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003DB 660f71f70a                      PSLLW     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003E0 660f72d70a                      PSRLD     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003E5 660f72e70a                      PSRAD     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003EA 660f72f70a                      PSLLD     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003EF 660f73d70a                      PSRLQ     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003F4 660f73df0a                      PSRLDQ    xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003F9 660f73f70a                      PSLLQ     xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000003FE 660f73ff0a                      PSLLDQ    xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000403 660f743b                        PCMPEQB   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000407 660f753b                        PCMPEQW   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000040B 660f763b                        PCMPEQD   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000040F 660f7efa                        MOVD      edx, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000413 66480f7efa                      MOVQ      rdx, xmm7
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000418 f30f7e3b                        MOVQ      xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000041C 660f7f3b                        MOVDQA    xmmword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000420 f30f7f3b                        MOVDQU    xmmword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000424 660fc23b0a                      CMPPD     xmm7, xmmword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000429 f20fc23b0a                      CMPSD     xmm7, qword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000042E 0fc313                          MOVNTI    dword ptr [rbx], edx
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1

0000000000000431 660fc4fa0a                      PINSRW    xmm7, edx, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000436 660fc43b0a                      PINSRW    xmm7, word ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000043B 660fc5d70a                      PEXTRW    edx, xmm7, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000440 66480fc5d70a                    PEXTRW    rdx, xmm7, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000446 660fc63b0a                      SHUFPD    xmm7, xmmword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000044B 660fd13b                        PSRLW     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000044F 660fd23b                        PSRLD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000453 660fd33b                        PSRLQ     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000457 660fd43b                        PADDQ     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000045B 660fd53b                        PMULLW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000045F 660fd63b                        MOVQ      qword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

0000000000000463 f30fd6f8                        MOVQ2DQ   xmm7, mm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1

0000000000000467 660fd7d7                        PMOVMSKB  edx, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 7
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

000000000000046B 660fd83b                        PSUBUSB   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000046F 660fd93b                        PSUBUSW   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000473 660fda3b                        PMINUB    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000477 660fdb3b                        PAND      xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000047B 660fdc3b                        PADDUSB   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000047F 660fdd3b                        PADDUSW   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000483 660fde3b                        PMAXUB    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000487 660fdf3b                        PANDN     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000048B 660fe03b                        PAVGB     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000048F 660fe13b                        PSRAW     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000493 660fe23b                        PSRAD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000497 660fe33b                        PAVGW     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000049B 660fe43b                        PMULHUW   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000049F 660fe53b                        PMULHW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004A3 660fe63b                        CVTTPD2DQ xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004A7 f30fe63b                        CVTDQ2PD  xmm7, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 5
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004AB f20fe63b                        CVTPD2DQ  xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: CONVERT, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004AF 660fe73b                        MOVNTDQ   xmmword ptr [rbx], xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 1
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1

00000000000004B3 660fe83b                        PSUBSB    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004B7 660fe93b                        PSUBSW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004BB 660fea3b                        PMINSW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004BF 660feb3b                        POR       xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004C3 660fec3b                        PADDSB    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004C7 660fed3b                        PADDSW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004CB 660fee3b                        PMAXSW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004CF 660fef3b                        PXOR      xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: LOGICAL, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004D3 660ff13b                        PSLLW     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004D7 660ff23b                        PSLLD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004DB 660ff33b                        PSLLQ     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004DF 660ff43b                        PMULUDQ   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004E3 660ff53b                        PMADDWD   xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004E7 660ff63b                        PSADBW    xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004EB 660ff7ff                        MASKMOVDQU xmm7, xmm7
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: S, 
                Segment: 3, Base: 7, 

00000000000004EF 660ff83b                        PSUBB     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004F3 660ff93b                        PSUBW     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004F7 660ffa3b                        PSUBD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004FB 660ffb3b                        PSUBQ     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004FF 660ffc3b                        PADDB     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000503 660ffd3b                        PADDW     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000507 660ffe3b                        PADDD     xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: SSE2, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 26
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

