0000000000000000 c4e2795023                      VPDPBUSD  xmm4, xmm0, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXVNNI, Ins cat: AVXVNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 4
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000005 c4e27d5023                      VPDPBUSD  ymm4, ymm0, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXVNNI, Ins cat: AVXVNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 4
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000000A c4e2795123                      VPDPBUSDS xmm4, xmm0, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXVNNI, Ins cat: AVXVNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 4
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000000F c4e27d5123                      VPDPBUSDS ymm4, ymm0, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXVNNI, Ins cat: AVXVNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 4
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000014 c4e2795223                      VPDPWSSD  xmm4, xmm0, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXVNNI, Ins cat: AVXVNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 4
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000019 c4e27d5223                      VPDPWSSD  ymm4, ymm0, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXVNNI, Ins cat: AVXVNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 4
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000001E c4e2795323                      VPDPWSSDS xmm4, xmm0, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVXVNNI, Ins cat: AVXVNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 4
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000023 c4e27d5323                      VPDPWSSDS ymm4, ymm0, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVXVNNI, Ins cat: AVXVNNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000001, reg: eax, bit: 4
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

