0000000000000000 e8fbffffff                      CALL      0x0
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  8, RawSize:  4, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

0000000000000005 ffd0                            CALL      rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

0000000000000007 67ff13                          CALL      qword ptr [ebx]
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

000000000000000A ff13                            CALL      qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

000000000000000C ebfe                            JMP       0xc
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  8, RawSize:  1, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1

000000000000000E ffe0                            JMP       rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000010 67ff23                          JMP       qword ptr [ebx]
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000013 ff23                            JMP       qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000015 66ff1b                          CALLF     dword ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Shadow stack: 3, 
                

0000000000000018 ff1b                            CALLF     fword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

000000000000001A 48ff1b                          CALLF     tbyte ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size: 10, RawSize: 10, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: S, Shadow stack: 3, 
                

000000000000001D 66ff2b                          JMPF      dword ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000020 ff2b                            JMPF      fword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1

0000000000000022 48ff2b                          JMPF      tbyte ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size: 10, RawSize: 10, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000025 72fe                            JC        0x25
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        FLAGS access
                CF: t, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: yes, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  8, RawSize:  1, Encoding: D
        Operand: 1, Acc:  CRCW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1

0000000000000027 73fe                            JNC       0x27
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        FLAGS access
                CF: t, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: yes, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  8, RawSize:  1, Encoding: D
        Operand: 1, Acc:  CRCW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1

0000000000000029 e2fe                            LOOP      0x29
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  8, RawSize:  1, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 2, Acc:  CRCW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1

000000000000002B e0fe                            LOOPNZ    0x2b
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        FLAGS access
                ZF: t, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  8, RawSize:  1, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 2, Acc:  CRCW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1

000000000000002D e3fe                            JRCXZ     0x2d
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  8, RawSize:  1, Encoding: D
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 2, Acc:  CRCW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1

000000000000002F 67e3fd                          JECXZ     0x2f
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  8, RawSize:  1, Encoding: D
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  CRCW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000032 cd21                            INT       0x21
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: INTERRUPT, CET tracked: yes
        FLAGS access
                TF: m, IF: m, NT: m, RF: m, VM: tm, AC: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I
        Operand: 1, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 3, Acc:  RW,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 5, Acc:  -W,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Shadow stack: 3, 
                

0000000000000034 cc                              INT3
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: INTERRUPT, CET tracked: yes
        FLAGS access
                TF: m, IF: m, NT: m, RF: m, VM: tm, AC: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 1, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 2, Acc:  RW,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 4, Acc:  -W,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Shadow stack: 3, 
                

0000000000000035 f1                              INT1
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: INTERRUPT, CET tracked: no
        FLAGS access
                TF: m, IF: m, NT: m, RF: m, VM: tm, AC: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 1, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 2, Acc:  RW,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000036 f1                              INT1
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: INTERRUPT, CET tracked: no
        FLAGS access
                TF: m, IF: m, NT: m, RF: m, VM: tm, AC: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 1, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 2, Acc:  RW,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000037 c3                              RETN
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

0000000000000038 c22000                          RETN      0x0020
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  2, RawSize:  2, Encoding: I
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 4, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

000000000000003B cb                              RETF
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

000000000000003C ca2000                          RETF      0x0020
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  2, RawSize:  2, Encoding: I
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

000000000000003F 66cf                            IRETW
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 4, Acc:  RW,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Shadow stack: 3, 
                

0000000000000041 cf                              IRETD
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 4, Acc:  RW,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Shadow stack: 3, 
                

0000000000000042 0f05                            SYSCALL
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: AMD, Ins cat: SYSCALL, CET tracked: yes
        CPUID leaf: 0x80000001, reg: ecx, bit: 11
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: 0xc0000081, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: 0xc0000082, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: 0xc0000084, RegCount: 1
        Operand: 3, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 4, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 5, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 11, RegCount: 1
        Operand: 6, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 7, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 8, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 9, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:              SSP, RegSize:  8, RegId: 0, RegCount: 1

0000000000000044 0f35                            SYSEXIT
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: PPRO, Ins cat: SYSRET, CET tracked: no
        CPUID leaf: 0x00000001, reg: edx, bit: 11
        Valid modes
                R0: yes, R1: no, R2: no, R3: no
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 4, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 3, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:               IP, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 4, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:              SSP, RegSize:  8, RegId: 0, RegCount: 1

