0000000000000000 50                              PUSH      ax
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: O, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000001 58                              POP       ax
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: O, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000002 6650                            PUSH      eax
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: O, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000004 6658                            POP       eax
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: O, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000006 6a7f                            PUSH      0x007f
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  2, RawSize:  1, Encoding: I
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000008 6668ff7f0000                    PUSH      0x00007fff
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  4, RawSize:  4, Encoding: I
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000000E ff37                            PUSH      word ptr [bx]
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000010 8f07                            POP       word ptr [bx]
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000012 67ff33                          PUSH      word ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000015 678f03                          POP       word ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000018 66ff37                          PUSH      dword ptr [bx]
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000001B 668f07                          POP       dword ptr [bx]
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000001E 6667ff33                        PUSH      dword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000022 66678f03                        POP       dword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000026 c8100020                        ENTER     0x0010, 0x20
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I186, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  2, RawSize:  2, Encoding: I
        Operand: 1, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I
        Operand: 2, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 5, RegCount: 1
        Operand: 3, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 4, RegCount: 1
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000002A c9                              LEAVE
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I186, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 5, RegCount: 1
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 5, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 4, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000002B 06                              PUSH      es
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000002C 07                              POP       es
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000002D 1e                              PUSH      ds
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 3, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000002E 1f                              POP       ds
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 3, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000002F 16                              PUSH      ss
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 2, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000030 17                              POP       ss
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000031 0fa0                            PUSH      fs
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 4, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000033 0fa1                            POP       fs
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000035 0fa8                            PUSH      gs
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 5, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000037 0fa9                            POP       gs
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 5, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

0000000000000039 60                              PUSHA
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I386, Ins cat: PUSH, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size: 16, RawSize: 16, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000003A 61                              POPA
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I386, Ins cat: POP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000003B 9c                              PUSHFW    
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000003C 9d                              POPFW     
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000003D 669c                            PUSHFD    
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: PUSH, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

000000000000003F 669d                            POPFD     
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: POP, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: yes, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 

