0000000000000000 90                              NOP
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: NOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no

0000000000000001 f390                            PAUSE
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: PAUSE, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: no, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no

0000000000000003 f8                              CLC
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                CF: 0, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000004 f5                              CMC
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                CF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000005 f9                              STC
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                CF: 1, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000006 fc                              CLD
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                DF: 0, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000007 fd                              STD
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                DF: 1, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000008 fa                              CLI
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                IF: 0, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000009 fb                              STI
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                IF: 1, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

000000000000000A 6698                            CBW
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: CONVERT, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  1, RawSize:  1, Encoding: S, RegType:  General Purpose, RegSize:  1, RegId: 0, RegCount: 1

000000000000000C 98                              CWDE
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: CONVERT, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1

000000000000000D 4898                            CDQE
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: CONVERT, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1

000000000000000F 6699                            CWD
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: CONVERT, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1

0000000000000011 99                              CDQ
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: CONVERT, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1

0000000000000012 4899                            CQO
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: CONVERT, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1

0000000000000014 9b                              WAIT
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: X87, Ins cat: X87_ALU, CET tracked: no
        FPU flags access
                C0: u, C1: u, C2: u, C3: u, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no

0000000000000015 9e                              SAHF
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                CF: m, PF: m, AF: m, ZF: m, SF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  1, RawSize:  1, Encoding: S, RegType:  General Purpose, RegSize:  1, RegId: 4, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000016 9f                              LAHF
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                CF: t, PF: t, AF: t, ZF: t, SF: t, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  1, RawSize:  1, Encoding: S, RegType:  General Purpose, RegSize:  1, RegId: 4, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000017 d6                              SALC
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: FLAGOP, CET tracked: no
        FLAGS access
                CF: t, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  1, RawSize:  1, Encoding: S, RegType:  General Purpose, RegSize:  1, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1

0000000000000018 66678d03                        LEA       ax, [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  --,  Type:     Memory, Size:  0, RawSize:  0, Encoding: M, Address Generator: yes, 
                Base: 3, 

000000000000001C 678d03                          LEA       eax, [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  --,  Type:     Memory, Size:  0, RawSize:  0, Encoding: M, Address Generator: yes, 
                Base: 3, 

000000000000001F 67488d03                        LEA       rax, [ebx]
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  --,  Type:     Memory, Size:  0, RawSize:  0, Encoding: M, Address Generator: yes, 
                Base: 3, 

0000000000000023 668d03                          LEA       ax, [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  --,  Type:     Memory, Size:  0, RawSize:  0, Encoding: M, Address Generator: yes, 
                Base: 3, 

0000000000000026 8d03                            LEA       eax, [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  --,  Type:     Memory, Size:  0, RawSize:  0, Encoding: M, Address Generator: yes, 
                Base: 3, 

0000000000000028 488d03                          LEA       rax, [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I86, Ins cat: MISC, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  --,  Type:     Memory, Size:  0, RawSize:  0, Encoding: M, Address Generator: yes, 
                Base: 3, 

000000000000002B 66670fb203                      LSS       ax, dword ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 2, RegCount: 1

0000000000000030 660fb203                        LSS       ax, dword ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 2, RegCount: 1

0000000000000034 670fb203                        LSS       eax, fword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 2, RegCount: 1

0000000000000038 0fb203                          LSS       eax, fword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 2, RegCount: 1

000000000000003B 67480fb203                      LSS       rax, tbyte ptr [ebx]
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 10, RawSize: 10, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 2, RegCount: 1

0000000000000040 480fb203                        LSS       rax, tbyte ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 10, RawSize: 10, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 2, RegCount: 1

0000000000000044 66670fb403                      LFS       ax, dword ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 4, RegCount: 1

0000000000000049 660fb403                        LFS       ax, dword ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 4, RegCount: 1

000000000000004D 670fb403                        LFS       eax, fword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 4, RegCount: 1

0000000000000051 0fb403                          LFS       eax, fword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 4, RegCount: 1

0000000000000054 67480fb403                      LFS       rax, tbyte ptr [ebx]
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 10, RawSize: 10, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 4, RegCount: 1

0000000000000059 480fb403                        LFS       rax, tbyte ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 10, RawSize: 10, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 4, RegCount: 1

000000000000005D 66670fb503                      LGS       ax, dword ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 5, RegCount: 1

0000000000000062 660fb503                        LGS       ax, dword ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 5, RegCount: 1

0000000000000066 670fb503                        LGS       eax, fword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 5, RegCount: 1

000000000000006A 0fb503                          LGS       eax, fword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 5, RegCount: 1

000000000000006D 67480fb503                      LGS       rax, tbyte ptr [ebx]
        DSIZE: 64, ASIZE: 32, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 10, RawSize: 10, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 5, RegCount: 1

0000000000000072 480fb503                        LGS       rax, tbyte ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: I386, Ins cat: SEGOP, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 10, RawSize: 10, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:          Segment, RegSize:  8, RegId: 5, RegCount: 1

0000000000000076 f30faec0                        RDFSBASE  eax
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: RDWRFSGS, Ins cat: RDWRFSGS, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 0
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM: no, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: -1073741568, RegCount: 1

000000000000007A f3480faec0                      RDFSBASE  rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: RDWRFSGS, Ins cat: RDWRFSGS, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 0
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM: no, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: -1073741568, RegCount: 1

000000000000007F f30faec8                        RDGSBASE  eax
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: RDWRFSGS, Ins cat: RDWRFSGS, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 0
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM: no, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: -1073741567, RegCount: 1

0000000000000083 f3480faec8                      RDGSBASE  rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: RDWRFSGS, Ins cat: RDWRFSGS, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 0
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM: no, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: -1073741567, RegCount: 1

0000000000000088 f30faed0                        WRFSBASE  eax
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: RDWRFSGS, Ins cat: RDWRFSGS, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 0
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM: no, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: -1073741568, RegCount: 1

000000000000008C f3480faed0                      WRFSBASE  rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: RDWRFSGS, Ins cat: RDWRFSGS, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 0
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM: no, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: -1073741568, RegCount: 1

0000000000000091 f30faed8                        WRGSBASE  eax
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: RDWRFSGS, Ins cat: RDWRFSGS, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 0
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM: no, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: -1073741567, RegCount: 1

0000000000000095 f3480faed8                      WRGSBASE  rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: RDWRFSGS, Ins cat: RDWRFSGS, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 0
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: no, Compat: no, Long: yes
                SMM: no, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: -1073741567, RegCount: 1

000000000000009A 660f38f003                      MOVBE     ax, word ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: MOVBE, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 22
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000009F 0f38f003                        MOVBE     eax, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: MOVBE, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 22
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000A3 480f38f003                      MOVBE     rax, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: MOVBE, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 22
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000A8 660f38f103                      MOVBE     word ptr [rbx], ax
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: MOVBE, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 22
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: R, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1

00000000000000AD 0f38f103                        MOVBE     dword ptr [rbx], eax
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: MOVBE, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 22
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1

00000000000000B1 480f38f103                      MOVBE     qword ptr [rbx], rax
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: MOVBE, Ins cat: DATAXFER, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 22
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1

00000000000000B6 f20f38f0c0                      CRC32     eax, al
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: SSE42, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  1, RawSize:  1, Encoding: M, RegType:  General Purpose, RegSize:  1, RegId: 0, RegCount: 1

00000000000000BB f2480f38f0c0                    CRC32     rax, al
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: SSE42, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  1, RawSize:  1, Encoding: M, RegType:  General Purpose, RegSize:  1, RegId: 0, RegCount: 1

00000000000000C1 f20f38f003                      CRC32     eax, byte ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: SSE42, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  1, RawSize:  1, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000C6 f2480f38f003                    CRC32     rax, byte ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: SSE42, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  1, RawSize:  1, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000CC 66f20f38f103                    CRC32     eax, word ptr [rbx]
        DSIZE: 16, ASIZE: 64, VLEN: -
        ISA Set: SSE42, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000D2 f20f38f103                      CRC32     eax, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: SSE42, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000D7 f2480f38f103                    CRC32     rax, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: SSE42, Ins cat: SSE, CET tracked: no
        CPUID leaf: 0x00000001, reg: ecx, bit: 20
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000DD 66480f38f6c1                    ADCX      rax, rcx
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: ADX, Ins cat: ARITH, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 19
        FLAGS access
                CF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1

00000000000000E3 66480f38f603                    ADCX      rax, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: ADX, Ins cat: ARITH, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 19
        FLAGS access
                CF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1

00000000000000E9 f3480f38f6c1                    ADOX      rax, rcx
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: ADX, Ins cat: ARITH, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 19
        FLAGS access
                OF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:  General Purpose, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1

00000000000000EF f3480f38f603                    ADOX      rax, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: -
        ISA Set: ADX, Ins cat: ARITH, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 19
        FLAGS access
                OF: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:  General Purpose, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:            Flags, RegSize:  8, RegId: 0, RegCount: 1

