0000000000000000 e8fdff                          CALL      0x0
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  2, RawSize:  2, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Shadow stack: 3, 
                

0000000000000003 ffd0                            CALL      ax
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: M, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Shadow stack: 3, 
                

0000000000000005 66ffd0                          CALL      eax
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Shadow stack: 3, 
                

0000000000000008 ff17                            CALL      word ptr [bx]
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Shadow stack: 3, 
                

000000000000000A 67ff13                          CALL      word ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Shadow stack: 3, 
                

000000000000000D 67ff13                          CALL      word ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Shadow stack: 3, 
                

0000000000000010 6667ff13                        CALL      dword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Shadow stack: 3, 
                

0000000000000014 ebfe                            JMP       0x14
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  2, RawSize:  1, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000016 ffe0                            JMP       ax
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: M, RegType:  General Purpose, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000018 66ffe0                          JMP       eax
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1

000000000000001B ff27                            JMP       word ptr [bx]
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

000000000000001D 67ff23                          JMP       word ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000020 67ff23                          JMP       word ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000023 6667ff23                        JMP       dword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: yes
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1

0000000000000027 9a00102000                      CALLF     0x0020:0x1000
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:    Address, Size:  4, RawSize:  4, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Shadow stack: 3, 
                

000000000000002C 669a000000102000                CALLF     0x0020:0x10000000
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:    Address, Size:  6, RawSize:  6, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

0000000000000034 ea00102000                      JMPF      0x0020:0x1000
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:    Address, Size:  4, RawSize:  4, Encoding: D
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000039 669a000000102000                CALLF     0x0020:0x10000000
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: no
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:    Address, Size:  6, RawSize:  6, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

0000000000000041 67ff1b                          CALLF     dword ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Shadow stack: 3, 
                

0000000000000044 ff1f                            CALLF     dword ptr [bx]
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Shadow stack: 3, 
                

0000000000000046 6667ff1b                        CALLF     fword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

000000000000004A 66ff1f                          CALLF     fword ptr [bx]
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: CALL, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 3, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  8, RawSize:  8, Encoding: S, Shadow stack: 3, 
                

000000000000004D 67ff2b                          JMPF      dword ptr [ebx]
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000050 ff2f                            JMPF      dword ptr [bx]
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000052 6667ff2b                        JMPF      fword ptr [ebx]
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1

0000000000000056 66ff2f                          JMPF      fword ptr [bx]
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: UNCOND_BR, CET tracked: yes
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1

0000000000000059 72fe                            JC        0x59
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        FLAGS access
                CF: t, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: yes, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  2, RawSize:  1, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1

000000000000005B 73fe                            JNC       0x5b
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        FLAGS access
                CF: t, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: yes, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  2, RawSize:  1, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1

000000000000005D e2fe                            LOOP      0x5d
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  2, RawSize:  1, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1

000000000000005F e0fe                            LOOPNZ    0x5f
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        FLAGS access
                ZF: t, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  2, RawSize:  1, Encoding: D
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1

0000000000000061 e3fe                            JCXZ      0x61
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  2, RawSize:  1, Encoding: D
        Operand: 1, Acc:  R-,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000063 67e3fd                          JECXZ     0x63
        DSIZE: 16, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: COND_BR, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:     Offset, Size:  2, RawSize:  1, Encoding: D
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1

0000000000000066 cd21                            INT       0x21
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: INTERRUPT, CET tracked: no
        FLAGS access
                TF: m, IF: m, NT: m, RF: m, VM: tm, AC: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 3, Acc:  RW,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 5, Acc:  -W,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Shadow stack: 3, 
                

0000000000000068 cc                              INT3
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: INTERRUPT, CET tracked: no
        FLAGS access
                TF: m, IF: m, NT: m, RF: m, VM: tm, AC: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  RW,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 4, Acc:  -W,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Shadow stack: 3, 
                

0000000000000069 f1                              INT1
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: INTERRUPT, CET tracked: no
        FLAGS access
                TF: m, IF: m, NT: m, RF: m, VM: tm, AC: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  RW,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1

000000000000006A f1                              INT1
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: INTERRUPT, CET tracked: no
        FLAGS access
                TF: m, IF: m, NT: m, RF: m, VM: tm, AC: m, 
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: no, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 1, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  RW,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1

000000000000006B c3                              RETN
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Shadow stack: 3, 
                

000000000000006C c22000                          RETN      0x0020
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: yes, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  2, RawSize:  2, Encoding: I
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:  General Purpose, RegSize:  2, RegId: 4, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  R-,  Type:     Memory, Size:  2, RawSize:  2, Encoding: S, Shadow stack: 3, 
                

000000000000006F cb                              RETF
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Shadow stack: 3, 
                

0000000000000070 ca2000                          RETF      0x0020
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:  Immediate, Size:  2, RawSize:  2, Encoding: I
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 2, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 4, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: S, Shadow stack: 3, 
                

0000000000000073 cf                              IRETW
        DSIZE: 16, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:          Segment, RegSize:  2, RegId: 1, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:               IP, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  RW,  Type:   Register, Size:  2, RawSize:  2, Encoding: S, RegType:            Flags, RegSize:  2, RegId: 0, RegCount: 1
        Operand: 4, Acc:  RW,  Type:     Memory, Size:  6, RawSize:  6, Encoding: S, Shadow stack: 3, 
                

0000000000000074 66cf                            IRETD
        DSIZE: 32, ASIZE: 16, VLEN: -
        ISA Set: I86, Ins cat: RET, CET tracked: no
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Stack: yes, 
                Segment: 2, Base: 4, 
        Operand: 3, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 4, Acc:  RW,  Type:     Memory, Size: 12, RawSize: 12, Encoding: S, Shadow stack: 3, 
                

