0000000000000000 6202fd48c8c7                    VEXP2PD   zmm24, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000006 6202fd18c8c7                    VEXP2PD   zmm24, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000000C 6262fd48c803                    VEXP2PD   zmm24, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000012 6262fd58c803                    VEXP2PD   zmm24, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

0000000000000018 6222fd48c844db04                VEXP2PD   zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000020 6222fd48c844dbfc                VEXP2PD   zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000028 6202fd4dc8c7                    VEXP2PD   zmm24{k5}, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000002E 6202fd1dc8c7                    VEXP2PD   zmm24{k5}, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000034 6262fd4dc803                    VEXP2PD   zmm24{k5}, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000003A 6262fd5dc803                    VEXP2PD   zmm24{k5}, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

0000000000000040 6222fd4dc844db04                VEXP2PD   zmm24{k5}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000048 6222fd4dc844dbfc                VEXP2PD   zmm24{k5}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000050 6202fdc8c8c7                    VEXP2PD   zmm24, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000056 6202fd98c8c7                    VEXP2PD   zmm24, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000005C 6262fdc8c803                    VEXP2PD   zmm24, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000062 6262fdd8c803                    VEXP2PD   zmm24, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

0000000000000068 6222fdc8c844db04                VEXP2PD   zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000070 6222fdc8c844dbfc                VEXP2PD   zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000078 6202fdcdc8c7                    VEXP2PD   zmm24{k5}{z}, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000007E 6202fd9dc8c7                    VEXP2PD   zmm24{k5}{z}, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000084 6262fdcdc803                    VEXP2PD   zmm24{k5}{z}, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000008A 6262fdddc803                    VEXP2PD   zmm24{k5}{z}, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

0000000000000090 6222fdcdc844db04                VEXP2PD   zmm24{k5}{z}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000098 6222fdcdc844dbfc                VEXP2PD   zmm24{k5}{z}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000000A0 62027d48c8c7                    VEXP2PS   zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000000A6 62027d18c8c7                    VEXP2PS   zmm24, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000000AC 62627d48c803                    VEXP2PS   zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000B2 62627d58c803                    VEXP2PS   zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

00000000000000B8 62227d48c844db04                VEXP2PS   zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000000C0 62227d48c844dbfc                VEXP2PS   zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000000C8 62027d4dc8c7                    VEXP2PS   zmm24{k5}, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000000CE 62027d1dc8c7                    VEXP2PS   zmm24{k5}, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000000D4 62627d4dc803                    VEXP2PS   zmm24{k5}, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000DA 62627d5dc803                    VEXP2PS   zmm24{k5}, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

00000000000000E0 62227d4dc844db04                VEXP2PS   zmm24{k5}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000000E8 62227d4dc844dbfc                VEXP2PS   zmm24{k5}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000000F0 62027dc8c8c7                    VEXP2PS   zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000000F6 62027d98c8c7                    VEXP2PS   zmm24, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000000FC 62627dc8c803                    VEXP2PS   zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000102 62627dd8c803                    VEXP2PS   zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000108 62227dc8c844db04                VEXP2PS   zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000110 62227dc8c844dbfc                VEXP2PS   zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000118 62027dcdc8c7                    VEXP2PS   zmm24{k5}{z}, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000011E 62027d9dc8c7                    VEXP2PS   zmm24{k5}{z}, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000124 62627dcdc803                    VEXP2PS   zmm24{k5}{z}, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000012A 62627dddc803                    VEXP2PS   zmm24{k5}{z}, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000130 62227dcdc844db04                VEXP2PS   zmm24{k5}{z}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000138 62227dcdc844dbfc                VEXP2PS   zmm24{k5}{z}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000140 6202fd48cac7                    VRCP28PD  zmm24, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000146 6202fd18cac7                    VRCP28PD  zmm24, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000014C 6262fd48ca03                    VRCP28PD  zmm24, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000152 6262fd58ca03                    VRCP28PD  zmm24, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

0000000000000158 6222fd48ca44db04                VRCP28PD  zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000160 6222fd48ca44dbfc                VRCP28PD  zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000168 6202fd4dcac7                    VRCP28PD  zmm24{k5}, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000016E 6202fd1dcac7                    VRCP28PD  zmm24{k5}, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000174 6262fd4dca03                    VRCP28PD  zmm24{k5}, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000017A 6262fd5dca03                    VRCP28PD  zmm24{k5}, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

0000000000000180 6222fd4dca44db04                VRCP28PD  zmm24{k5}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000188 6222fd4dca44dbfc                VRCP28PD  zmm24{k5}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000190 6202fdc8cac7                    VRCP28PD  zmm24, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000196 6202fd98cac7                    VRCP28PD  zmm24, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000019C 6262fdc8ca03                    VRCP28PD  zmm24, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000001A2 6262fdd8ca03                    VRCP28PD  zmm24, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

00000000000001A8 6222fdc8ca44db04                VRCP28PD  zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000001B0 6222fdc8ca44dbfc                VRCP28PD  zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000001B8 6202fdcdcac7                    VRCP28PD  zmm24{k5}{z}, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000001BE 6202fd9dcac7                    VRCP28PD  zmm24{k5}{z}, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000001C4 6262fdcdca03                    VRCP28PD  zmm24{k5}{z}, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000001CA 6262fdddca03                    VRCP28PD  zmm24{k5}{z}, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

00000000000001D0 6222fdcdca44db04                VRCP28PD  zmm24{k5}{z}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000001D8 6222fdcdca44dbfc                VRCP28PD  zmm24{k5}{z}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000001E0 62027d48cac7                    VRCP28PS  zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000001E6 62027d18cac7                    VRCP28PS  zmm24, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000001EC 62627d48ca03                    VRCP28PS  zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000001F2 62627d58ca03                    VRCP28PS  zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

00000000000001F8 62227d48ca44db04                VRCP28PS  zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000200 62227d48ca44dbfc                VRCP28PS  zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000208 62027d4dcac7                    VRCP28PS  zmm24{k5}, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000020E 62027d1dcac7                    VRCP28PS  zmm24{k5}, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000214 62627d4dca03                    VRCP28PS  zmm24{k5}, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000021A 62627d5dca03                    VRCP28PS  zmm24{k5}, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000220 62227d4dca44db04                VRCP28PS  zmm24{k5}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000228 62227d4dca44dbfc                VRCP28PS  zmm24{k5}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000230 62027dc8cac7                    VRCP28PS  zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000236 62027d98cac7                    VRCP28PS  zmm24, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000023C 62627dc8ca03                    VRCP28PS  zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000242 62627dd8ca03                    VRCP28PS  zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000248 62227dc8ca44db04                VRCP28PS  zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000250 62227dc8ca44dbfc                VRCP28PS  zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000258 62027dcdcac7                    VRCP28PS  zmm24{k5}{z}, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000025E 62027d9dcac7                    VRCP28PS  zmm24{k5}{z}, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000264 62627dcdca03                    VRCP28PS  zmm24{k5}{z}, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000026A 62627dddca03                    VRCP28PS  zmm24{k5}{z}, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000270 62227dcdca44db04                VRCP28PS  zmm24{k5}{z}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000278 62227dcdca44dbfc                VRCP28PS  zmm24{k5}{z}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000280 62f2c508cbd0                    VRCP28SD  xmm2, xmm7, xmm0
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000286 62f2c518cbd0                    VRCP28SD  xmm2, xmm7, xmm0, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000028C 62f2c508cb13                    VRCP28SD  xmm2, xmm7, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000292 62b2c508cb54db20                VRCP28SD  xmm2, xmm7, qword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000020, 

000000000000029A 62b2c508cb54dbe0                VRCP28SD  xmm2, xmm7, qword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffe0, 

00000000000002A2 62f2c50dcbd0                    VRCP28SD  xmm2{k5}, xmm7, xmm0
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000002A8 62f2c51dcbd0                    VRCP28SD  xmm2{k5}, xmm7, xmm0, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000002AE 62f2c50dcb13                    VRCP28SD  xmm2{k5}, xmm7, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002B4 62b2c50dcb54db20                VRCP28SD  xmm2{k5}, xmm7, qword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000020, 

00000000000002BC 62b2c50dcb54dbe0                VRCP28SD  xmm2{k5}, xmm7, qword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffe0, 

00000000000002C4 62f2c588cbd0                    VRCP28SD  xmm2, xmm7, xmm0
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000002CA 62f2c598cbd0                    VRCP28SD  xmm2, xmm7, xmm0, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000002D0 62f2c588cb13                    VRCP28SD  xmm2, xmm7, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002D6 62b2c588cb54db20                VRCP28SD  xmm2, xmm7, qword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000020, 

00000000000002DE 62b2c588cb54dbe0                VRCP28SD  xmm2, xmm7, qword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffe0, 

00000000000002E6 62f2c58dcbd0                    VRCP28SD  xmm2{k5}{z}, xmm7, xmm0
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000002EC 62f2c59dcbd0                    VRCP28SD  xmm2{k5}{z}, xmm7, xmm0, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000002F2 62f2c58dcb13                    VRCP28SD  xmm2{k5}{z}, xmm7, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000002F8 62b2c58dcb54db20                VRCP28SD  xmm2{k5}{z}, xmm7, qword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000020, 

0000000000000300 62b2c58dcb54dbe0                VRCP28SD  xmm2{k5}{z}, xmm7, qword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffe0, 

0000000000000308 62f24508cbd0                    VRCP28SS  xmm2, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000030E 62f24518cbd0                    VRCP28SS  xmm2, xmm7, xmm0, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000314 62f24508cb13                    VRCP28SS  xmm2, xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000031A 62b24508cb54db40                VRCP28SS  xmm2, xmm7, dword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000040, 

0000000000000322 62b24508cb54dbc0                VRCP28SS  xmm2, xmm7, dword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffc0, 

000000000000032A 62f2450dcbd0                    VRCP28SS  xmm2{k5}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000330 62f2451dcbd0                    VRCP28SS  xmm2{k5}, xmm7, xmm0, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000336 62f2450dcb13                    VRCP28SS  xmm2{k5}, xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000033C 62b2450dcb54db40                VRCP28SS  xmm2{k5}, xmm7, dword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000040, 

0000000000000344 62b2450dcb54dbc0                VRCP28SS  xmm2{k5}, xmm7, dword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffc0, 

000000000000034C 62f24588cbd0                    VRCP28SS  xmm2, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000352 62f24598cbd0                    VRCP28SS  xmm2, xmm7, xmm0, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000358 62f24588cb13                    VRCP28SS  xmm2, xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000035E 62b24588cb54db40                VRCP28SS  xmm2, xmm7, dword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000040, 

0000000000000366 62b24588cb54dbc0                VRCP28SS  xmm2, xmm7, dword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffc0, 

000000000000036E 62f2458dcbd0                    VRCP28SS  xmm2{k5}{z}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000374 62f2459dcbd0                    VRCP28SS  xmm2{k5}{z}, xmm7, xmm0, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000037A 62f2458dcb13                    VRCP28SS  xmm2{k5}{z}, xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000380 62b2458dcb54db40                VRCP28SS  xmm2{k5}{z}, xmm7, dword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000040, 

0000000000000388 62b2458dcb54dbc0                VRCP28SS  xmm2{k5}{z}, xmm7, dword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffc0, 

0000000000000390 6202fd48ccc7                    VRSQRT28PD zmm24, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000396 6202fd18ccc7                    VRSQRT28PD zmm24, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000039C 6262fd48cc03                    VRSQRT28PD zmm24, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003A2 6262fd58cc03                    VRSQRT28PD zmm24, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

00000000000003A8 6222fd48cc44db04                VRSQRT28PD zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000003B0 6222fd48cc44dbfc                VRSQRT28PD zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000003B8 6202fd4dccc7                    VRSQRT28PD zmm24{k5}, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000003BE 6202fd1dccc7                    VRSQRT28PD zmm24{k5}, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000003C4 6262fd4dcc03                    VRSQRT28PD zmm24{k5}, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003CA 6262fd5dcc03                    VRSQRT28PD zmm24{k5}, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

00000000000003D0 6222fd4dcc44db04                VRSQRT28PD zmm24{k5}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000003D8 6222fd4dcc44dbfc                VRSQRT28PD zmm24{k5}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000003E0 6202fdc8ccc7                    VRSQRT28PD zmm24, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000003E6 6202fd98ccc7                    VRSQRT28PD zmm24, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000003EC 6262fdc8cc03                    VRSQRT28PD zmm24, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000003F2 6262fdd8cc03                    VRSQRT28PD zmm24, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

00000000000003F8 6222fdc8cc44db04                VRSQRT28PD zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000400 6222fdc8cc44dbfc                VRSQRT28PD zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000408 6202fdcdccc7                    VRSQRT28PD zmm24{k5}{z}, zmm31
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000040E 6202fd9dccc7                    VRSQRT28PD zmm24{k5}{z}, zmm31, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000414 6262fdcdcc03                    VRSQRT28PD zmm24{k5}{z}, zmmword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000041A 6262fdddcc03                    VRSQRT28PD zmm24{k5}{z}, qword ptr [rbx]{1to8}
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times

0000000000000420 6222fdcdcc44db04                VRSQRT28PD zmm24{k5}{z}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000428 6222fdcdcc44dbfc                VRSQRT28PD zmm24{k5}{z}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000430 62027d48ccc7                    VRSQRT28PS zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000436 62027d18ccc7                    VRSQRT28PS zmm24, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000043C 62627d48cc03                    VRSQRT28PS zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000442 62627d58cc03                    VRSQRT28PS zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000448 62227d48cc44db04                VRSQRT28PS zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000450 62227d48cc44dbfc                VRSQRT28PS zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000458 62027d4dccc7                    VRSQRT28PS zmm24{k5}, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000045E 62027d1dccc7                    VRSQRT28PS zmm24{k5}, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000464 62627d4dcc03                    VRSQRT28PS zmm24{k5}, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000046A 62627d5dcc03                    VRSQRT28PS zmm24{k5}, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000470 62227d4dcc44db04                VRSQRT28PS zmm24{k5}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

0000000000000478 62227d4dcc44dbfc                VRSQRT28PS zmm24{k5}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

0000000000000480 62027dc8ccc7                    VRSQRT28PS zmm24, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

0000000000000486 62027d98ccc7                    VRSQRT28PS zmm24, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

000000000000048C 62627dc8cc03                    VRSQRT28PS zmm24, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000492 62627dd8cc03                    VRSQRT28PS zmm24, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

0000000000000498 62227dc8cc44db04                VRSQRT28PS zmm24, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000004A0 62227dc8cc44dbfc                VRSQRT28PS zmm24, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000004A8 62027dcdccc7                    VRSQRT28PS zmm24{k5}{z}, zmm31
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000004AE 62027d9dccc7                    VRSQRT28PS zmm24{k5}{z}, zmm31, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1

00000000000004B4 62627dcdcc03                    VRSQRT28PS zmm24{k5}{z}, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004BA 62627dddcc03                    VRSQRT28PS zmm24{k5}{z}, dword ptr [rbx]{1to16}
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 4 bytes element 16 times

00000000000004C0 62227dcdcc44db04                VRSQRT28PS zmm24{k5}{z}, zmmword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000004, 

00000000000004C8 62227dcdcc44dbfc                VRSQRT28PS zmm24{k5}{z}, zmmword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E2
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 24, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xfffffffffffffffc, 

00000000000004D0 62f2c508cdd0                    VRSQRT28SD xmm2, xmm7, xmm0
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000004D6 62f2c518cdd0                    VRSQRT28SD xmm2, xmm7, xmm0, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000004DC 62f2c508cd13                    VRSQRT28SD xmm2, xmm7, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000004E2 62b2c508cd54db20                VRSQRT28SD xmm2, xmm7, qword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000020, 

00000000000004EA 62b2c508cd54dbe0                VRSQRT28SD xmm2, xmm7, qword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffe0, 

00000000000004F2 62f2c50dcdd0                    VRSQRT28SD xmm2{k5}, xmm7, xmm0
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000004F8 62f2c51dcdd0                    VRSQRT28SD xmm2{k5}, xmm7, xmm0, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000004FE 62f2c50dcd13                    VRSQRT28SD xmm2{k5}, xmm7, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000504 62b2c50dcd54db20                VRSQRT28SD xmm2{k5}, xmm7, qword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000020, 

000000000000050C 62b2c50dcd54dbe0                VRSQRT28SD xmm2{k5}, xmm7, qword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffe0, 

0000000000000514 62f2c588cdd0                    VRSQRT28SD xmm2, xmm7, xmm0
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000051A 62f2c598cdd0                    VRSQRT28SD xmm2, xmm7, xmm0, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000520 62f2c588cd13                    VRSQRT28SD xmm2, xmm7, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000526 62b2c588cd54db20                VRSQRT28SD xmm2, xmm7, qword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000020, 

000000000000052E 62b2c588cd54dbe0                VRSQRT28SD xmm2, xmm7, qword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffe0, 

0000000000000536 62f2c58dcdd0                    VRSQRT28SD xmm2{k5}{z}, xmm7, xmm0
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000053C 62f2c59dcdd0                    VRSQRT28SD xmm2{k5}{z}, xmm7, xmm0, {sae}
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000542 62f2c58dcd13                    VRSQRT28SD xmm2{k5}{z}, xmm7, qword ptr [rbx]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000548 62b2c58dcd54db20                VRSQRT28SD xmm2{k5}{z}, xmm7, qword ptr [rbx+r11*8+0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000020, 

0000000000000550 62b2c58dcd54dbe0                VRSQRT28SD xmm2{k5}{z}, xmm7, qword ptr [rbx+r11*8-0x100]
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffe0, 

0000000000000558 62f24508cdd0                    VRSQRT28SS xmm2, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

000000000000055E 62f24518cdd0                    VRSQRT28SS xmm2, xmm7, xmm0, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000564 62f24508cd13                    VRSQRT28SS xmm2, xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000056A 62b24508cd54db40                VRSQRT28SS xmm2, xmm7, dword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000040, 

0000000000000572 62b24508cd54dbc0                VRSQRT28SS xmm2, xmm7, dword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffc0, 

000000000000057A 62f2450dcdd0                    VRSQRT28SS xmm2{k5}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000580 62f2451dcdd0                    VRSQRT28SS xmm2{k5}, xmm7, xmm0, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

0000000000000586 62f2450dcd13                    VRSQRT28SS xmm2{k5}, xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000058C 62b2450dcd54db40                VRSQRT28SS xmm2{k5}, xmm7, dword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000040, 

0000000000000594 62b2450dcd54dbc0                VRSQRT28SS xmm2{k5}, xmm7, dword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffc0, 

000000000000059C 62f24588cdd0                    VRSQRT28SS xmm2, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000005A2 62f24598cdd0                    VRSQRT28SS xmm2, xmm7, xmm0, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000005A8 62f24588cd13                    VRSQRT28SS xmm2, xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000005AE 62b24588cd54db40                VRSQRT28SS xmm2, xmm7, dword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000040, 

00000000000005B6 62b24588cd54dbc0                VRSQRT28SS xmm2, xmm7, dword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffc0, 

00000000000005BE 62f2458dcdd0                    VRSQRT28SS xmm2{k5}{z}, xmm7, xmm0
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000005C4 62f2459dcdd0                    VRSQRT28SS xmm2{k5}{z}, xmm7, xmm0, {sae}
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 0, RegCount: 1

00000000000005CA 62f2458dcd13                    VRSQRT28SS xmm2{k5}{z}, xmm7, dword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000005D0 62b2458dcd54db40                VRSQRT28SS xmm2{k5}{z}, xmm7, dword ptr [rbx+r11*8+0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0x0000000000000040, 

00000000000005D8 62b2458dcd54dbc0                VRSQRT28SS xmm2{k5}{z}, xmm7, dword ptr [rbx+r11*8-0x100]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX512ER, Ins cat: KNL, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ebx, bit: 27
        EVEX Tuple Type: Tuple 1 Scalar
        Exception class: EVEX, exception type: E3
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  4, RawSize:  4, Encoding: M, Compressed displacement: yes, 
                Segment: 3, Base: 3, Index: 11 * 8, Displacement: 0xffffffffffffffc0, 

