0000000000000000 c4e2919294fb00100000            VGATHERDPD xmm2, qword ptr [rbx+xmm7*8+0x1000], xmm13
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 7 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 4, VSIB element size: 8, VSIB element count: 2
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000000A c4e2119294fb00100000            VGATHERDPS xmm2, dword ptr [rbx+xmm7*8+0x1000], xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 7 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 4, VSIB element size: 4, VSIB element count: 4
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000014 c4e2919394fb00100000            VGATHERQPD xmm2, qword ptr [rbx+xmm7*8+0x1000], xmm13
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 7 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 8, VSIB element size: 8, VSIB element count: 2
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000001E c4e2119394fb00100000            VGATHERQPS xmm2, dword ptr [rbx+xmm7*8+0x1000], xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 7 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 8, VSIB element size: 4, VSIB element count: 2
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000028 c4e2159394cb00100000            VGATHERQPS xmm2, dword ptr [rbx+ymm1*8+0x1000], xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 1 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 8, VSIB element size: 4, VSIB element count: 4
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000032 c4e2119094fb00100000            VPGATHERDD xmm2, dword ptr [rbx+xmm7*8+0x1000], xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 7 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 4, VSIB element size: 4, VSIB element count: 4
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000003C c4e2919094fb00100000            VPGATHERDQ xmm2, qword ptr [rbx+xmm7*8+0x1000], xmm13
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 7 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 4, VSIB element size: 8, VSIB element count: 2
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000046 c4e2119194fb00100000            VPGATHERQD xmm2, dword ptr [rbx+xmm7*8+0x1000], xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 7 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 8, VSIB element size: 4, VSIB element count: 2
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000050 c4e2159194cb00100000            VPGATHERQD xmm2, dword ptr [rbx+ymm1*8+0x1000], xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 1 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 8, VSIB element size: 4, VSIB element count: 4
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000005A c4e2919194fb00100000            VPGATHERQQ xmm2, qword ptr [rbx+xmm7*8+0x1000], xmm13
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: AVX2GATHER, Ins cat: AVX2GATHER, CET tracked: no
        Exception class: SSE/VEX, exception type: 12
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  CRW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 2, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, VSIB Addressing: yes, 
                Segment: 3, Base: 3, Index: 7 * 8, Displacement: 0x0000000000001000, 
                VSIB index size: 8, VSIB element size: 8, VSIB element count: 2
        Operand: 2, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

