From: jbeulich@novell.com
Subject: Xen: para-virtual watchdog driver
Patch-mainline: n/a

--- head-2011-01-30.orig/drivers/watchdog/Kconfig	2011-01-31 12:42:35.000000000 +0100
+++ head-2011-01-30/drivers/watchdog/Kconfig	2011-02-02 15:10:41.000000000 +0100
@@ -1119,6 +1119,16 @@ config WATCHDOG_RIO
 
 # XTENSA Architecture
 
+# Xen Architecture
+
+config XEN_WDT
+	tristate "Xen Watchdog support"
+	depends on PARAVIRT_XEN || XEN
+	help
+	  Say Y here to support the hypervisor watchdog capability provided
+	  by Xen 4.0 and newer.  The watchdog timeout period is normally one
+	  minute but can be changed with a boot-time parameter.
+
 #
 # ISA-based Watchdog Cards
 #
--- head-2011-01-30.orig/drivers/watchdog/Makefile	2011-01-31 12:42:35.000000000 +0100
+++ head-2011-01-30/drivers/watchdog/Makefile	2011-02-02 15:10:41.000000000 +0100
@@ -148,6 +148,9 @@ obj-$(CONFIG_WATCHDOG_CP1XXX)		+= cpwd.o
 
 # XTENSA Architecture
 
+# Xen
+obj-$(CONFIG_XEN_WDT) += xen_wdt.o
+
 # Architecture Independant
 obj-$(CONFIG_WM831X_WATCHDOG) += wm831x_wdt.o
 obj-$(CONFIG_WM8350_WATCHDOG) += wm8350_wdt.o
--- /dev/null	1970-01-01 00:00:00.000000000 +0000
+++ head-2011-01-30/drivers/watchdog/xen_wdt.c	2011-02-02 15:10:41.000000000 +0100
@@ -0,0 +1,360 @@
+/*
+ *	Xen Watchdog Driver
+ *
+ *	(c) Copyright 2010 Novell, Inc.
+ *
+ *	This program is free software; you can redistribute it and/or
+ *	modify it under the terms of the GNU General Public License
+ *	as published by the Free Software Foundation; either version
+ *	2 of the License, or (at your option) any later version.
+ */
+
+#define DRV_NAME	"wdt"
+#define DRV_VERSION	"0.01"
+#define PFX		DRV_NAME ": "
+
+#include <linux/bug.h>
+#include <linux/errno.h>
+#include <linux/fs.h>
+#include <linux/hrtimer.h>
+#include <linux/kernel.h>
+#include <linux/ktime.h>
+#include <linux/init.h>
+#include <linux/miscdevice.h>
+#include <linux/module.h>
+#include <linux/moduleparam.h>
+#include <linux/platform_device.h>
+#include <linux/spinlock.h>
+#include <linux/uaccess.h>
+#include <linux/watchdog.h>
+#ifdef CONFIG_PARAVIRT_XEN
+#include <xen/xen.h>
+#include <asm/xen/hypercall.h>
+#endif
+#include <xen/interface/sched.h>
+
+static struct platform_device *platform_device;
+static DEFINE_SPINLOCK(wdt_lock);
+static struct sched_watchdog wdt;
+static __kernel_time_t wdt_expires;
+static bool is_active, expect_release;
+
+#define WATCHDOG_TIMEOUT 60 /* in seconds */
+static unsigned int timeout = WATCHDOG_TIMEOUT;
+module_param(timeout, uint, S_IRUGO);
+MODULE_PARM_DESC(timeout, "Watchdog timeout in seconds "
+	"(default=" __MODULE_STRING(WATCHDOG_TIMEOUT) ")");
+
+static bool nowayout = WATCHDOG_NOWAYOUT;
+module_param(nowayout, bool, S_IRUGO);
+MODULE_PARM_DESC(nowayout, "Watchdog cannot be stopped once started "
+	"(default=" __MODULE_STRING(WATCHDOG_NOWAYOUT) ")");
+
+static inline __kernel_time_t set_timeout(void)
+{
+	wdt.timeout = timeout;
+	return ktime_to_timespec(ktime_get()).tv_sec + timeout;
+}
+
+static int xen_wdt_start(void)
+{
+	__kernel_time_t expires;
+	int err;
+
+	spin_lock(&wdt_lock);
+
+	expires = set_timeout();
+	if (!wdt.id)
+		err = HYPERVISOR_sched_op(SCHEDOP_watchdog, &wdt);
+	else
+		err = -EBUSY;
+	if (err > 0) {
+		wdt.id = err;
+		wdt_expires = expires;
+		err = 0;
+	} else
+		BUG_ON(!err);
+
+	spin_unlock(&wdt_lock);
+
+	return err;
+}
+
+static int xen_wdt_stop(void)
+{
+	int err = 0;
+
+	spin_lock(&wdt_lock);
+
+	wdt.timeout = 0;
+	if (wdt.id)
+		err = HYPERVISOR_sched_op(SCHEDOP_watchdog, &wdt);
+	if (!err)
+		wdt.id = 0;
+
+	spin_unlock(&wdt_lock);
+
+	return err;
+}
+
+static int xen_wdt_kick(void)
+{
+	__kernel_time_t expires;
+	int err;
+
+	spin_lock(&wdt_lock);
+
+	expires = set_timeout();
+	if (wdt.id)
+		err = HYPERVISOR_sched_op(SCHEDOP_watchdog, &wdt);
+	else
+		err = -ENXIO;
+	if (!err)
+		wdt_expires = expires;
+
+	spin_unlock(&wdt_lock);
+
+	return err;
+}
+
+static int xen_wdt_open(struct inode *inode, struct file *file)
+{
+	int err;
+
+	/* /dev/watchdog can only be opened once */
+	if (xchg(&is_active, true))
+		return -EBUSY;
+
+	err = xen_wdt_start();
+	if (err == -EBUSY)
+		err = xen_wdt_kick();
+	return err ?: nonseekable_open(inode, file);
+}
+
+static int xen_wdt_release(struct inode *inode, struct file *file)
+{
+	if (expect_release)
+		xen_wdt_stop();
+	else {
+		pr_crit(PFX "unexpected close, not stopping watchdog!\n");
+		xen_wdt_kick();
+	}
+	is_active = false;
+	expect_release = false;
+	return 0;
+}
+
+static ssize_t xen_wdt_write(struct file *file, const char __user *data,
+			     size_t len, loff_t *ppos)
+{
+	/* See if we got the magic character 'V' and reload the timer */
+	if (len) {
+		if (!nowayout) {
+			size_t i;
+
+			/* in case it was set long ago */
+			expect_release = false;
+
+			/* scan to see whether or not we got the magic
+			   character */
+			for (i = 0; i != len; i++) {
+				char c;
+				if (get_user(c, data + i))
+					return -EFAULT;
+				if (c == 'V')
+					expect_release = true;
+			}
+		}
+
+		/* someone wrote to us, we should reload the timer */
+		xen_wdt_kick();
+	}
+	return len;
+}
+
+static long xen_wdt_ioctl(struct file *file, unsigned int cmd,
+			  unsigned long arg)
+{
+	int new_options, retval = -EINVAL;
+	int new_timeout;
+	int __user *argp = (void __user *)arg;
+	static const struct watchdog_info ident = {
+		.options =		WDIOF_SETTIMEOUT | WDIOF_MAGICCLOSE,
+		.firmware_version =	0,
+		.identity =		DRV_NAME,
+	};
+
+	switch (cmd) {
+	case WDIOC_GETSUPPORT:
+		return copy_to_user(argp, &ident, sizeof(ident)) ? -EFAULT : 0;
+
+	case WDIOC_GETSTATUS:
+	case WDIOC_GETBOOTSTATUS:
+		return put_user(0, argp);
+
+	case WDIOC_SETOPTIONS:
+		if (get_user(new_options, argp))
+			return -EFAULT;
+
+		if (new_options & WDIOS_DISABLECARD)
+			retval = xen_wdt_stop();
+		if (new_options & WDIOS_ENABLECARD) {
+			retval = xen_wdt_start();
+			if (retval == -EBUSY)
+				retval = xen_wdt_kick();
+		}
+		return retval;
+
+	case WDIOC_KEEPALIVE:
+		xen_wdt_kick();
+		return 0;
+
+	case WDIOC_SETTIMEOUT:
+		if (get_user(new_timeout, argp))
+			return -EFAULT;
+		if (!new_timeout)
+			return -EINVAL;
+		timeout = new_timeout;
+		xen_wdt_kick();
+		/* fall through */
+	case WDIOC_GETTIMEOUT:
+		return put_user(timeout, argp);
+
+	case WDIOC_GETTIMELEFT:
+		retval = wdt_expires - ktime_to_timespec(ktime_get()).tv_sec;
+		return put_user(retval, argp);
+	}
+
+	return -ENOTTY;
+}
+
+static const struct file_operations xen_wdt_fops = {
+	.owner =		THIS_MODULE,
+	.llseek =		no_llseek,
+	.write =		xen_wdt_write,
+	.unlocked_ioctl =	xen_wdt_ioctl,
+	.open =			xen_wdt_open,
+	.release =		xen_wdt_release,
+};
+
+static struct miscdevice xen_wdt_miscdev = {
+	.minor =	WATCHDOG_MINOR,
+	.name =		"watchdog",
+	.fops =		&xen_wdt_fops,
+};
+
+static int __devinit xen_wdt_probe(struct platform_device *dev)
+{
+	struct sched_watchdog wd = { .id = ~0 };
+	int ret = HYPERVISOR_sched_op(SCHEDOP_watchdog, &wd);
+
+	switch (ret) {
+	case -EINVAL:
+		if (!timeout) {
+			timeout = WATCHDOG_TIMEOUT;
+			pr_info(PFX "timeout value invalid, using %d\n",
+				timeout);
+		}
+
+		ret = misc_register(&xen_wdt_miscdev);
+		if (ret) {
+			pr_err(PFX "can't register miscdev on minor=%d (%d)\n",
+			       WATCHDOG_MINOR, ret);
+			break;
+		}
+
+		pr_info(PFX "initialized (timeout=%ds, nowayout=%d)\n",
+			timeout, nowayout);
+		break;
+
+	case -ENOSYS:
+		pr_info(PFX "not supported\n");
+		ret = -ENODEV;
+		break;
+
+	default:
+		pr_warning(PFX "bogus return value %d\n", ret);
+		break;
+	}
+
+	return ret;
+}
+
+static int __devexit xen_wdt_remove(struct platform_device *dev)
+{
+	/* Stop the timer before we leave */
+	if (!nowayout)
+		xen_wdt_stop();
+
+	misc_deregister(&xen_wdt_miscdev);
+
+	return 0;
+}
+
+static void xen_wdt_shutdown(struct platform_device *dev)
+{
+	xen_wdt_stop();
+}
+
+static int xen_wdt_suspend(struct platform_device *dev, pm_message_t state)
+{
+	return xen_wdt_stop();
+}
+
+static int xen_wdt_resume(struct platform_device *dev)
+{
+	return xen_wdt_start();
+}
+
+static struct platform_driver xen_wdt_driver = {
+	.probe          = xen_wdt_probe,
+	.remove         = __devexit_p(xen_wdt_remove),
+	.shutdown       = xen_wdt_shutdown,
+	.suspend        = xen_wdt_suspend,
+	.resume         = xen_wdt_resume,
+	.driver         = {
+		.owner  = THIS_MODULE,
+		.name   = DRV_NAME,
+	},
+};
+
+static int __init xen_wdt_init_module(void)
+{
+	int err;
+
+#ifdef CONFIG_PARAVIRT_XEN
+	if (!xen_domain())
+		return -ENODEV;
+#endif
+
+	pr_info(PFX "Xen WatchDog Timer Driver v%s\n", DRV_VERSION);
+
+	err = platform_driver_register(&xen_wdt_driver);
+	if (err)
+		return err;
+
+	platform_device = platform_device_register_simple(DRV_NAME,
+								  -1, NULL, 0);
+	if (IS_ERR(platform_device)) {
+		err = PTR_ERR(platform_device);
+		platform_driver_unregister(&xen_wdt_driver);
+	}
+
+	return err;
+}
+
+static void __exit xen_wdt_cleanup_module(void)
+{
+	platform_device_unregister(platform_device);
+	platform_driver_unregister(&xen_wdt_driver);
+	pr_info(PFX "module unloaded\n");
+}
+
+module_init(xen_wdt_init_module);
+module_exit(xen_wdt_cleanup_module);
+
+MODULE_AUTHOR("Jan Beulich <jbeulich@novell.com>");
+MODULE_DESCRIPTION("Xen WatchDog Timer Driver");
+MODULE_VERSION(DRV_VERSION);
+MODULE_LICENSE("GPL");
+MODULE_ALIAS_MISCDEV(WATCHDOG_MINOR);
