Subject: /sys/class/scsi_host/hostX/config doesn't show any information
From: Linda Xie <lxiep@us.ibm.com>
References: 439970 - LTC49349
Patch-mainline: not yet

This patch changes the size of the buffer used for transfering config 
data to 4K. It was tested against 2.6.19-rc2 tree.

Signed-off-by: lxie@us.ibm.com
Signed-off-by: Olaf Hering <olh@suse.de>

---
 drivers/scsi/ibmvscsi/ibmvscsi.c |   14 ++++++++------
 1 file changed, 8 insertions(+), 6 deletions(-)

--- a/drivers/scsi/ibmvscsi/ibmvscsi.c
+++ b/drivers/scsi/ibmvscsi/ibmvscsi.c
@@ -99,6 +99,8 @@ static int max_requests = IBMVSCSI_MAX_R
 static int max_events = IBMVSCSI_MAX_REQUESTS_DEFAULT + 2;
 static int fast_fail = 1;
 static int client_reserve = 1;
+/*host data buffer size*/
+#define buff_size 4096
 
 static struct scsi_transport_template *ibmvscsi_transport_template;
 
@@ -1667,7 +1669,7 @@ static ssize_t show_host_srp_version(str
 	struct ibmvscsi_host_data *hostdata = shost_priv(shost);
 	int len;
 
-	len = snprintf(buf, PAGE_SIZE, "%s\n",
+       len = snprintf(buf, buff_size, "%s\n",
 		       hostdata->madapter_info.srp_version);
 	return len;
 }
@@ -1688,7 +1690,7 @@ static ssize_t show_host_partition_name(
 	struct ibmvscsi_host_data *hostdata = shost_priv(shost);
 	int len;
 
-	len = snprintf(buf, PAGE_SIZE, "%s\n",
+       len = snprintf(buf, buff_size, "%s\n",
 		       hostdata->madapter_info.partition_name);
 	return len;
 }
@@ -1709,7 +1711,7 @@ static ssize_t show_host_partition_numbe
 	struct ibmvscsi_host_data *hostdata = shost_priv(shost);
 	int len;
 
-	len = snprintf(buf, PAGE_SIZE, "%d\n",
+       len = snprintf(buf, buff_size, "%d\n",
 		       hostdata->madapter_info.partition_number);
 	return len;
 }
@@ -1729,7 +1731,7 @@ static ssize_t show_host_mad_version(str
 	struct ibmvscsi_host_data *hostdata = shost_priv(shost);
 	int len;
 
-	len = snprintf(buf, PAGE_SIZE, "%d\n",
+       len = snprintf(buf, buff_size, "%d\n",
 		       hostdata->madapter_info.mad_version);
 	return len;
 }
@@ -1749,7 +1751,7 @@ static ssize_t show_host_os_type(struct
 	struct ibmvscsi_host_data *hostdata = shost_priv(shost);
 	int len;
 
-	len = snprintf(buf, PAGE_SIZE, "%d\n", hostdata->madapter_info.os_type);
+       len = snprintf(buf, buff_size, "%d\n", hostdata->madapter_info.os_type);
 	return len;
 }
 
@@ -1768,7 +1770,7 @@ static ssize_t show_host_config(struct d
 	struct ibmvscsi_host_data *hostdata = shost_priv(shost);
 
 	/* returns null-terminated host config data */
-	if (ibmvscsi_do_host_config(hostdata, buf, PAGE_SIZE) == 0)
+       if (ibmvscsi_do_host_config(hostdata, buf, buff_size) == 0)
 		return strlen(buf);
 	else
 		return 0;
