0000000000000000 f00f20c0                        MOV       eax, cr8
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: DATAXFER, CET tracked: no
        Valid modes
                R0: yes, R1: no, R2: no, R3: no
                Real: yes, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:          Control, RegSize:  4, RegId: 8, RegCount: 1

0000000000000004 f00f22c0                        MOV       cr8, eax
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: I86, Ins cat: DATAXFER, CET tracked: no
        Valid modes
                R0: yes, R1: no, R2: no, R3: no
                Real: yes, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: R, RegType:          Control, RegSize:  4, RegId: 8, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: M, RegType:  General Purpose, RegSize:  4, RegId: 0, RegCount: 1

