0000000000000000 0f                              db 0x0f (0x80000009)
0000000000000010 0f05                            SYSCALL
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: AMD, Ins cat: SYSCALL, CET tracked: yes
        CPUID leaf: 0x80000001, reg: ecx, bit: 11
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: 0xc0000081, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: 0xc0000082, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: 0xc0000084, RegCount: 1
        Operand: 3, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 4, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 1, RegCount: 1
        Operand: 5, Acc:  -W,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 11, RegCount: 1
        Operand: 6, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 7, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 8, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 9, Acc:  RW,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:              SSP, RegSize:  4, RegId: 0, RegCount: 1

0000000000000020 0f07                            SYSRET
        DSIZE: 32, ASIZE: 32, VLEN: -
        ISA Set: AMD, Ins cat: SYSRET, CET tracked: no
        CPUID leaf: 0x80000001, reg: ecx, bit: 11
        FLAGS access
                Entire register
        Valid modes
                R0: yes, R1: no, R2: no, R3: no
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM on: yes, SMM off: yes, SGX on: no, SGX off: yes, TSX on: yes, TSX off: yes
                VMXRoot: yes, VMXNonRoot: yes, VMXRoot SEAM: yes, VMXNonRoot SEAM: yes, VMX off: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:   Model Specific, RegSize:  8, RegId: 0xc0000081, RegCount: 1
        Operand: 1, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 2, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:  General Purpose, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: S, RegType:  General Purpose, RegSize:  8, RegId: 11, RegCount: 1
        Operand: 4, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:          Segment, RegSize:  4, RegId: 1, RegCount: 1
        Operand: 5, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:               IP, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 6, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:            Flags, RegSize:  4, RegId: 0, RegCount: 1
        Operand: 7, Acc:  -W,  Type:   Register, Size:  4, RawSize:  4, Encoding: S, RegType:              SSP, RegSize:  4, RegId: 0, RegCount: 1

0000000000000030 f3                              db 0xf3 (0x80000002)
0000000000000040 f3                              db 0xf3 (0x80000002)
0000000000000050 f3                              db 0xf3 (0x80000002)
0000000000000060 f3                              db 0xf3 (0x80000002)
