0000000000000000 0f0fc70c                        PI2FW     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000004 0f0fc70d                        PI2FD     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000008 0f0fc71c                        PF2IW     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

000000000000000C 0f0fc71d                        PF2ID     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000010 0f0fc786                        PFRCPV    mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000014 0f0fc787                        PFRSQRTV  mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000018 0f0fc78a                        PFNACC    mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

000000000000001C 0f0fc78e                        PFPNACC   mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000020 0f0fc790                        PFCMPGE   mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000024 0f0fc794                        PFMIN     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000028 0f0fc794                        PFMIN     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

000000000000002C 0f0fc797                        PFRSQRT   mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000030 0f0fc79a                        PFSUB     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000034 0f0fc79e                        PFADD     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000038 0f0fc7a0                        PFCMPGT   mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

000000000000003C 0f0fc7a4                        PFMAX     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000040 0f0fc7a6                        PFRCPIT1  mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000044 0f0fc7a7                        PFRSQIT1  mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000048 0f0fc7aa                        PFSUBR    mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

000000000000004C 0f0fc7ae                        PFACC     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000050 0f0fc7b0                        PFCMPEQ   mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000054 0f0fc7b4                        PFMUL     mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000058 0f0fc7b6                        PFRCPIT2  mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

000000000000005C 0f0fc7bb                        PSWAPD    mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000060 0f0fc7bf                        PAVGUSB   mm0, mm7
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: M, RegType:              MMX, RegSize:  8, RegId: 7, RegCount: 1

0000000000000064 0f0f030c                        PI2FW     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000068 0f0f030d                        PI2FD     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000006C 0f0f031c                        PF2IW     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000070 0f0f031d                        PF2ID     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000074 0f0f0386                        PFRCPV    mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000078 0f0f0387                        PFRSQRTV  mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000007C 0f0f038a                        PFNACC    mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000080 0f0f038e                        PFPNACC   mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000084 0f0f0390                        PFCMPGE   mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000088 0f0f0394                        PFMIN     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000008C 0f0f0394                        PFMIN     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000090 0f0f0397                        PFRSQRT   mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000094 0f0f039a                        PFSUB     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000098 0f0f039e                        PFADD     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000009C 0f0f03a0                        PFCMPGT   mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000A0 0f0f03a4                        PFMAX     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000A4 0f0f03a6                        PFRCPIT1  mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000A8 0f0f03a7                        PFRSQIT1  mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000AC 0f0f03aa                        PFSUBR    mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000B0 0f0f03ae                        PFACC     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000B4 0f0f03b0                        PFCMPEQ   mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000B8 0f0f03b4                        PFMUL     mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000BC 0f0f03b6                        PFRCPIT2  mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000C0 0f0f03bb                        PSWAPD    mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000C4 0f0f03bf                        PAVGUSB   mm0, qword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: -
        ISA Set: 3DNOW, Ins cat: 3DNOW, CET tracked: no
        CPUID leaf: 0x80000001, reg: edx, bit: 31
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size:  8, RawSize:  8, Encoding: R, RegType:              MMX, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, 
                Segment: 3, Base: 3, 

