0000000000000000 66410f38cffd                    GF2P8MULB xmm7, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

0000000000000006 66410f3acefd0a                  GF2P8AFFINEQB xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000000D 66410f3acffd0a                  GF2P8AFFINEINVQB xmm7, xmm13, 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000014 660f38cf3b                      GF2P8MULB xmm7, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

0000000000000019 660f3ace3b0a                    GF2P8AFFINEQB xmm7, xmmword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000001F 660f3acf3b0a                    GF2P8AFFINEINVQB xmm7, xmmword ptr [rbx], 0x0a
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: yes, V8086: yes, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  RW,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 2, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000025 c4c201cffd                      VGF2P8MULB xmm7, xmm15, xmm13
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1

000000000000002A c4c381cefd0a                    VGF2P8AFFINEQB xmm7, xmm15, xmm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000030 c4c381cffd0a                    VGF2P8AFFINEINVQB xmm7, xmm15, xmm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: M, RegType:           Vector, RegSize: 16, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000036 c4e201cf3b                      VGF2P8MULB xmm7, xmm15, xmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000003B c4e381ce3b0a                    VGF2P8AFFINEQB xmm7, xmm15, xmmword ptr [rbx], 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 3, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000041 c4e381cf3b0a                    VGF2P8AFFINEINVQB xmm7, xmm15, xmmword ptr [rbx], 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 128
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 16, RawSize: 16, Encoding: R, RegType:           Vector, RegSize: 16, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 16, RawSize: 16, Encoding: V, RegType:           Vector, RegSize: 16, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 16, RawSize: 16, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 3, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000047 c4c205cffd                      VGF2P8MULB ymm7, ymm15, ymm13
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1

000000000000004C c4c385cefd0a                    VGF2P8AFFINEQB ymm7, ymm15, ymm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 256
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000052 c4c385cffd0a                    VGF2P8AFFINEINVQB ymm7, ymm15, ymm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 256
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: M, RegType:           Vector, RegSize: 32, RegId: 13, RegCount: 1
        Operand: 3, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000058 c4e205cf3b                      VGF2P8MULB ymm7, ymm15, ymmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 256
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 

000000000000005D c4e385ce3b0a                    VGF2P8AFFINEQB ymm7, ymm15, ymmword ptr [rbx], 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 256
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 3, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000063 c4e385cf3b0a                    VGF2P8AFFINEINVQB ymm7, ymm15, ymmword ptr [rbx], 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 256
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        Exception class: SSE/VEX, exception type: 4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 32, RawSize: 32, Encoding: R, RegType:           Vector, RegSize: 32, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size: 32, RawSize: 32, Encoding: V, RegType:           Vector, RegSize: 32, RegId: 15, RegCount: 1
        Operand: 2, Acc:  R-,  Type:     Memory, Size: 32, RawSize: 32, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 3, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000069 62d20540cffd                    VGF2P8MULB zmm7, zmm31, zmm13
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full Mem
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1

000000000000006F 62d38540cefd0a                  VGF2P8AFFINEQB zmm7, zmm31, zmm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000076 62d38540cffd0a                  VGF2P8AFFINEINVQB zmm7, zmm31, zmm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000007D 62d20545cffd                    VGF2P8MULB zmm7{k5}, zmm31, zmm13
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full Mem
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1

0000000000000083 62d38545cefd0a                  VGF2P8AFFINEQB zmm7{k5}, zmm31, zmm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000008A 62d38545cffd0a                  VGF2P8AFFINEINVQB zmm7{k5}, zmm31, zmm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

0000000000000091 62d205c5cffd                    VGF2P8MULB zmm7{k5}{z}, zmm31, zmm13
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full Mem
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1

0000000000000097 62d385c5cefd0a                  VGF2P8AFFINEQB zmm7{k5}{z}, zmm31, zmm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

000000000000009E 62d385c5cffd0a                  VGF2P8AFFINEINVQB zmm7{k5}{z}, zmm31, zmm13, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: M, RegType:           Vector, RegSize: 64, RegId: 13, RegCount: 1
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000000A5 62f20540cf3b                    VGF2P8MULB zmm7, zmm31, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full Mem
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000AB 62f38540ce3b0a                  VGF2P8AFFINEQB zmm7, zmm31, zmmword ptr [rbx], 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000000B2 62f38540cf3b0a                  VGF2P8AFFINEINVQB zmm7, zmm31, zmmword ptr [rbx], 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000000B9 62f20540cf3b                    VGF2P8MULB zmm7, zmm31, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full Mem
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000BF 62f38550ce3b0a                  VGF2P8AFFINEQB zmm7, zmm31, qword ptr [rbx]{1to8}, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000000C6 62f38550cf3b0a                  VGF2P8AFFINEINVQB zmm7, zmm31, qword ptr [rbx]{1to8}, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 0, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000000CD 62f20545cf3b                    VGF2P8MULB zmm7{k5}, zmm31, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full Mem
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000D3 62f38555ce3b0a                  VGF2P8AFFINEQB zmm7{k5}, zmm31, qword ptr [rbx]{1to8}, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000000DA 62f38555cf3b0a                  VGF2P8AFFINEINVQB zmm7{k5}, zmm31, qword ptr [rbx]{1to8}, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000000E1 62f205c5cf3b                    VGF2P8MULB zmm7{k5}{z}, zmm31, zmmword ptr [rbx]
        DSIZE: 32, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full Mem
        Exception class: EVEX, exception type: E4
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size: 64, RawSize: 64, Encoding: M, 
                Segment: 3, Base: 3, 

00000000000000E7 62f385d5ce3b0a                  VGF2P8AFFINEQB zmm7{k5}{z}, zmm31, qword ptr [rbx]{1to8}, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

00000000000000EE 62f385d5cf3b0a                  VGF2P8AFFINEINVQB zmm7{k5}{z}, zmm31, qword ptr [rbx]{1to8}, 0x0a
        DSIZE: 64, ASIZE: 64, VLEN: 512
        ISA Set: GFNI, Ins cat: GFNI, CET tracked: no
        CPUID leaf: 0x00000007, sub-leaf: 0x00000000, reg: ecx, bit: 8
        EVEX Tuple Type: Full
        Exception class: EVEX, exception type: E4NF
        Valid modes
                R0: yes, R1: yes, R2: yes, R3: yes
                Real: no, V8086: no, Prot: yes, Compat: yes, Long: yes
                SMM: yes, SGX: yes, TSX: yes, VMXRoot: yes, VMXNonRoot: yes
        Valid prefixes
                REP: no, REPcc: no, LOCK: no
                HLE: no, XACQUIRE only: no, XRELEASE only: no
                BND: no, BHINT: no, DNT: no
        Operand: 0, Acc:  -W,  Type:   Register, Size: 64, RawSize: 64, Encoding: R, RegType:           Vector, RegSize: 64, RegId: 7, RegCount: 1
                Decorator: Mask k5
                Decorator: Zero (no merging)
        Operand: 1, Acc:  R-,  Type:   Register, Size:  8, RawSize:  8, Encoding: A, RegType:             Mask, RegSize:  8, RegId: 5, RegCount: 1
        Operand: 2, Acc:  R-,  Type:   Register, Size: 64, RawSize: 64, Encoding: V, RegType:           Vector, RegSize: 64, RegId: 31, RegCount: 1
        Operand: 3, Acc:  R-,  Type:     Memory, Size:  8, RawSize:  8, Encoding: M, Broadcast: yes, 
                Segment: 3, Base: 3, 
                Decorator: Broadcast 8 bytes element 8 times
        Operand: 4, Acc:  R-,  Type:  Immediate, Size:  1, RawSize:  1, Encoding: I

