{
    "name": "FRR",
    "category": "router",
    "description": "FRRouting (FRR) is an IP routing protocol suite for Linux and Unix platforms which includes protocol daemons for BGP, IS-IS, LDP, OSPF, PIM, and RIP.\n\nFRR's seamless integration with the native Linux/Unix IP networking stacks makes it applicable to a wide variety of use cases including connecting hosts/VMs/containers to the network, advertising network services, LAN switching and routing, Internet access routers, and Internet peering.\n\nThis is an unofficial VM of FRR.",
    "vendor_name": "FRRouting Project",
    "vendor_url": "https://frrouting.org",
    "product_name": "FRR",
    "registry_version": 3,
    "status": "stable",
    "maintainer": "GNS3 Team",
    "maintainer_email": "developers@gns3.net",
    "usage": "Credentials: root / root\nIf you exit from the router CLI, you can get back by typing 'vtysh' to the console.",
    "port_name_format": "eth{0}",
    "qemu": {
        "adapter_type": "e1000",
        "adapters": 8,
        "ram": 256,
        "hda_disk_interface": "ide",
        "arch": "x86_64",
        "console_type": "telnet",
        "kvm": "allow"
    },
    "images": [
        {
            "filename": "frr-7.3.1.qcow2",
            "version": "7.3.1",
            "md5sum": "e6bd9591a5c630bfe2c8688dc043b20b",
            "filesize": 47348224,
            "download_url": "https://sourceforge.net/projects/gns-3/files/Qemu%20Appliances/",
            "direct_download_url": "http://downloads.sourceforge.net/project/gns-3/Qemu%20Appliances/frr-7.3.1.qcow2"
        }
    ],
    "versions": [
        {
            "name": "7.3.1",
            "images": {
                "hda_disk_image": "frr-7.3.1.qcow2"
            }
        }
    ]
}
